-- extracted from rfc4807.txt
-- at Tue Mar 13 06:22:42 2007

IPSEC-SPD-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, Integer32,
    Unsigned32, mib-2            FROM SNMPv2-SMI
                                        -- [RFC2578]

    TEXTUAL-CONVENTION, RowStatus, TruthValue,
    TimeStamp, StorageType, VariablePointer
                                        FROM SNMPv2-TC
                                        -- [RFC2579]

    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                                        FROM SNMPv2-CONF
                                        -- [RFC2580]

    InterfaceIndex
                                        FROM IF-MIB
                                        -- [RFC2863]

    diffServMIBMultiFieldClfrGroup, IfDirection,
    diffServMultiFieldClfrNextFree
                                        FROM DIFFSERV-MIB
                                        -- [RFC3289]

    InetAddressType, InetAddress
                                        FROM INET-ADDRESS-MIB
                                        -- [RFC4001]

    SnmpAdminString                     FROM SNMP-FRAMEWORK-MIB
                                        -- [RFC3411]

    ;

--
-- module identity
--

spdMIB MODULE-IDENTITY
    LAST-UPDATED "200702070000Z"    -- 7 February 2007
    ORGANIZATION "IETF IP Security Policy Working Group"
    CONTACT-INFO "Michael Baer
                  P.O. Box 72682
                  Davis, CA 95617
                  Phone: +1 530 902 3131
                  Email: baerm@tislabs.com

                  Ricky Charlet
                  Email: rcharlet@alumni.calpoly.edu

                  Wes Hardaker
                  Sparta, Inc.
                  P.O. Box 382
                  Davis, CA  95617
                  Phone: +1 530 792 1913
                  Email: hardaker@tislabs.com

                  Robert Story
                  Revelstone Software
                  PO Box 1812
                  Tucker, GA 30085
                  Phone: +1 770 617 3722
                  Email: rstory@ipsp.revelstone.com

                  Cliff Wang
                  ARO
                  4300 S. Miami Blvd.
                  Durham, NC 27703
                  E-Mail: cliffwangmail@yahoo.com"
    DESCRIPTION
     "This MIB module defines configuration objects for managing
      IPsec Security Policies.  In general, this MIB can be
      implemented anywhere IPsec security services exist (e.g.,
      bump-in-the-wire, host, gateway, firewall, router, etc.).

      Copyright (C) The IETF Trust (2007).  This version of
      this MIB module is part of RFC 4807; see the RFC itself for
      full legal notices."

-- Revision History

    REVISION     "200702070000Z"    -- 7 February 2007
    DESCRIPTION  "Initial version, published as RFC 4807."

    ::= { mib-2 153 }

--
-- groups of related objects
--

spdConfigObjects         OBJECT IDENTIFIER
     ::= { spdMIB 1 }
spdNotificationObjects   OBJECT IDENTIFIER
     ::= { spdMIB 2 }
spdConformanceObjects    OBJECT IDENTIFIER
     ::= { spdMIB 3 }
spdActions               OBJECT IDENTIFIER
     ::= { spdMIB 4 }

--
-- Textual Conventions
--

SpdBooleanOperator ::= TEXTUAL-CONVENTION
    STATUS   current
    DESCRIPTION
        "The SpdBooleanOperator operator is used to specify
         whether sub-components in a decision-making process are
         ANDed or ORed together to decide if the resulting
         expression is true or false."
    SYNTAX      INTEGER { or(1), and(2) }

SpdAdminStatus ::= TEXTUAL-CONVENTION
    STATUS   current
    DESCRIPTION
        "The SpdAdminStatus is used to specify the administrative
         status of an object.  Objects that are disabled MUST NOT
         be used by the packet processing engine."
    SYNTAX      INTEGER { enabled(1), disabled(2) }

SpdIPPacketLogging ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "d"
    STATUS   current
    DESCRIPTION
        "SpdIPPacketLogging specifies whether an audit message
         SHOULD be logged if a packet is passed through a Security
         Association (SA) and if some of that packet is included in
         the log event.  A value of '-1' indicates no logging.  A
         value of '0' or greater indicates that logging SHOULD be
         done and indicates the number of bytes starting at the
         beginning of the packet to place in the log.  Values greater
         than the size of the packet being processed indicate that
         the entire packet SHOULD be sent.

         Examples:
         '-1' no logging
         '0'  log but do not include any of the packet in the log
         '20' log and include the first 20 bytes of the packet
              in the log."

    SYNTAX      Integer32 (-1..65535)


SpdTimePeriod ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "31t"
    STATUS       current
    DESCRIPTION
        "This property identifies an overall range of calendar dates
         and time.  In a boolean context, a value within this time
         range, inclusive, is considered true.

         This information is encoded as an octet string using
         the UTF-8 transformation format described in STD 63,
         RFC 3629.

         It uses the format suggested in RFC 3060.  An octet string
         represents a start date and time and an end date and time.
         For example:

         yyyymmddThhmmss/yyyymmddThhmmss

         Where: yyyy = year     mm = month     dd = day
                  hh = hour     mm = minute    ss = second

         The first 'yyyymmddThhmmss' sub-string indicates the start
         date and time.  The second 'yyyymmddThhmmss' sub-string
         indicates the end date and time.  The character 'T' within
         these sub-strings indicates the beginning of the time
         portion of each sub-string.  The solidus character '/'
         separates the start from the end date and time.  The end
         date and time MUST be subsequent to the start date and
         time.

         There are also two allowed substitutes for a
         'yyyymmddThhmmss' sub-string: one for the start date and
         time, and one for the end date and time.

         If the start date and time are replaced with the string
         'THISANDPRIOR', this sub-string would indicate the current
         date and time and the previous dates and time.

         If the end date and time are replaced with the string
         'THISANDFUTURE', this sub-string would indicate the current
         date and time and the subsequent dates and time.

         Any of the following SHOULD be considered a
         'wrongValue' error:
         - Setting a value with the end date and time earlier than
           or equal to the start date and time.
         - Setting the start date and time to 'THISANDFUTURE'.
         - Setting the end date and time to 'THISANDPRIOR'."
    REFERENCE "RFC 3060, 3269"
    SYNTAX      OCTET STRING (SIZE (0..31))
--
-- Policy group definitions
--

spdLocalConfigObjects OBJECT IDENTIFIER
     ::= { spdConfigObjects 1 }

spdIngressPolicyGroupName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object indicates the global system policy group that
        is to be applied on ingress packets (i.e., arriving at an
        interface from a network) when a given endpoint does not
        contain a policy definition in the spdEndpointToGroupTable.
        Its value can be used as an index into the
        spdGroupContentsTable to retrieve a list of policies.  A
        zero length string indicates that no system-wide policy exists
        and the default policy of 'drop' SHOULD be executed for
        ingress packets until one is imposed by either this object
        or by the endpoint processing a given packet.

        This object MUST be persistent"
    DEFVAL { "" }
    ::= { spdLocalConfigObjects 1 }

spdEgressPolicyGroupName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This object indicates the policy group containing the
         global system policy that is to be applied on egress
         packets (i.e., packets leaving an interface and entering a
         network) when a given endpoint does not contain a policy
         definition in the spdEndpointToGroupTable.  Its value can
         be used as an index into the spdGroupContentsTable to
         retrieve a list of policies.  A zero length string
         indicates that no system-wide policy exists and the default
         policy of 'drop' SHOULD be executed for egress packets
         until one is imposed by either this object or by the
         endpoint processing a given packet.

         This object MUST be persistent"
    DEFVAL { "" }
    ::= { spdLocalConfigObjects 2 }


spdEndpointToGroupTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdEndpointToGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table maps policies (groupings) onto an endpoint
         (interface).  A policy group assigned to an endpoint is then
         used to control access to the network traffic passing
         through that endpoint.
         If an endpoint has been configured with a policy group and
         no rule within that policy group matches that packet, the
         default action in this case SHALL be to drop the packet.

         If no policy group has been assigned to an endpoint, then
         the policy group specified by spdIngressPolicyGroupName MUST
         be used on traffic inbound from the network through that
         endpoint, and the policy group specified by
         spdEgressPolicyGroupName MUST be used for traffic outbound
         to the network through that endpoint."
    ::= { spdConfigObjects 2 }

spdEndpointToGroupEntry OBJECT-TYPE
    SYNTAX      SpdEndpointToGroupEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A mapping assigning a policy group to an endpoint."

    INDEX { spdEndGroupDirection, spdEndGroupInterface }
    ::= { spdEndpointToGroupTable 1 }

SpdEndpointToGroupEntry ::= SEQUENCE {
    spdEndGroupDirection                      IfDirection,
    spdEndGroupInterface                      InterfaceIndex,
    spdEndGroupName                           SnmpAdminString,
    spdEndGroupLastChanged                    TimeStamp,
    spdEndGroupStorageType                    StorageType,
    spdEndGroupRowStatus                      RowStatus
}

spdEndGroupDirection OBJECT-TYPE
    SYNTAX      IfDirection
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object indicates which direction of packets crossing
         the interface are associated with which spdEndGroupName
         object.  Ingress packets, or packets into the device match
         when this value is inbound(1).  Egress packets or packets
         out of the device match when this value is outbound(2)."
    ::= { spdEndpointToGroupEntry 1 }

spdEndGroupInterface OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This value matches the IF-MIB's ifTable's ifIndex column
         and indicates the interface associated with a given
         endpoint.  This object can be used to uniquely identify an
         endpoint that a set of policy groups are applied to."
    ::= { spdEndpointToGroupEntry 2 }

spdEndGroupName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The policy group name to apply at this endpoint.  The
         value of the spdEndGroupName object is then used as an
         index into the spdGroupContentsTable to come up with a list
         of rules that MUST be applied at this endpoint."
    ::= { spdEndpointToGroupEntry 3 }

spdEndGroupLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdEndpointToGroupEntry 4 }

spdEndGroupStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdEndpointToGroupEntry 5 }

spdEndGroupRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         This object is considered 'notReady' and MUST NOT be set to
         active until one or more active rows exist within the
         spdGroupContentsTable for the group referenced by the
         spdEndGroupName object."
    ::= { spdEndpointToGroupEntry 6 }

--
-- policy group definition table
--

spdGroupContentsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdGroupContentsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of rules and/or subgroups
         contained within a given policy group.  For a given value
         of spdGroupContName, the set of rows sharing that value
         forms a 'group'.  The rows in a group MUST be processed
         according to the value of the spdGroupContPriority object
         in each row.  The processing MUST be executed starting with
         the lowest value of spdGroupContPriority and in ascending
         order thereafter.

         If an action is executed as the result of the processing of
         a row in a group, the processing of further rows in that
         group MUST stop.  Iterating to the next policy group row by
         finding the next largest spdGroupContPriority object SHALL
         only be done if no actions were run while processing the
         current row for a given packet."
    ::= { spdConfigObjects 3 }

spdGroupContentsEntry OBJECT-TYPE
    SYNTAX      SpdGroupContentsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines a given sub-component within a policy group.  A
         sub-component is either a rule or another group as
         indicated by spdGroupContComponentType and referenced by
         spdGroupContComponentName."

    INDEX   { spdGroupContName, spdGroupContPriority }
    ::= { spdGroupContentsTable 1 }

SpdGroupContentsEntry ::= SEQUENCE {
    spdGroupContName                        SnmpAdminString,
    spdGroupContPriority                    Integer32,
    spdGroupContFilter                      VariablePointer,
    spdGroupContComponentType               INTEGER,
    spdGroupContComponentName               SnmpAdminString,
    spdGroupContLastChanged                 TimeStamp,
    spdGroupContStorageType                 StorageType,
    spdGroupContRowStatus                   RowStatus
}

spdGroupContName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The administrative name of the group associated with this
        row.  A 'group' is formed by all the rows in this table that
        have the same value of this object."
    ::= { spdGroupContentsEntry 1 }

spdGroupContPriority OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The priority (sequence number) of the sub-component in
         a group that this row represents.  This value indicates
         the order that each row of this table MUST be processed
         from low to high.  For example, a row with a priority of 0
         is processed before a row with a priority of 1, a 1 before
         a 2, etc."
    ::= { spdGroupContentsEntry 2 }

spdGroupContFilter OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "spdGroupContFilter points to a filter that is evaluated
         to determine whether the spdGroupContComponentName within
         this row is exercised.  Managers can use this object to
         classify groups of rules, or subgroups, together in order to
         achieve a greater degree of control and optimization over
         the execution order of the items within the group.  If the
         filter evaluates to false, the rule or subgroup will be
         skipped and the next rule or subgroup will be evaluated
         instead.  This value can be used to indicate a scalar or
         row in a table.  When indicating a row in a table, this
         value MUST point to the first column instance in that row.

         An example usage of this object would be to limit a
         group of rules to executing only when the IP packet
         being processed is designated to be processed by IKE.
         This effectively creates a group of IKE-specific rules.

         The following tables and scalars can be pointed to by this
         column.  All but diffServMultiFieldClfrTable are defined in
         this MIB:

                diffServMultiFieldClfrTable
                spdIpOffsetFilterTable
                spdTimeFilterTable
                spdCompoundFilterTable
                spdTrueFilter
                spdIpsoHeaderFilterTable

         Implementations MAY choose to provide support for other
         filter tables or scalars.

         If this column is set to a VariablePointer value, which
         references a non-existent row in an otherwise supported
         table, the inconsistentName exception MUST be returned.  If
         the table or scalar pointed to by the VariablePointer is
         not supported at all, then an inconsistentValue exception
         MUST be returned.

         If, during packet processing, a row in this table is applied
         to a packet and the value of this column in that row
         references a non-existent or non-supported object, the
         packet MUST be dropped."
    REFERENCE "RFC 3289"
    DEFVAL { spdTrueFilterInstance }
    ::= { spdGroupContentsEntry 3 }

spdGroupContComponentType OBJECT-TYPE
    SYNTAX      INTEGER { group(1), rule(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether the spdGroupContComponentName object
         is the name of another group defined within the
         spdGroupContentsTable or is the name of a rule defined
         within the spdRuleDefinitionTable."
    DEFVAL { rule }
    ::= { spdGroupContentsEntry 4 }

spdGroupContComponentName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the policy rule or subgroup contained within
         this row, as indicated by the spdGroupContComponentType
         object."
    ::= { spdGroupContentsEntry 5 }

spdGroupContLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem,
         this object SHOULD have a zero value."
    ::= { spdGroupContentsEntry 6 }

spdGroupContStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdGroupContentsEntry 7 }

spdGroupContRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.
         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         This object MUST NOT be set to active until the row to
         which the spdGroupContComponentName points to exists and is
         active.

         If active, this object MUST remain active unless one of the
         following two conditions are met:

         I.  No active row in spdEndpointToGroupTable exists that
             references this row's group (i.e., indicate this row's
             spdGroupContName).

         II. Or at least one other active row in this table has a
             matching spdGroupContName.

         If neither condition is met, an attempt to set this row to
         something other than active MUST result in an
         inconsistentValue error."
    ::= { spdGroupContentsEntry 8 }


--
-- policy definition table
--

spdRuleDefinitionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdRuleDefinitionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table defines a rule by associating a filter
         or a set of filters to an action to be executed."
    ::= { spdConfigObjects 4 }

spdRuleDefinitionEntry OBJECT-TYPE
    SYNTAX      SpdRuleDefinitionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row defining a particular rule definition.  A rule
         definition binds a filter pointer to an action pointer."
    INDEX   { spdRuleDefName }
    ::= { spdRuleDefinitionTable 1 }

SpdRuleDefinitionEntry ::= SEQUENCE {
    spdRuleDefName                          SnmpAdminString,
    spdRuleDefDescription                   SnmpAdminString,
    spdRuleDefFilter                        VariablePointer,
    spdRuleDefFilterNegated                 TruthValue,
    spdRuleDefAction                        VariablePointer,
    spdRuleDefAdminStatus                   SpdAdminStatus,
    spdRuleDefLastChanged                   TimeStamp,
    spdRuleDefStorageType                   StorageType,
    spdRuleDefRowStatus                     RowStatus
}

spdRuleDefName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "spdRuleDefName is the administratively assigned name of
         the rule referred to by the spdGroupContComponentName
         object."
    ::= { spdRuleDefinitionEntry 1 }

spdRuleDefDescription OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A user defined string.  This field MAY be used for
         administrative tracking purposes."
    DEFVAL { "" }
    ::= { spdRuleDefinitionEntry 2 }

spdRuleDefFilter OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "spdRuleDefFilter points to a filter that is used to
         evaluate whether the action associated with this row is
         executed or not.  The action will only execute if the
         filter referenced by this object evaluates to TRUE after
         first applying any negation required by the
         spdRuleDefFilterNegated object.

         The following tables and scalars can be pointed to by this
         column.  All but diffServMultiFieldClfrTable are defined in
         this MIB.  Implementations MAY choose to provide support
         for other filter tables or scalars as well:

                diffServMultiFieldClfrTable
                spdIpOffsetFilterTable
                spdTimeFilterTable
                spdCompoundFilterTable
                spdTrueFilter

         If this column is set to a VariablePointer value, which
         references a non-existent row in an otherwise supported
         table, the inconsistentName exception MUST be returned.  If
         the table or scalar pointed to by the VariablePointer is
         not supported at all, then an inconsistentValue exception
         MUST be returned.

         If, during packet processing, this column has a value that
         references a non-existent or non-supported object, the
         packet MUST be dropped."
    REFERENCE "RFC 3289"
    ::= { spdRuleDefinitionEntry 3 }

spdRuleDefFilterNegated OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "spdRuleDefFilterNegated specifies whether or not the results of
         the filter referenced by the spdRuleDefFilter object is
         negated."
    DEFVAL { false }
    ::= { spdRuleDefinitionEntry 4 }

spdRuleDefAction OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This column points to the action to be taken.  It MAY,
         but is not limited to, point to a row in one of the
         following tables:

            spdCompoundActionTable
            ipsaSaPreconfiguredActionTable
            ipiaIkeActionTable
            ipiaIpsecActionTable

         It MAY also point to one of the scalar objects beneath
         spdStaticActions.

         If this object is set to a pointer to a row in an
         unsupported (or unknown) table, an inconsistentValue
         error MUST be returned.

         If this object is set to point to a non-existent row in an
         otherwise supported table, an inconsistentName error MUST
         be returned.

         If, during packet processing, this column has a value that
         references a non-existent or non-supported object, the
         packet MUST be dropped."
    ::= { spdRuleDefinitionEntry 5 }

spdRuleDefAdminStatus OBJECT-TYPE
    SYNTAX      SpdAdminStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether the current rule definition is considered
         active.  If the value is enabled, the rule MUST be evaluated
         when processing packets.  If the value is disabled, the
         packet processing MUST continue as if this rule's filter
         had effectively failed."
    DEFVAL { enabled }
    ::= { spdRuleDefinitionEntry 6 }

spdRuleDefLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdRuleDefinitionEntry 7 }

spdRuleDefStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a
         storage type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdRuleDefinitionEntry 8 }

spdRuleDefRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         This object MUST NOT be set to active until the containing
         conditions, filters, and actions have been defined.  Once
         active, it MUST remain active until no active
         policyGroupContents entries are referencing it.  A failed
         attempt to do so MUST return an inconsistentValue error."
    ::= { spdRuleDefinitionEntry 9 }

--
-- Policy compound filter definition table
--

spdCompoundFilterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdCompoundFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table defining compound filters and their associated
         parameters.  A row in this table can be pointed to by a
         spdRuleDefFilter object."
    ::= { spdConfigObjects 5 }

spdCompoundFilterEntry OBJECT-TYPE
    SYNTAX      SpdCompoundFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the spdCompoundFilterTable.  Each entry in this
         table represents a compound filter.  A filter defined by
         this table is considered to have a TRUE return value if and
         only if:

         spdCompFiltLogicType is AND and all of the sub-filters
         associated with it, as defined in the spdSubfiltersTable,
         are all true themselves (after applying any required
         negation, as defined by the ficFilterIsNegated object).

         spdCompFiltLogicType is OR and at least one of the
         sub-filters associated with it, as defined in the
         spdSubfiltersTable, is true itself (after applying any
         required negation, as defined by the ficFilterIsNegated
         object."
    INDEX       { spdCompFiltName }
    ::= { spdCompoundFilterTable 1 }

SpdCompoundFilterEntry ::= SEQUENCE {
    spdCompFiltName                          SnmpAdminString,
    spdCompFiltDescription                   SnmpAdminString,
    spdCompFiltLogicType                     SpdBooleanOperator,
    spdCompFiltLastChanged                   TimeStamp,
    spdCompFiltStorageType                   StorageType,
    spdCompFiltRowStatus                     RowStatus
}

spdCompFiltName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A user definable string.  This value is used as an index
         into this table."
    ::= { spdCompoundFilterEntry 1 }

spdCompFiltDescription OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A user definable string.  This field MAY be used for
         your administrative tracking purposes."
    DEFVAL { "" }
    ::= { spdCompoundFilterEntry 2 }

spdCompFiltLogicType OBJECT-TYPE
    SYNTAX      SpdBooleanOperator
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether the sub-component filters of this
         compound filter are functionally ANDed or ORed together."
    DEFVAL { and }
    ::= { spdCompoundFilterEntry 3 }

spdCompFiltLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdCompoundFilterEntry 4 }

spdCompFiltStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a
         storage type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdCompoundFilterEntry 5 }

spdCompFiltRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         Once active, it MUST NOT have its value changed if any
         active rows in the spdRuleDefinitionTable are currently
         pointing at this row."
    ::= { spdCompoundFilterEntry 6 }

--
-- Policy filters in a cf table
--

spdSubfiltersTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdSubfiltersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table defines a list of filters contained within a
         given compound filter defined in the
         spdCompoundFilterTable."
    ::= { spdConfigObjects 6 }

spdSubfiltersEntry OBJECT-TYPE
    SYNTAX      SpdSubfiltersEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the spdSubfiltersTable.  There is an entry in
         this table for each sub-filter of all compound filters
         present in the spdCompoundFilterTable."
    INDEX       {  spdCompFiltName, spdSubFiltPriority }
    ::= { spdSubfiltersTable 1 }

SpdSubfiltersEntry ::= SEQUENCE {
    spdSubFiltPriority                      Integer32,
    spdSubFiltSubfilter                     VariablePointer,
    spdSubFiltSubfilterIsNegated            TruthValue,
    spdSubFiltLastChanged                   TimeStamp,
    spdSubFiltStorageType                   StorageType,
    spdSubFiltRowStatus                     RowStatus
}

spdSubFiltPriority OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The priority of a given filter within a compound filter.
         The order of execution is from lowest to highest priority
         value (i.e., priority 0 before priority 1, 1 before 2,
         etc.).  Implementations MAY choose to follow this ordering,
         as set by the manager that created the rows.  This can allow
         a manager to intelligently construct filter lists such that
         faster filters are evaluated first."
    ::= { spdSubfiltersEntry 1 }

spdSubFiltSubfilter OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The OID of the contained filter.  The value of this
         object is a VariablePointer that references the filter to
         be included in this compound filter.

         The following tables and scalars can be pointed to by this
         column.  All but diffServMultiFieldClfrTable are defined in
         this MIB.  Implementations MAY choose to provide support
         for other filter tables or scalars as well:

                diffServMultiFieldClfrTable
                spdIpsoHeaderFilterTable
                spdIpOffsetFilterTable
                spdTimeFilterTable
                spdCompoundFilterTable
                spdTrueFilter

         If this column is set to a VariablePointer value that
         references a non-existent row in an otherwise supported
         table, the inconsistentName exception MUST be returned.  If
         the table or scalar pointed to by the VariablePointer is
         not supported at all, then an inconsistentValue exception
         MUST be returned.

         If, during packet processing, this column has a value that
         references a non-existent or non-supported object, the
         packet MUST be dropped."
    REFERENCE "RFC 3289"
    ::= { spdSubfiltersEntry 2 }

spdSubFiltSubfilterIsNegated OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether or not the result of applying this sub-filter
         is negated."
    DEFVAL { false }
    ::= { spdSubfiltersEntry 3 }

spdSubFiltLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.
         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdSubfiltersEntry 4 }

spdSubFiltStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a
         storage type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdSubfiltersEntry 5 }

spdSubFiltRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         This object cannot be made active until a filter
         referenced by the spdSubFiltSubfilter object is both
         defined and active.  An attempt to do so MUST result in
         an inconsistentValue error.

         If active, this object MUST remain active unless one of the
         following two conditions are met:

         I.  No active row in the SpdCompoundFilterTable exists
             that has a matching spdCompFiltName.

         II. Or, at least one other active row in this table has a
             matching spdCompFiltName.

         If neither condition is met, an attempt to set this row to
         something other than active MUST result in an
         inconsistentValue error."
    ::= { spdSubfiltersEntry 6 }

--
-- Static Filters
--

spdStaticFilters OBJECT IDENTIFIER ::= { spdConfigObjects 7 }

spdTrueFilter OBJECT-TYPE
        SYNTAX      Integer32 (1)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
            "This scalar indicates a (automatic) true result for
             a filter.  That is, this is a filter that is always
             true; it is useful for adding as a default filter for a
             default action or a set of actions."
        ::= { spdStaticFilters 1 }


spdTrueFilterInstance OBJECT IDENTIFIER ::= { spdTrueFilter 0 }


--
-- Policy IP Offset filter definition table
--

spdIpOffsetFilterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdIpOffsetFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of filter definitions to be
         used within the spdRuleDefinitionTable or the
         spdSubfiltersTable.

         This type of filter is used to compare an administrator
         specified octet string to the octets at a particular
         location in a packet."
    ::= { spdConfigObjects 8 }

spdIpOffsetFilterEntry OBJECT-TYPE
    SYNTAX      SpdIpOffsetFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A definition of a particular filter."
    INDEX       {  spdIpOffFiltName }
    ::= { spdIpOffsetFilterTable 1 }

SpdIpOffsetFilterEntry ::= SEQUENCE {
    spdIpOffFiltName                         SnmpAdminString,
    spdIpOffFiltOffset                       Unsigned32,
    spdIpOffFiltType                         INTEGER,
    spdIpOffFiltValue                        OCTET STRING,
    spdIpOffFiltLastChanged                  TimeStamp,
    spdIpOffFiltStorageType                  StorageType,
    spdIpOffFiltRowStatus                    RowStatus
}

spdIpOffFiltName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The administrative name for this filter."
    ::= { spdIpOffsetFilterEntry 1 }

spdIpOffFiltOffset OBJECT-TYPE
    SYNTAX      Unsigned32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the byte offset from the front of the entire IP
         packet where the value or arithmetic comparison is done.  A
         value of '0' indicates the first byte of the packet header.
         If this value is greater than the length of the packet, the
         filter represented by this row should be considered to
         fail."
    ::= { spdIpOffsetFilterEntry 2 }

spdIpOffFiltType OBJECT-TYPE
    SYNTAX INTEGER { equal(1),
                     notEqual(2),
                     arithmeticLess(3),
                     arithmeticGreaterOrEqual(4),
                     arithmeticGreater(5),
                     arithmeticLessOrEqual(6) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This defines the various tests that are used when
         evaluating a given filter.

         The various tests definable in this table are as follows:

         equal:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', matches
             a value in the packet starting at the given offset in
             the packet and comparing the entire OCTET STRING of
             'spdIpOffFiltValue'.  Any values compared this way are
             assumed to be unsigned integer values in network byte
             order of the same length as 'spdIpOffFiltValue'.

         notEqual:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', does
             not match a value in the packet starting at the given
             offset in the packet and comparing to the entire OCTET
             STRING of 'spdIpOffFiltValue'.  Any values compared
             this way are assumed to be unsigned integer values in
             network byte order of the same length as
             'spdIpOffFiltValue'.

         arithmeticLess:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', is
             arithmetically less than ('<') the value starting at
             the given offset within the packet.  The value in the
             packet is assumed to be an unsigned integer in network
             byte order of the same length as 'spdIpOffFiltValue'.

         arithmeticGreaterOrEqual:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', is
             arithmetically greater than or equal to ('>=') the
             value starting at the given offset within the packet.
             The value in the packet is assumed to be an unsigned
             integer in network byte order of the same length as
             'spdIpOffFiltValue'.

         arithmeticGreater:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', is
             arithmetically greater than ('>') the value starting at
             the given offset within the packet.  The value in the
             packet is assumed to be an unsigned integer in network
             byte order of the same length as 'spdIpOffFiltValue'.

         arithmeticLessOrEqual:
           - Tests if the OCTET STRING, 'spdIpOffFiltValue', is
             arithmetically less than or equal to ('<=') the value
             starting at the given offset within the packet.  The
             value in the packet is assumed to be an unsigned
             integer in network byte order of the same length as
             'spdIpOffFiltValue'."

    ::= { spdIpOffsetFilterEntry 3 }

spdIpOffFiltValue OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..1024))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "spdIpOffFiltValue is used for match comparisons of a
         packet at spdIpOffFiltOffset."
    ::= { spdIpOffsetFilterEntry 4 }

spdIpOffFiltLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdIpOffsetFilterEntry 5 }


spdIpOffFiltStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a
         storage type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdIpOffsetFilterEntry 6 }

spdIpOffFiltRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         If active, this object MUST remain active if it is
         referenced by an active row in another table.  An attempt
         to set it to anything other than active while it is
         referenced by an active row in another table MUST result in
         an inconsistentValue error."
    ::= { spdIpOffsetFilterEntry 7 }


--
-- Time/scheduling filter table
--

spdTimeFilterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdTimeFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Defines a table of filters that can be used to
         effectively enable or disable policies based on a valid
         time range."
    ::= { spdConfigObjects 9 }

spdTimeFilterEntry OBJECT-TYPE
    SYNTAX      SpdTimeFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row describing a given time frame for which a policy
         is filtered on to activate or deactivate the rule.

         If all the column objects in a row are true for the current
         time, the row evaluates as 'true'.  More explicitly, the
         time matching column objects in a row MUST be logically
         ANDed together to form the boolean true/false for the row."
    INDEX   { spdTimeFiltName }
    ::= { spdTimeFilterTable 1 }

SpdTimeFilterEntry ::= SEQUENCE {
    spdTimeFiltName                 SnmpAdminString,
    spdTimeFiltPeriod               SpdTimePeriod,
    spdTimeFiltMonthOfYearMask      BITS,
    spdTimeFiltDayOfMonthMask       OCTET STRING,
    spdTimeFiltDayOfWeekMask        BITS,
    spdTimeFiltTimeOfDayMask        SpdTimePeriod,
    spdTimeFiltLastChanged          TimeStamp,
    spdTimeFiltStorageType          StorageType,
    spdTimeFiltRowStatus            RowStatus
}
spdTimeFiltName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An administratively assigned name for this filter."
    ::= { spdTimeFilterEntry 1 }


spdTimeFiltPeriod OBJECT-TYPE
    SYNTAX      SpdTimePeriod
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The valid time period for this filter.  This column is
         considered 'true' if the current time is within the range of
         this object."
    DEFVAL { "THISANDPRIOR/THISANDFUTURE" }
    ::= { spdTimeFilterEntry 2 }


spdTimeFiltMonthOfYearMask OBJECT-TYPE
    SYNTAX      BITS { january(0), february(1), march(2),
                       april(3), may(4), june(5), july(6),
                       august(7), september(8), october(9),
                       november(10), december(11) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A bit mask that indicates acceptable months of the year.
         This column evaluates to 'true' if the current month's bit
         is set."
    DEFVAL { { january, february, march, april, may, june, july,
               august, september, october, november, december } }
    ::= { spdTimeFilterEntry 3 }

spdTimeFiltDayOfMonthMask OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(8))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Defines which days of the month the current time is
         valid for.  It is a sequence of 64 BITS, where each BIT
         represents a corresponding day of the month in forward or
         reverse order.  Starting from the left-most bit, the first
         31 bits identify the day of the month, counting from the
         beginning of the month.  The following 31 bits (bits 32-62)
         indicate the day of the month, counting from the end of the
         month.  For months with fewer than 31 days, the bits that
         correspond to the non-existent days of that month are
         ignored (e.g., for non-leap year Februarys, bits 29-31 and
         60-62 are ignored).

         This column evaluates to 'true' if the current day of the
         month's bit is set.

         For example, a value of 0X'80 00 00 01 00 00 00 00'
         indicates that this column evaluates to true on the first
         and last days of the month.

         The last two bits in the string MUST be zero."
    DEFVAL { 'fffffffffffffffe'H }
    ::= { spdTimeFilterEntry 4 }

spdTimeFiltDayOfWeekMask OBJECT-TYPE
    SYNTAX      BITS { sunday(0), monday(1), tuesday(2),
                       wednesday(3), thursday(4), friday(5),
                       saturday(6) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A bit mask that defines which days of the week that the current
         time is valid for.  This column evaluates to 'true' if the
         current day of the week's bit is set."
    DEFVAL { { monday, tuesday, wednesday, thursday, friday,
               saturday, sunday } }
    ::= { spdTimeFilterEntry 5 }

spdTimeFiltTimeOfDayMask OBJECT-TYPE
    SYNTAX      SpdTimePeriod
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the start and end time of the day for which this
         filter evaluates to true.  The date portions of the
         spdTimePeriod TC are ignored for purposes of evaluating this
         mask, and only the time-specific portions are used.

         This column evaluates to 'true' if the current time of day
         is within the range of the start and end times of the day
         indicated by this object."
    DEFVAL { "00000000T000000/00000000T240000" }
    ::= { spdTimeFilterEntry 6 }

spdTimeFiltLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdTimeFilterEntry 7 }

spdTimeFiltStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdTimeFilterEntry 8 }

spdTimeFiltRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this
         row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         If active, this object MUST remain active if it is
         referenced by an active row in another table.  An attempt
         to set it to anything other than active while it is
         referenced by an active row in another table MUST result in
         an inconsistentValue error."
    ::= { spdTimeFilterEntry 9 }

--
-- IPSO protection authority filtering
--
spdIpsoHeaderFilterTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdIpsoHeaderFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of IPSO header filter
         definitions to be used within the spdRuleDefinitionTable or
         the spdSubfiltersTable.  IPSO headers and their values are
         described in RFC 1108."
    REFERENCE "RFC 1108"
    ::= { spdConfigObjects 10 }

spdIpsoHeaderFilterEntry OBJECT-TYPE
    SYNTAX      SpdIpsoHeaderFilterEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A definition of a particular filter."
    INDEX       {  spdIpsoHeadFiltName }
    ::= { spdIpsoHeaderFilterTable 1 }

SpdIpsoHeaderFilterEntry ::= SEQUENCE {
    spdIpsoHeadFiltName                     SnmpAdminString,
    spdIpsoHeadFiltType                     BITS,
    spdIpsoHeadFiltClassification           INTEGER,
    spdIpsoHeadFiltProtectionAuth           INTEGER,
    spdIpsoHeadFiltLastChanged              TimeStamp,
    spdIpsoHeadFiltStorageType              StorageType,
    spdIpsoHeadFiltRowStatus                RowStatus
}

spdIpsoHeadFiltName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The administrative name for this filter."
    ::= { spdIpsoHeaderFilterEntry 1 }

spdIpsoHeadFiltType OBJECT-TYPE
    SYNTAX      BITS { classificationLevel(0),
                       protectionAuthority(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates which of the IPSO header field a
         packet is filtered on for this row.  If this object is set
         to classification(0), the spdIpsoHeadFiltClassification
         object indicates how the packet is filtered.  If this object
         is set to protectionAuthority(1), the
         spdIpsoHeadFiltProtectionAuth object indicates how the
         packet is filtered."
    ::= { spdIpsoHeaderFilterEntry 2 }

spdIpsoHeadFiltClassification OBJECT-TYPE
    SYNTAX      INTEGER { topSecret(61), secret(90),
                          confidential(150), unclassified(171) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the IPSO classification header field
         value that the packet MUST have for this row to evaluate to
         'true'.

         The values of these enumerations are defined by RFC 1108."
    REFERENCE "RFC 1108"
    ::= { spdIpsoHeaderFilterEntry 3 }

spdIpsoHeadFiltProtectionAuth OBJECT-TYPE
    SYNTAX      INTEGER { genser(0), siopesi(1), sci(2),
                          nsa(3), doe(4) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the IPSO protection authority header
         field value that the packet MUST have for this row to
         evaluate to 'true'.

         The values of these enumerations are defined by RFC 1108.
         Hence the reason the SMIv2 convention of not using 0 in
         enumerated lists is violated here."
    REFERENCE "RFC 1108"
    ::= { spdIpsoHeaderFilterEntry 4 }

spdIpsoHeadFiltLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdIpsoHeaderFilterEntry 5 }

spdIpsoHeadFiltStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdIpsoHeaderFilterEntry 6 }

spdIpsoHeadFiltRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         However, this object MUST NOT be set to active if the
         requirements of the spdIpsoHeadFiltType object are not met.
         Specifically, if the spdIpsoHeadFiltType bit for
         classification(0) is set, the spdIpsoHeadFiltClassification
         column MUST have a valid value for the row status to be set
         to active.  If the spdIpsoHeadFiltType bit for
         protectionAuthority(1) is set, the
         spdIpsoHeadFiltProtectionAuth column MUST have a valid
         value for the row status to be set to active.

         If active, this object MUST remain active if it is
         referenced by an active row in another table.  An attempt
         to set it to anything other than active while it is
         referenced by an active row in another table MUST result in
         an inconsistentValue error."
    ::= { spdIpsoHeaderFilterEntry 7 }

--
-- compound actions table
--

spdCompoundActionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdCompoundActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table used to allow multiple actions to be associated
         with a rule.  It uses the spdSubactionsTable to do this.
         The rows from spdSubactionsTable that are partially indexed
         by spdCompActName form the set of compound actions to be
         performed.  The spdCompActExecutionStrategy column in this
         table indicates how those actions are processed."
    ::= { spdConfigObjects 11 }

spdCompoundActionEntry OBJECT-TYPE
    SYNTAX      SpdCompoundActionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in the spdCompoundActionTable."
    INDEX   { spdCompActName }
    ::= { spdCompoundActionTable 1 }

SpdCompoundActionEntry ::= SEQUENCE {
    spdCompActName                      SnmpAdminString,
    spdCompActExecutionStrategy         INTEGER,
    spdCompActLastChanged               TimeStamp,
    spdCompActStorageType               StorageType,
    spdCompActRowStatus                 RowStatus
}

spdCompActName OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This is an administratively assigned name of this
         compound action."
    ::= { spdCompoundActionEntry 1 }

spdCompActExecutionStrategy OBJECT-TYPE
    SYNTAX      INTEGER { doAll(1),
                          doUntilSuccess(2),
                          doUntilFailure(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates how the sub-actions are executed
         based on the success of the actions as they finish
         executing.
         doAll           - run each sub-action regardless of the
                           exit status of the previous action.
                           This parent action is always
                           considered to have acted successfully.

         doUntilSuccess  - run each sub-action until one succeeds,
                           at which point stop processing the
                           sub-actions within this parent
                           compound action.  If one of the
                           sub-actions did execute successfully,
                           this parent action is also considered
                           to have executed successfully.

         doUntilFailure  - run each sub-action until one fails,
                           at which point stop processing the
                           sub-actions within this compound
                           action.  If any sub-action fails, the
                           result of this parent action is
                           considered to have failed."
    DEFVAL { doUntilSuccess }
    ::= { spdCompoundActionEntry 2 }

spdCompActLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdCompoundActionEntry 3 }

spdCompActStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdCompoundActionEntry 4 }

spdCompActRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         Once a row in the spdCompoundActionTable has been made
         active, this object MUST NOT be set to destroy without
         first destroying all the contained rows listed in the
         spdSubactionsTable."
    ::= { spdCompoundActionEntry 5 }


--
-- actions contained within a compound action
--

spdSubactionsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SpdSubactionsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains a list of the sub-actions within a
         given compound action.  Compound actions executing these
         actions MUST execute them in series based on the
         spdSubActPriority value, with the lowest value executing
         first."
    ::= { spdConfigObjects 12 }

spdSubactionsEntry OBJECT-TYPE
    SYNTAX      SpdSubactionsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row containing a reference to a given compound-action
         sub-action."
    INDEX   { spdCompActName, spdSubActPriority }
    ::= { spdSubactionsTable 1 }

SpdSubactionsEntry ::= SEQUENCE {
    spdSubActPriority                          Integer32,
    spdSubActSubActionName                     VariablePointer,
    spdSubActLastChanged                       TimeStamp,
    spdSubActStorageType                       StorageType,
    spdSubActRowStatus                         RowStatus
}

spdSubActPriority OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The priority of a given sub-action within a compound
         action.  The order in which sub-actions MUST be executed
         are based on the value from this column, with the lowest
         numeric value executing first (i.e., priority 0 before
         priority 1, 1 before 2, etc.)."
    ::= { spdSubactionsEntry 1 }

spdSubActSubActionName OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This column points to the action to be taken.  It MAY,
         but is not limited to, point to a row in one of the
         following tables:

            spdCompoundActionTable         - Allowing recursion
            ipsaSaPreconfiguredActionTable
            ipiaIkeActionTable
            ipiaIpsecActionTable

         It MAY also point to one of the scalar objects beneath
         spdStaticActions.

         If this object is set to a pointer to a row in an
         unsupported (or unknown) table, an inconsistentValue
         error MUST be returned.

         If this object is set to point to a non-existent row in
         an otherwise supported table, an inconsistentName error
         MUST be returned.

         If, during packet processing, this column has a value that
         references a non-existent or non-supported object, the
         packet MUST be dropped."
    ::= { spdSubactionsEntry 2 }

spdSubActLastChanged OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this row was last modified
         or created either through SNMP SETs or by some other
         external means.

         If this row has not been modified since the last
         re-initialization of the network management subsystem, this
         object SHOULD have a zero value."
    ::= { spdSubactionsEntry 3 }

spdSubActStorageType OBJECT-TYPE
    SYNTAX      StorageType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The storage type for this row.  Rows in this table that
         were created through an external process MAY have a storage
         type of readOnly or permanent.

         For a storage type of permanent, none of the columns have
         to be writable."
    DEFVAL { nonVolatile }
    ::= { spdSubactionsEntry 4 }

spdSubActRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the conceptual status of this row.

         The value of this object has no effect on whether other
         objects in this conceptual row can be modified.

         If active, this object MUST remain active unless one of the
         following two conditions are met.  An attempt to set it to
         anything other than active while the following conditions
         are not met MUST result in an inconsistentValue error.  The
         two conditions are:

         I.  No active row in the spdCompoundActionTable exists
             which has a matching spdCompActName.

         II. Or, at least one other active row in this table has a
             matching spdCompActName."
    ::= { spdSubactionsEntry 5 }

--
-- Static Actions
--

-- these are static actions that can be pointed to by the
-- spdRuleDefAction or the spdSubActSubActionName objects to
-- drop, accept, or reject packets.

spdStaticActions OBJECT IDENTIFIER ::= { spdConfigObjects 13 }

spdDropAction    OBJECT-TYPE
    SYNTAX      Integer32 (1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar indicates that a packet MUST be dropped
         and SHOULD NOT have action/packet logging."
    ::= { spdStaticActions 1 }

spdDropActionLog OBJECT-TYPE
    SYNTAX      Integer32 (1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar indicates that a packet MUST be dropped
         and SHOULD have action/packet logging."
    ::= { spdStaticActions 2 }

spdAcceptAction OBJECT-TYPE
    SYNTAX      Integer32 (1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This Scalar indicates that a packet MUST be accepted
         (pass-through) and SHOULD NOT have action/packet logging."
    ::= { spdStaticActions 3 }

spdAcceptActionLog OBJECT-TYPE
    SYNTAX      Integer32 (1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This scalar indicates that a packet MUST be accepted
         (pass-through) and SHOULD have action/packet logging."
    ::= { spdStaticActions 4 }

--
--
-- Notification objects information
--
--

spdNotificationVariables OBJECT IDENTIFIER ::=
   { spdNotificationObjects 1 }

spdNotifications OBJECT IDENTIFIER ::=
   { spdNotificationObjects 0 }

spdActionExecuted OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Points to the action instance that was executed that
         resulted in the notification being sent."
    ::= { spdNotificationVariables 1 }

spdIPEndpointAddType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the address type for the interface that the
         notification triggering packet is passing through."
    ::= { spdNotificationVariables 2 }

spdIPEndpointAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the interface address for the interface that the
         notification triggering packet is passing through.

         The format of this object is specified by the
         spdIPEndpointAddType object."
    ::= { spdNotificationVariables 3 }

spdIPSourceType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the source address type of the packet that
         triggered the notification."
    ::= { spdNotificationVariables 4 }

spdIPSourceAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the source address of the packet that
         triggered the notification.

         The format of this object is specified by the
         spdIPSourceType object."
    ::= { spdNotificationVariables 5 }

spdIPDestinationType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the destination address type of the packet
         that triggered the notification."
    ::= { spdNotificationVariables 6 }

spdIPDestinationAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Contains the destination address of the packet that
         triggered the notification.

         The format of this object is specified by the
         spdIPDestinationType object."
    ::= { spdNotificationVariables 7 }

spdPacketDirection OBJECT-TYPE
    SYNTAX      IfDirection
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "Indicates if the packet that triggered the action in
         questions was ingress (inbound) or egress (outbound)."
    ::= { spdNotificationVariables 8 }

spdPacketPart OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..65535))
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "spdPacketPart is the front part of the full IP packet that
         triggered this notification.  The initial size limit is
         determined by the smaller of the size, indicated by:

         I.  The value of the object with the TC syntax
             'SpdIPPacketLogging' that indicated the packet SHOULD be
             logged and

         II. The size of the triggering packet.

         The final limit is determined by the SNMP packet size when
         sending the notification.  The maximum size that can be
         included will be the smaller of the initial size, given the
         above, and the length that will fit in a single SNMP
         notification packet after the rest of the notification's
         objects and any other necessary packet data (headers encoding,
         etc.) have been included in the packet."
    ::= { spdNotificationVariables 9 }

spdActionNotification NOTIFICATION-TYPE
    OBJECTS { spdActionExecuted, spdIPEndpointAddType,
              spdIPEndpointAddress,
              spdIPSourceType, spdIPSourceAddress,
              spdIPDestinationType,
              spdIPDestinationAddress,
              spdPacketDirection }
    STATUS  current
    DESCRIPTION
        "Notification that an action was executed by a rule.
         Only actions with logging enabled will result in this
         notification getting sent.  The object includes the
         spdActionExecuted object, which will indicate which action
         was executed within the scope of the rule.  Additionally,
         the spdIPSourceType, spdIPSourceAddress,
         spdIPDestinationType, and spdIPDestinationAddress objects
         are included to indicate the packet source and destination
         of the packet that triggered the action.  Finally, the
         spdIPEndpointAddType, spdIPEndpointAddress, and
         spdPacketDirection objects indicate which interface the
         executed action was associated with, and if the packet was
         ingress or egress through the endpoint.

         A spdActionNotification SHOULD be limited to a maximum of
         one notification sent per minute for any action
         notifications that do not have any other configuration
         controlling their send rate.
         Note that compound actions with multiple executed
         sub-actions may result in multiple notifications being sent
         from a single rule execution."
    ::= { spdNotifications 1 }

spdPacketNotification NOTIFICATION-TYPE
    OBJECTS { spdActionExecuted, spdIPEndpointAddType,
              spdIPEndpointAddress,
              spdIPSourceType, spdIPSourceAddress,
              spdIPDestinationType,
              spdIPDestinationAddress,
              spdPacketDirection,
              spdPacketPart }
    STATUS  current
    DESCRIPTION
        "Notification that a packet passed through a Security
         Association (SA).  Only SAs created by actions with packet
         logging enabled will result in this notification getting
         sent.  The objects sent MUST include the spdActionExecuted,
         which will indicate which action was executed within the
         scope of the rule.  Additionally, the spdIPSourceType,
         spdIPSourceAddress, spdIPDestinationType, and
         spdIPDestinationAddress objects MUST be included to
         indicate the packet source and destination of the packet
         that triggered the action.  The spdIPEndpointAddType,
         spdIPEndpointAddress, and spdPacketDirection objects are
         included to indicate which endpoint the packet was
         associated with.  Finally, spdPacketPart is included to
         enable sending a variable sized part of the front of the
         packet with the size dependent on the value of the object of
         TC syntax 'SpdIPPacketLogging', which indicated that logging
         should be done.

         A spdPacketNotification SHOULD be limited to a maximum of
         one notification sent per minute for any action
         notifications that do not have any other configuration
         controlling their send rate.

         An action notification SHOULD be limited to a maximum of
         one notification sent per minute for any action
         notifications that do not have any other configuration
         controlling their send rate."
    ::= { spdNotifications 2 }


--
--
-- Conformance information
--
--

spdCompliances OBJECT IDENTIFIER
    ::= { spdConformanceObjects 1 }
spdGroups OBJECT IDENTIFIER
    ::= { spdConformanceObjects 2 }

--
-- Compliance statements
--
--
spdRuleFilterFullCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for SNMP entities that include
         an IPsec MIB implementation with Endpoint, Rules, and
         filters support.

         When this MIB is implemented with support for read-create,
         then such an implementation can claim full compliance.  Such
         devices can then be both monitored and configured with this
         MIB."

    MODULE -- This Module
        MANDATORY-GROUPS { spdEndpointGroup,
                           spdGroupContentsGroup,
                           spdRuleDefinitionGroup,
                           spdStaticFilterGroup,
                           spdStaticActionGroup ,
                           diffServMIBMultiFieldClfrGroup }

        GROUP spdIpsecSystemPolicyNameGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support a system policy group
             name."

        GROUP spdCompoundFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support compound filters."

        GROUP spdIPOffsetFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support IP Offset filters.  In
             general, this SHOULD be supported by a compliant IPsec
             Policy implementation."

        GROUP spdTimeFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support time filters."

        GROUP spdIpsoHeaderFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support IPSO Header filters."

        GROUP  spdCompoundActionGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support compound actions."

        OBJECT      spdEndGroupLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdGroupContComponentType
        SYNTAX      INTEGER {
                rule(2)
        }
        DESCRIPTION
            "Support of the value group(1) is only required for
             implementations that support Policy Groups within
             Policy Groups."

        OBJECT      spdGroupContLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdRuleDefLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdCompFiltLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdSubFiltLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
             "This object not required for compliance."

        OBJECT      spdIpOffFiltLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdTimeFiltLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdIpsoHeadFiltLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdCompActLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      spdSubActLastChanged
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object not required for compliance."

        OBJECT      diffServMultiFieldClfrNextFree
        MIN-ACCESS  not-accessible
        DESCRIPTION
            "This object is not required for compliance."

    ::= { spdCompliances 1 }


spdLoggingCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for SNMP entities that support
         sending notifications when actions are invoked."
    MODULE -- This Module
        MANDATORY-GROUPS { spdActionLoggingObjectGroup,
                           spdActionNotificationGroup }

    ::= { spdCompliances 2 }

--
-- ReadOnly Compliances
--
spdRuleFilterReadOnlyCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for SNMP entities that include
         an IPsec MIB implementation with Endpoint, Rules, and
         filters support.

         If this MIB is implemented without support for read-create
         (i.e., in read-only), it is not in full compliance, but it
         can claim read-only compliance.  Such a device can then be
         monitored, but cannot be configured with this MIB."

    MODULE -- This Module
        MANDATORY-GROUPS { spdEndpointGroup,
                           spdGroupContentsGroup,
                           spdRuleDefinitionGroup,
                           spdStaticFilterGroup,
                           spdStaticActionGroup ,
                           diffServMIBMultiFieldClfrGroup }

        GROUP spdIpsecSystemPolicyNameGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support a system policy group
             name."

        GROUP spdCompoundFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support compound filters."

        GROUP spdIPOffsetFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support IP Offset filters.  In
             general, this SHOULD be supported by a compliant IPsec
             Policy implementation."

        GROUP spdTimeFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support time filters."

        GROUP spdIpsoHeaderFilterGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support IPSO Header filters."

        GROUP  spdCompoundActionGroup
        DESCRIPTION
            "This group is mandatory for IPsec Policy
             implementations that support compound actions."

        OBJECT       spdCompActExecutionStrategy
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompActLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdCompActRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompActStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompFiltDescription
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompFiltLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdCompFiltLogicType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompFiltRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdCompFiltStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdEgressPolicyGroupName
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdEndGroupLastChanged
        DESCRIPTION
           "This object is not required for compliance."

        OBJECT       spdEndGroupName
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdEndGroupRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdEndGroupStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdGroupContComponentName
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdGroupContComponentType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdGroupContFilter
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdGroupContLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdGroupContRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdGroupContStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIngressPolicyGroupName
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpOffFiltLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdIpOffFiltOffset
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpOffFiltRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpOffFiltStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpOffFiltType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpOffFiltValue
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpsoHeadFiltClassification
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpsoHeadFiltLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdIpsoHeadFiltProtectionAuth
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpsoHeadFiltRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpsoHeadFiltStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdIpsoHeadFiltType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefAction
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefAdminStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefDescription
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefFilter
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefFilterNegated
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdRuleDefRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdRuleDefStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubActLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdSubActRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubActStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubActSubActionName
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubFiltLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdSubFiltRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubFiltStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubFiltSubfilter
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdSubFiltSubfilterIsNegated
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltDayOfMonthMask
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltDayOfWeekMask
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltLastChanged
        DESCRIPTION
            "This object is not required for compliance."

        OBJECT       spdTimeFiltMonthOfYearMask
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltPeriod
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltRowStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltTimeOfDayMask
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       spdTimeFiltStorageType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

    ::= { spdCompliances 3 }

--
--
-- Compliance Groups Definitions
--

--
-- Endpoint, Rule, Filter Compliance Groups
--

spdEndpointGroup OBJECT-GROUP
    OBJECTS {
        spdEndGroupName, spdEndGroupLastChanged,
        spdEndGroupStorageType, spdEndGroupRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy
         Endpoint Table."
    ::= { spdGroups 1 }

spdGroupContentsGroup OBJECT-GROUP
    OBJECTS {
        spdGroupContComponentType, spdGroupContFilter,
        spdGroupContComponentName, spdGroupContLastChanged,
        spdGroupContStorageType, spdGroupContRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy
         Group Contents Table."
    ::= { spdGroups 2 }

spdIpsecSystemPolicyNameGroup OBJECT-GROUP
    OBJECTS {
        spdIngressPolicyGroupName,
        spdEgressPolicyGroupName
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects represent the System
         Policy Group Names."
    ::= { spdGroups 3}

spdRuleDefinitionGroup OBJECT-GROUP
    OBJECTS {
        spdRuleDefDescription, spdRuleDefFilter,
        spdRuleDefFilterNegated, spdRuleDefAction,
        spdRuleDefAdminStatus, spdRuleDefLastChanged,
        spdRuleDefStorageType, spdRuleDefRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy Rule
        Definition Table."
    ::= { spdGroups 4 }

spdCompoundFilterGroup OBJECT-GROUP
    OBJECTS {
        spdCompFiltDescription, spdCompFiltLogicType,
        spdCompFiltLastChanged, spdCompFiltStorageType,
        spdCompFiltRowStatus, spdSubFiltSubfilter,
        spdSubFiltSubfilterIsNegated, spdSubFiltLastChanged,
        spdSubFiltStorageType, spdSubFiltRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy
         Compound Filter Table and Sub-Filter Table Group."
    ::= { spdGroups 5 }

spdStaticFilterGroup OBJECT-GROUP
        OBJECTS { spdTrueFilter }
     STATUS current
     DESCRIPTION
         "The static filter group.  Currently this is just a true
          filter."
    ::= { spdGroups 6 }

spdIPOffsetFilterGroup OBJECT-GROUP
    OBJECTS {
        spdIpOffFiltOffset, spdIpOffFiltType,
        spdIpOffFiltValue, spdIpOffFiltLastChanged,
        spdIpOffFiltStorageType, spdIpOffFiltRowStatus
    }

    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy IP
         Offset Filter Table."
    ::= { spdGroups 7 }

spdTimeFilterGroup OBJECT-GROUP
    OBJECTS {
        spdTimeFiltPeriod,
        spdTimeFiltMonthOfYearMask, spdTimeFiltDayOfMonthMask,
        spdTimeFiltDayOfWeekMask, spdTimeFiltTimeOfDayMask,
        spdTimeFiltLastChanged,
        spdTimeFiltStorageType, spdTimeFiltRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy Time
         Filter Table."
    ::= { spdGroups 8 }

spdIpsoHeaderFilterGroup OBJECT-GROUP
    OBJECTS {
        spdIpsoHeadFiltType, spdIpsoHeadFiltClassification,
        spdIpsoHeadFiltProtectionAuth, spdIpsoHeadFiltLastChanged,
        spdIpsoHeadFiltStorageType, spdIpsoHeadFiltRowStatus
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy IPSO
         Header Filter Table."
    ::= { spdGroups 9 }

--
-- action compliance groups
--

spdStaticActionGroup OBJECT-GROUP
    OBJECTS {
        spdDropAction, spdAcceptAction,
        spdDropActionLog, spdAcceptActionLog
    }
    STATUS current
    DESCRIPTION
        "This group is made up of objects from the IPsec Policy
         Static Actions."
    ::= { spdGroups 10 }

spdCompoundActionGroup OBJECT-GROUP
    OBJECTS {
        spdCompActExecutionStrategy, spdCompActLastChanged,
        spdCompActStorageType,

        spdCompActRowStatus, spdSubActSubActionName,
        spdSubActLastChanged, spdSubActStorageType,
        spdSubActRowStatus
    }
    STATUS current
    DESCRIPTION
        "The IPsec Policy Compound Action Table and Actions In
         Compound Action Table Group."
    ::= { spdGroups 11 }

spdActionLoggingObjectGroup OBJECT-GROUP
    OBJECTS {
        spdActionExecuted,
        spdIPEndpointAddType,   spdIPEndpointAddress,
        spdIPSourceType,        spdIPSourceAddress,
        spdIPDestinationType,   spdIPDestinationAddress,
        spdPacketDirection,     spdPacketPart
    }
    STATUS current
    DESCRIPTION
        "This group is made up of all the Notification objects for
        this MIB."
    ::= { spdGroups 12 }

spdActionNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
        spdActionNotification,
        spdPacketNotification
    }
    STATUS current
    DESCRIPTION
        "This group is made up of all the Notifications for this MIB."
    ::= { spdGroups 13 }


END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

