-- extracted from rfc4268.txt
-- at Thu Dec  1 06:40:07 2005

   ENTITY-STATE-TC-MIB DEFINITIONS ::= BEGIN

   IMPORTS
      MODULE-IDENTITY, mib-2       FROM SNMPv2-SMI
      TEXTUAL-CONVENTION           FROM SNMPv2-TC;

    entityStateTc MODULE-IDENTITY
        LAST-UPDATED "200511220000Z"
        ORGANIZATION "IETF Entity MIB Working Group"
        CONTACT-INFO
                "General Discussion: entmib@ietf.org
                 To Subscribe:
                 http://www.ietf.org/mailman/listinfo/entmib

                 http://www.ietf.org/html.charters/entmib-charter.html

                 Sharon Chisholm
                 Nortel Networks
                 PO Box 3511 Station C
                 Ottawa, Ont.  K1Y 4H7
                 Canada
                 schishol@nortel.com

                 David T. Perkins
                 548 Qualbrook Ct
                 San Jose, CA 95110
                 USA
                 Phone: 408 394-8702
                 dperkins@snmpinfo.com"
         DESCRIPTION
                "This MIB defines state textual conventions.

                 Copyright (C) The Internet Society 2005.  This version
                 of this MIB module is part of RFC 4268;  see the RFC
                 itself for full legal notices."
         REVISION    "200511220000Z"
         DESCRIPTION
             "Initial version, published as RFC 4268."
        ::= { mib-2 130 }

     EntityAdminState  ::=  TEXTUAL-CONVENTION
       STATUS         current
       DESCRIPTION
            " Represents the various possible administrative states.
              A value of 'locked' means the resource is administratively
              prohibited from use.  A value of 'shuttingDown' means that
              usage is administratively limited to current instances of
              use.  A value of 'unlocked' means the resource is not
              administratively prohibited from use.  A value of
              'unknown' means that this resource is unable to
              report administrative state."
       SYNTAX         INTEGER
                 {
                 unknown (1),
                 locked (2),
                 shuttingDown (3),
                 unlocked (4)
                 }

     EntityOperState  ::=  TEXTUAL-CONVENTION
       STATUS         current
       DESCRIPTION
            " Represents the possible values of operational states.

              A value of 'disabled' means the resource is totally
              inoperable.  A value of 'enabled' means the resource
              is partially or fully operable.  A value of 'testing'
              means the resource is currently being tested
              and cannot therefore report whether it is operational
              or not.  A value of 'unknown' means that this
              resource is unable to report operational state."
       SYNTAX         INTEGER
                 {
                 unknown (1),
                 disabled (2),
                 enabled (3),
                 testing (4)
                 }

     EntityUsageState  ::=  TEXTUAL-CONVENTION
       STATUS         current
       DESCRIPTION
            " Represents the possible values of usage states.
              A value of 'idle' means the resource is servicing no
              users.  A value of 'active' means the resource is
              currently in use and it has sufficient spare capacity
              to provide for additional users.  A value of 'busy'
              means the resource is currently in use, but it
              currently has no spare capacity to provide for
              additional users.  A value of 'unknown' means
              that this resource is unable to report usage state."
       SYNTAX         INTEGER
                 {
                 unknown (1),
                 idle (2),
                 active (3),
                 busy (4)
                 }


    EntityAlarmStatus  ::=  TEXTUAL-CONVENTION
       STATUS         current
       DESCRIPTION
          " Represents the possible values of alarm status.
            An Alarm [RFC3877] is a persistent indication
            of an error or warning condition.

            When no bits of this attribute are set, then no active
            alarms are known against this entity and it is not under
            repair.

            When the 'value of underRepair' is set, the resource is
            currently being repaired, which, depending on the
            implementation, may make the other values in this bit
            string not meaningful.

            When the value of 'critical' is set, one or more critical
            alarms are active against the resource.  When the value
            of 'major' is set, one or more major alarms are active
            against the resource.  When the value of 'minor' is set,
            one or more minor alarms are active against the resource.
            When the value of 'warning' is set, one or more warning
            alarms are active against the resource.  When the value
            of 'indeterminate' is set, one or more alarms of whose
            perceived severity cannot be determined are active
            against this resource.

            A value of 'unknown' means that this resource is
            unable to report alarm state."
             SYNTAX         BITS
                {
                unknown (0),
                underRepair (1),
                critical(2),
                major(3),
                minor(4),
                -- The following are not defined in X.733
                warning (5),
                indeterminate (6)
                              }

     EntityStandbyStatus  ::=  TEXTUAL-CONVENTION
       STATUS         current
       DESCRIPTION
            " Represents the possible values of standby status.

              A value of 'hotStandby' means the resource is not
              providing service, but it will be immediately able to
              take over the role of the resource to be backed up,
              without the need for initialization activity, and will
              contain the same information as the resource to be
              backed up.  A value of 'coldStandy' means that the
              resource is to back up another resource, but will not
              be immediately able to take over the role of a resource
              to be backed up, and will require some initialization
              activity.  A value of 'providingService' means the
              resource is providing service.  A value of
              'unknown' means that this resource is unable to
              report standby state."
             SYNTAX         INTEGER
               {
               unknown (1),
               hotStandby (2),
               coldStandby (3),
               providingService (4)
               }

   END

-- 
--    Copyright (C) The Internet Society (2005).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 

