-- extracted from rfc4803.txt
-- at Thu Mar  1 06:08:21 2007

GMPLS-LABEL-STD-MIB DEFINITIONS ::= BEGIN

IMPORTS
  MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, Integer32
    FROM SNMPv2-SMI                                   -- RFC 2578
  MODULE-COMPLIANCE, OBJECT-GROUP
    FROM SNMPv2-CONF                                  -- RFC 2580
  RowStatus, StorageType
    FROM SNMPv2-TC                                    -- RFC 2579
  InterfaceIndexOrZero
    FROM IF-MIB                                       -- RFC 2863
  IndexIntegerNextFree
    FROM DIFFSERV-MIB                                 -- RFC 3289
  MplsLabel, mplsStdMIB
    FROM MPLS-TC-STD-MIB                              -- RFC 3811
  GmplsLabelTypeTC, GmplsFreeformLabelTC
    FROM GMPLS-TC-STD-MIB                             -- RFC 4801
;

gmplsLabelStdMIB MODULE-IDENTITY
  LAST-UPDATED
    "200702270000Z" -- 27 February 2007 00:00:00 GMT
  ORGANIZATION
    "IETF Common Control and Measurement Plane (CCAMP) Working Group"
  CONTACT-INFO
    "       Thomas D. Nadeau
            Cisco Systems, Inc.
     Email: tnadeau@cisco.com

            Adrian Farrel
            Old Dog Consulting
     Email: adrian@olddog.co.uk

     Comments about this document should be emailed directly to the
     CCAMP working group mailing list at ccamp@ops.ietf.org."

  DESCRIPTION
    "Copyright (C) The IETF Trust (2007).  This version of
     this MIB module is part of RFC 4803; see the RFC itself for
     full legal notices.
     This MIB module contains managed object definitions for labels
     within GMPLS systems as defined in
     Generalized Multi-Protocol Label Switching (GMPLS) Signaling
     Functional Description, Berger, L. (Editor), RFC 3471,
     January 2003."
  REVISION
    "200702270000Z" -- 27 February 2007 00:00:00 GMT
  DESCRIPTION
    "Initial version issued as part of RFC 4803."
  ::= { mplsStdMIB 16 }

-- no notifications are currently defined.

gmplsLabelObjects        OBJECT IDENTIFIER ::= { gmplsLabelStdMIB 1 }
gmplsLabelConformance    OBJECT IDENTIFIER ::= { gmplsLabelStdMIB 2 }

gmplsLabelIndexNext OBJECT-TYPE
  SYNTAX        IndexIntegerNextFree
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "This object contains an unused value for gmplsLabelIndex,
       or a zero to indicate that no unused value exists or is
       available.

       A management application wishing to create a row in the
       gmplsLabelTable may read this object and then attempt to
       create a row in the table.  If row creation fails (because
       another application has already created a row with the
       supplied index), the management application should read this
       object again to get a new index value.

       When a row is created in the gmplsLabelTable with the
       gmplsLabelIndex value held by this object, an implementation
       MUST change the value in this object."
  ::= { gmplsLabelObjects 1 }

gmplsLabelTable OBJECT-TYPE
  SYNTAX        SEQUENCE OF GmplsLabelEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "Table of GMPLS Labels.  This table allows the representation
     of the more complex label forms required for GMPLS that cannot
     be held within the TEXTUAL-CONVENTION MplsLabel; that is, labels
     that cannot be encoded within 32 bits.  It is, nevertheless, also
     capable of holding 32-bit labels or regular MPLS Labels if
     desired.
     Each entry in this table represents an individual GMPLS Label
     value.  The representation of Labels in tables in other MIB
     modules may be achieved by a referrence to an entry in this
     table by means of a row pointer into this table.  The indexing
     of this table provides for arbitrary indexing and also for
     concatenation of labels.

     For an example of label concatenation, see RFC 3945, section 7.1.
     In essence, a GMPLS Label may be composite in order to identify
     a set of resources in the data plane.  Practical examples are
     timeslots and wavelength sets (which are not contiguous like
     wavebands).

     The indexing mechanism allows multiple entries in this table to
     be seen as a sequence of labels that should be concatenated.
     Ordering is potentially very sensitive for concatenation."
   REFERENCE
     "1. Generalized Multiprotocol Label Switching (GMPLS)
         Architecture, RFC 3945, section 7.1."
::= { gmplsLabelObjects 2 }

gmplsLabelEntry OBJECT-TYPE
  SYNTAX        GmplsLabelEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "An entry in this table represents a single label value.  There
     are three indexes into the table.

     -  The interface index may be helpful to distinguish which
        labels are in use on which interfaces or to handle cases
        where there are a very large number of labels in use in the
        system.  When label representation is desired to apply to the
        whole system or when it is not important to distinguish
        labels by their interfaces, this index MAY be set to zero.

     -  The label index provides a way of identifying the label.

     -  The label sub-index is only used for concatenated labels.  It
        identifies each component label.  When non-concatenated labels
        are used, this index SHOULD be set to zero.

     A storage type object is supplied to control the storage type
     for each entry, but implementations should note that the storage
     type of conceptual rows in other tables that include row
     pointers to an entry in this table SHOULD dictate the storage
     type of the rows in this table where the row in the other table
     is more persistent."

  INDEX {
    gmplsLabelInterface,
    gmplsLabelIndex,
    gmplsLabelSubindex }
::= { gmplsLabelTable 1 }

GmplsLabelEntry ::= SEQUENCE {
  gmplsLabelInterface           InterfaceIndexOrZero,
  gmplsLabelIndex               Unsigned32,
  gmplsLabelSubindex            Unsigned32,
  gmplsLabelType                GmplsLabelTypeTC,
  gmplsLabelMplsLabel           MplsLabel,
  gmplsLabelPortWavelength      Unsigned32,
  gmplsLabelFreeform            GmplsFreeformLabelTC,
  gmplsLabelSonetSdhSignalIndex Integer32,
  gmplsLabelSdhVc               Integer32,
  gmplsLabelSdhVcBranch         Integer32,
  gmplsLabelSonetSdhBranch      Integer32,
  gmplsLabelSonetSdhGroupBranch Integer32,
  gmplsLabelWavebandId          Unsigned32,
  gmplsLabelWavebandStart       Unsigned32,
  gmplsLabelWavebandEnd         Unsigned32,
  gmplsLabelStorageType         StorageType,
  gmplsLabelRowStatus           RowStatus
}

gmplsLabelInterface OBJECT-TYPE
  SYNTAX        InterfaceIndexOrZero
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "The interface on which this label is used.  If this object is set
     to zero, the label MUST have applicability across the
     whole system and not be limited to a single interface."
::= { gmplsLabelEntry 1 }

gmplsLabelIndex OBJECT-TYPE
  SYNTAX        Unsigned32 (0..4294967295)
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "An arbitrary index into the table to identify a label.

     Note that implementations that are representing 32-bit labels
     within this table MAY choose to align this index with the value
     of the label, and this may result in the use of the value zero
     since it represents a valid label value.  Such implementation
     should be aware of the implications of sparsely populated
     tables.

     A management application may read the gmplsLabelIndexNext
     object to find a suitable value for this object."
::= { gmplsLabelEntry 2 }

gmplsLabelSubindex OBJECT-TYPE
  SYNTAX        Unsigned32 (0..4294967295)
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "In conjunction with gmplsLabelInterface and gmplsLabelIndex,
     this object uniquely identifies this row.  This sub-index allows
     a single GMPLS Label to be defined as a concatenation of labels.
     This is particularly useful in TDM.

     The ordering of sub-labels is strict with the sub-label with
     the lowest gmplsLabelSubindex appearing first.  Note that all
     sub-labels of a single GMPLS Label must share the same
     gmplsLabelInterface and gmplsLabelIndex values.  For labels that
     are not composed of concatenated sub-labels, this value SHOULD
     be set to zero."
::= { gmplsLabelEntry 3 }

gmplsLabelType OBJECT-TYPE
  SYNTAX        GmplsLabelTypeTC
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "Identifies the type of this label.  Note that this object does
     not determine whether MPLS or GMPLS signaling is in use: a value
     of gmplsMplsLabel(1) denotes that an MPLS Packet Label is
     present in the gmplsLabelMplsLabel object and encoded using the
     MplsLabel TEXTUAL-CONVENTION (may be a 20-bit MPLS Label, a 10-
     or 23-bit Frame Relay Label, or an Asynchronous Transfer Mode
     (ATM) Label), but does not describe whether this is signaled
     using MPLS or GMPLS.

     The value of this object helps determine which of the following
     objects are valid.  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
   REFERENCE
     "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
         Functional Description, RFC 3471, section 3."
::= { gmplsLabelEntry 4 }

gmplsLabelMplsLabel OBJECT-TYPE
  SYNTAX         MplsLabel
  MAX-ACCESS     read-create
  STATUS         current
  DESCRIPTION
    "The value of an MPLS Label (that is a Packet Label) if this
     table is used to store it.  This may be used in MPLS systems even
     though the label values can be adequately stored in the MPLS MIB
     modules (MPLS-LSR-STD-MIB and MPLS-TE-STD-MIB).  Furthermore, in
     mixed MPLS and GMPLS systems, it may be advantageous to store all
     labels in a single label table.  Lastly, in GMPLS systems where
     Packet Labels are used (that is in systems that use GMPLS
     signaling and GMPLS Labels for packet switching), it may be
     desirable to use this table.

     This object is only valid if gmplsLabelType is set
     to gmplsMplsLabel(1).  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. MPLS Label Stack Encoding, RFC 3032."
  DEFVAL { 0 }
::= { gmplsLabelEntry 5 }

gmplsLabelPortWavelength OBJECT-TYPE
  SYNTAX        Unsigned32
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The value of a Port or Wavelength Label when carried as a
     Generalized Label.  Only valid if gmplsLabelType is set to
     gmplsPortWavelengthLabel(2).  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
        Functional Description, RFC 3471, section 3.2.1.1."
  DEFVAL { 0 }
::= { gmplsLabelEntry 6 }

gmplsLabelFreeform OBJECT-TYPE
  SYNTAX        GmplsFreeformLabelTC
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The value of a Freeform Generalized Label that does not conform
     to one of the standardized label encodings or that an
     implementation chooses to represent as an octet string without
     further decoding.  Only valid if gmplsLabelType is set to
     gmplsFreeformLabel(3).  This object cannot be modified
     if gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
        Functional Description, RFC 3471, section 3.2."
  DEFVAL { '00'h }
::= { gmplsLabelEntry 7 }

gmplsLabelSonetSdhSignalIndex OBJECT-TYPE
  SYNTAX        Integer32 (0..4095)
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The Signal Index value (S) of a SONET or SDH Generalized Label.
     Zero indicates that this field is non-significant.  Only valid if
     gmplsLabelType is set to gmplsSonetLabel(4) or gmplsSdhLabel(5).
     This object cannot be modified if gmplsLabelRowStatus is
     active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Extensions
        for Synchronous Optical Network (SONET) and Synchronous
        Digital Hierarchy (SDH) Control, RFC 4606, section 3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 8 }

gmplsLabelSdhVc OBJECT-TYPE
  SYNTAX        Integer32 (0..15)
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The VC Indicator (U) of an SDH Generalized Label.  Zero indicates
     that this field is non-significant.  Only valid if gmplsLabelType
     is set to gmplsSdhLabel(5).  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Extensions
        for Synchronous Optical Network (SONET) and Synchronous
        Digital Hierarchy (SDH) Control, RFC 4606, section 3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 9 }

gmplsLabelSdhVcBranch OBJECT-TYPE
  SYNTAX        Integer32 (0..15)
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The VC Branch Indicator (K) of an SDH Generalized Label.  Zero
     indicates that this field is non-significant.  Only valid if
     gmplsLabelType is set to gmplsSdhLabel(5).  This
     object cannot be modified if gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Extensions
        for Synchronous Optical Network (SONET) and Synchronous
        Digital Hierarchy (SDH) Control, RFC 4606, section 3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 10 }

gmplsLabelSonetSdhBranch OBJECT-TYPE
  SYNTAX        Integer32 (0..15)
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The Branch Indicator (L) of a SONET or SDH Generalized Label.
     Zero indicates that this field is non-significant.  Only valid
     gmplsLabelType is set to gmplsSonetLabel(4) or
     gmplsSdhLabel(5).  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Extensions
        for Synchronous Optical Network (SONET) and Synchronous
        Digital Hierarchy (SDH) Control, RFC 4606, section 3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 11 }

gmplsLabelSonetSdhGroupBranch OBJECT-TYPE
  SYNTAX        Integer32 (0..15)
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The Group Branch Indicator (M) of a SONET or SDH Generalized
     Label.  Zero indicates that this field is non-significant.
     Only valid if gmplsLabelType is set to gmplsSonetLabel(4) or
     gmplsSdhLabel(5).  This object cannot be modified if
     gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Extensions
        for Synchronous Optical Network (SONET) and Synchronous
        Digital Hierarchy (SDH) Control, RFC 4606, section 3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 12 }

gmplsLabelWavebandId OBJECT-TYPE
  SYNTAX        Unsigned32
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The waveband identifier component of a Waveband Label.  Only
     valid if gmplsLabelType is set to gmplsWavebandLabel(6).  This
     object cannot be modified if gmplsLabelRowStatus is active(1)."

  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
        Functional Description, RFC 3471, section 3.3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 13 }

gmplsLabelWavebandStart OBJECT-TYPE
  SYNTAX        Unsigned32
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The starting label component of a Waveband Label.  Only valid if
     gmplsLabelType is set to gmplsWavebandLabel(6).  This object
     cannot be modified if gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
        Functional Description, RFC 3471, section 3.3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 14 }

gmplsLabelWavebandEnd OBJECT-TYPE
  SYNTAX        Unsigned32
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "The end label component of a Waveband Label.  Only valid if
     gmplsLabelType is set to gmplsWavebandLabel(6).  This object
     cannot be modified if gmplsLabelRowStatus is active(1)."
  REFERENCE
    "1. Generalized Multi-Protocol Label Switching (GMPLS) Signaling
        Functional Description, RFC 3471, section 3.3."
  DEFVAL { 0 }
::= { gmplsLabelEntry 15 }

gmplsLabelStorageType OBJECT-TYPE
  SYNTAX        StorageType
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "This variable indicates the storage type for this row.  The
     agent MUST ensure that this object's value remains consistent
     with the storage type of any rows in other tables that contain
     pointers to this row.  In particular, the storage type of this
     row must be at least as permanent as that of any row that points
     to it.
     Conceptual rows having the value 'permanent' need not
     allow write-access to any columnar objects in the row."
  REFERENCE
    "1. Textual Conventions for SMIv2, STD 58, RFC 2579, section 2."
  DEFVAL { volatile }
::= { gmplsLabelEntry 16 }

gmplsLabelRowStatus OBJECT-TYPE
  SYNTAX        RowStatus
  MAX-ACCESS    read-create
  STATUS        current
  DESCRIPTION
    "This variable is used to create, modify, and/or delete a row in
     this table.  When a row in this table has a row in the active(1)
     state, no objects in this row can be modified except the
     gmplsLabelRowStatus and gmplsLabelStorageType.

     The gmplsLabelType object does not have a default and must be
     set before a row can become active.  The corresponding label
     objects (dependent on the value of gmplsLabelType) should also
     be set unless they happen to need to use the specified default
     values as follows:

     gmplsLabelType setting             objects to be set
     --------------------------------------------------------------
     gmplsMplsLabel(1)                  gmplsLabelMplsLabel

     gmplsPortWavelengthLabel(2)        gmplsLabelPortWavelength

     gmplsFreeformLabel(3)              gmplsLabelFreeform

     gmplsSonetLabel(4)                 gmplsLabelSonetSdhSignalIndex
                                        gmplsLabelSdhVc
                                        gmplsLabelSdhVcBranch
                                        gmplsLabelSonetSdhBranch
                                        gmplsLabelSonetSdhGroupBranch

     gmplsSdhLabel(5)                   gmplsLabelSonetSdhSignalIndex
                                        gmplsLabelSdhVc
                                        gmplsLabelSdhVcBranch
                                        gmplsLabelSonetSdhBranch
                                        gmplsLabelSonetSdhGroupBranch

     gmplsWavebandLabel(6)              gmplsLabelWavebandId
                                        gmplsLabelWavebandStart
                                        gmplsLabelWavebandEnd"
::= { gmplsLabelEntry 17 }

gmplsLabelGroups
  OBJECT IDENTIFIER ::= { gmplsLabelConformance 1 }

gmplsLabelCompliances
  OBJECT IDENTIFIER ::= { gmplsLabelConformance 2 }

gmplsLabelModuleReadOnlyCompliance MODULE-COMPLIANCE
  STATUS current
  DESCRIPTION
    "Compliance requirement for implementations that only provide
     read-only support for GMPLS-LABEL-STD-MIB.  Such devices can then
     be monitored but cannot be configured using this MIB module."

  MODULE -- this module

  -- The mandatory groups have to be implemented by LSRs claiming
  -- support for this MIB module.  This MIB module is, however, not
  -- mandatory for a working implementation of a GMPLS LSR with full
  -- MIB support if the GMPLS Labels in use can be represented within
  -- a 32-bit quantity.

  MANDATORY-GROUPS {
    gmplsLabelTableGroup
  }

  GROUP gmplsLabelPacketGroup
  DESCRIPTION
    "This group extends gmplsLabelTableGroup for implementations that
     support Packet Labels.  It is optional for implementations that
     do not support Packet Labels."

  GROUP gmplsLabelPortWavelengthGroup
  DESCRIPTION
    "This group extends gmplsLabelTableGroup for implementations that
     support Port and Wavelength Labels.  It is optional for
     implementations that do not support Wavelength Labels."

  GROUP gmplsLabelFreeformGroup
  DESCRIPTION
    "This group extends gmplsLabelTableGroup for implementations that
     support Freeform Labels.  It is optional for implementations that
     do not support Freeform Labels."

  GROUP gmplsLabelSonetSdhGroup
  DESCRIPTION
    "This group extends gmplsLabelTableGroup for implementations that
     support SONET or SDH Labels.  It is optional for implementations
     that do not support SONET or SDH Labels."

  GROUP gmplsLabelWavebandGroup
  DESCRIPTION
    "This group extends gmplsLabelTableGroup for implementations that
     support Waveband Labels.  It is optional for implementations that
     do not support Waveband Labels."
  OBJECT      gmplsLabelType
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelMplsLabel
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelPortWavelength
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelFreeform
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelSonetSdhSignalIndex
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelSdhVc
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelSdhVcBranch
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelSonetSdhBranch
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelSonetSdhGroupBranch
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelWavebandId
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."
  OBJECT      gmplsLabelWavebandStart
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelWavebandEnd
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT      gmplsLabelStorageType
  MIN-ACCESS  read-only
  DESCRIPTION
    "Write access is not required."

  OBJECT       gmplsLabelRowStatus
  SYNTAX       RowStatus { active(1) }
  MIN-ACCESS   read-only
  DESCRIPTION
    "Write access is not required, and active(1) is
     the only status that needs to be supported."

::= { gmplsLabelCompliances 1 }

gmplsLabelModuleFullCompliance MODULE-COMPLIANCE
  STATUS current
  DESCRIPTION
    "Compliance statement for agents that support the complete
     GMPLS-LABEL-STD-MIB module.

     The mandatory groups have to be implemented by GMPLS LSRs
     claiming support for this MIB module.  This MIB module is,
     however, not mandatory for a working implementation of a GMPLS
     LSR with full MIB support if the GMPLS Labels in use can be
     represented within a 32-bit quantity."

  MODULE -- this module

  MANDATORY-GROUPS {
    gmplsLabelTableGroup
  }

::= { gmplsLabelCompliances 2 }
gmplsLabelTableGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelIndexNext,
    gmplsLabelType,
    gmplsLabelStorageType,
    gmplsLabelRowStatus
  }

  STATUS  current
  DESCRIPTION
    "Necessary, but not sufficient, set of objects to implement label
     table support.  In addition, depending on the type of labels
     supported, the following other groups defined below are
     mandatory:

       gmplsLabelWavebandGroup and/or
       gmplsLabelPacketGroup and/or
       gmplsLabelPortWavelengthGroup and/or
       gmplsLabelFreeformGroup and/or
       gmplsLabelSonetSdhGroup."
::= { gmplsLabelGroups 1 }

gmplsLabelPacketGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelMplsLabel
  }
  STATUS  current
  DESCRIPTION
    "Object needed to implement Packet (MPLS) Labels."
::= { gmplsLabelGroups 2 }

gmplsLabelPortWavelengthGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelPortWavelength
  }
  STATUS  current
  DESCRIPTION
    "Object needed to implement Port and Wavelength Labels."
::= { gmplsLabelGroups 3 }

gmplsLabelFreeformGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelFreeform
  }
  STATUS  current
  DESCRIPTION
    "Object needed to implement Freeform Labels."
::= { gmplsLabelGroups 4 }
gmplsLabelSonetSdhGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelSonetSdhSignalIndex,
    gmplsLabelSdhVc,
    gmplsLabelSdhVcBranch,
    gmplsLabelSonetSdhBranch,
    gmplsLabelSonetSdhGroupBranch
  }
  STATUS  current
  DESCRIPTION
    "Objects needed to implement SONET and SDH Labels."
::= { gmplsLabelGroups 5 }

gmplsLabelWavebandGroup OBJECT-GROUP
  OBJECTS {
    gmplsLabelWavebandId,
    gmplsLabelWavebandStart,
    gmplsLabelWavebandEnd
  }
  STATUS  current
  DESCRIPTION
    "Objects needed to implement Waveband Labels."
::= { gmplsLabelGroups 6 }

END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

