

   SNMPv2-TM DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, OBJECT-IDENTITY,
       snmpModules, snmpDomains, snmpProxys
           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION
           FROM SNMPv2-TC;

   snmpv2tm MODULE-IDENTITY
       LAST-UPDATED "200210160000Z"
       ORGANIZATION "IETF SNMPv3 Working Group"
       CONTACT-INFO
               "WG-EMail:   snmpv3@lists.tislabs.com
                Subscribe:  snmpv3-request@lists.tislabs.com

                Co-Chair:   Russ Mundy
                            Network Associates Laboratories
                postal:     15204 Omega Drive, Suite 300
                            Rockville, MD 20850-4601
                            USA
                EMail:      mundy@tislabs.com
                phone:      +1 301 947-7107
                Co-Chair:   David Harrington
                            Enterasys Networks
                postal:     35 Industrial Way
                            P. O. Box 5005
                            Rochester, NH 03866-5005
                            USA
                EMail:      dbh@enterasys.com
                phone:      +1 603 337-2614

                Editor:     Randy Presuhn
                            BMC Software, Inc.
                postal:     2141 North First Street
                            San Jose, CA 95131
                            USA
                EMail:      randy_presuhn@bmc.com
                phone:      +1 408 546-1006"
       DESCRIPTION
               "The MIB module for SNMP transport mappings.

                Copyright (C) The Internet Society (2002). This
                version of this MIB module is part of RFC 3417;
                see the RFC itself for full legal notices.
               "
       REVISION     "200210160000Z"
       DESCRIPTION
               "Clarifications, published as RFC 3417."
       REVISION    "199601010000Z"
       DESCRIPTION
               "Clarifications, published as RFC 1906."
       REVISION    "199304010000Z"
       DESCRIPTION
               "The initial version, published as RFC 1449."
       ::= { snmpModules 19 }

   -- SNMP over UDP over IPv4

   snmpUDPDomain  OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "The SNMP over UDP over IPv4 transport domain.
               The corresponding transport address is of type
               SnmpUDPAddress."
       ::= { snmpDomains 1 }





   SnmpUDPAddress ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "1d.1d.1d.1d/2d"
       STATUS       current
       DESCRIPTION
               "Represents a UDP over IPv4 address:

                  octets   contents        encoding
                   1-4     IP-address      network-byte order
                   5-6     UDP-port        network-byte order
               "
       SYNTAX       OCTET STRING (SIZE (6))

   -- SNMP over OSI

   snmpCLNSDomain OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "The SNMP over CLNS transport domain.
               The corresponding transport address is of type
               SnmpOSIAddress."
       ::= { snmpDomains 2 }

   snmpCONSDomain OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "The SNMP over CONS transport domain.
               The corresponding transport address is of type
               SnmpOSIAddress."
       ::= { snmpDomains 3 }

   SnmpOSIAddress ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "*1x:/1x:"
       STATUS       current
       DESCRIPTION
               "Represents an OSI transport-address:

             octets   contents           encoding
                1     length of NSAP     'n' as an unsigned-integer
                                            (either 0 or from 3 to 20)
             2..(n+1) NSAP                concrete binary representation
             (n+2)..m TSEL                string of (up to 64) octets
               "
       SYNTAX       OCTET STRING (SIZE (1 | 4..85))

   -- SNMP over DDP

   snmpDDPDomain  OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "The SNMP over DDP transport domain.  The corresponding
               transport address is of type SnmpNBPAddress."
       ::= { snmpDomains 4 }

   SnmpNBPAddress ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "Represents an NBP name:

            octets        contents          encoding
               1          length of object  'n' as an unsigned integer
             2..(n+1)     object            string of (up to 32) octets
              n+2         length of type    'p' as an unsigned integer
         (n+3)..(n+2+p)   type              string of (up to 32) octets
             n+3+p        length of zone    'q' as an unsigned integer
       (n+4+p)..(n+3+p+q) zone              string of (up to 32) octets

               For comparison purposes, strings are
               case-insensitive. All strings may contain any octet
               other than 255 (hex ff)."
       SYNTAX       OCTET STRING (SIZE (3..99))

   -- SNMP over IPX

   snmpIPXDomain  OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "The SNMP over IPX transport domain.  The corresponding
               transport address is of type SnmpIPXAddress."
       ::= { snmpDomains 5 }

   SnmpIPXAddress ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "4x.1x:1x:1x:1x:1x:1x.2d"
       STATUS       current
       DESCRIPTION
               "Represents an IPX address:

                  octets   contents            encoding
                   1-4     network-number      network-byte order
                   5-10    physical-address    network-byte order
                  11-12    socket-number       network-byte order
               "
       SYNTAX       OCTET STRING (SIZE (12))

   -- for proxy to SNMPv1 (RFC 1157)

   rfc1157Proxy   OBJECT IDENTIFIER ::= { snmpProxys 1 }

   rfc1157Domain  OBJECT-IDENTITY
       STATUS     deprecated
       DESCRIPTION
               "The transport domain for SNMPv1 over UDP over IPv4.
               The corresponding transport address is of type
               SnmpUDPAddress."
       ::= { rfc1157Proxy 1 }

   --  ::= { rfc1157Proxy 2 }            this OID is obsolete

   END

