-- extracted from rfc3877.txt
-- at Sat Sep 18 06:23:14 2004

ALARM-MIB DEFINITIONS ::= BEGIN

IMPORTS
   MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
   Integer32, Unsigned32, Gauge32,
   TimeTicks, Counter32, Counter64,
   IpAddress, Opaque, mib-2,
   zeroDotZero
       FROM SNMPv2-SMI                 -- [RFC2578]
   DateAndTime,
   RowStatus, RowPointer,
   TEXTUAL-CONVENTION
       FROM SNMPv2-TC                  -- [RFC2579]
   SnmpAdminString
       FROM SNMP-FRAMEWORK-MIB         -- [RFC3411]
   InetAddressType, InetAddress
       FROM INET-ADDRESS-MIB           -- [RFC3291]
   MODULE-COMPLIANCE, OBJECT-GROUP,
   NOTIFICATION-GROUP
       FROM SNMPv2-CONF                -- [RFC2580]
   ZeroBasedCounter32
       FROM RMON2-MIB;                 -- [RFC2021]

  alarmMIB MODULE-IDENTITY
      LAST-UPDATED "200409090000Z"  -- September 09, 2004
      ORGANIZATION "IETF Distributed Management Working Group"
      CONTACT-INFO
           "WG EMail: disman@ietf.org
           Subscribe: disman-request@ietf.org
           http://www.ietf.org/html.charters/disman-charter.html
           Chair:     Randy Presuhn
                      randy_presuhn@mindspring.com

           Editors:   Sharon Chisholm
                      Nortel Networks
                      PO Box 3511 Station C
                      Ottawa, Ont.  K1Y 4H7
                      Canada
                      schishol@nortelnetworks.com

                      Dan Romascanu
                      Avaya
                      Atidim Technology Park, Bldg. #3
                      Tel Aviv, 61131
                      Israel
                      Tel: +972-3-645-8414
                      Email: dromasca@avaya.com"
      DESCRIPTION
           "The MIB module describes a generic solution
           to model alarms and to store the current list
           of active alarms.

           Copyright (C) The Internet Society (2004).  The
           initial version of this MIB module was published
           in RFC 3877.  For full legal notices see the RFC
           itself.  Supplementary information may be available on:
           http://www.ietf.org/copyrights/ianamib.html"
      REVISION    "200409090000Z"  -- September 09, 2004
      DESCRIPTION
          "Initial version, published as RFC 3877."
      ::= { mib-2 118 }

alarmObjects OBJECT IDENTIFIER ::= { alarmMIB 1 }

alarmNotifications OBJECT IDENTIFIER ::= { alarmMIB 0 }

alarmModel OBJECT IDENTIFIER ::= { alarmObjects 1 }

alarmActive  OBJECT IDENTIFIER ::= { alarmObjects 2 }

alarmClear OBJECT IDENTIFIER ::= { alarmObjects 3 }

-- Textual Conventions

 -- ResourceId is intended to be a general textual convention
 -- that can be used outside of the set of MIBs related to
 -- Alarm Management.

ResourceId ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
            "A unique identifier for this resource.

            The type of the resource can be determined by looking
            at the OID that describes the resource.

            Resources must be identified in a consistent manner.
            For example, if this resource is an interface, this
            object MUST point to an ifIndex and if this resource
            is a physical entity [RFC2737], then this MUST point
            to an entPhysicalDescr, given that entPhysicalIndex
            is not accessible.  In general, the value is the
            name of the instance of the first accessible columnar
            object in the conceptual row of a table that is
            meaningful for this resource type, which SHOULD
            be defined in an IETF standard MIB."
    SYNTAX         OBJECT IDENTIFIER

 -- LocalSnmpEngineOrZeroLenStr is intended to be a general
 -- textual convention that can be used outside of the set of
 -- MIBs related to Alarm Management.

  LocalSnmpEngineOrZeroLenStr ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "An SNMP Engine ID or a zero-length string.  The
           instantiation of this textual convention will provide
           guidance on when this will be an SNMP Engine ID and
           when it will be a zero lengths string"
      SYNTAX         OCTET STRING (SIZE(0 | 5..32))

-- Alarm Model

alarmModelLastChanged  OBJECT-TYPE
      SYNTAX      TimeTicks
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The value of sysUpTime at the time of the last
         creation, deletion or modification of an entry in
         the alarmModelTable.

         If the number and content of entries has been unchanged
         since the last re-initialization of the local network
         management subsystem, then the value of this object
         MUST be zero."
      ::= { alarmModel 1 }

alarmModelTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF AlarmModelEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "A table of information about possible alarms on the system,
        and how they have been modelled."
   ::= { alarmModel 2 }

alarmModelEntry OBJECT-TYPE
   SYNTAX      AlarmModelEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "Entries appear in this table for each possible alarm state.
       This table MUST be persistent across system reboots."
   INDEX       { alarmListName, alarmModelIndex, alarmModelState }
   ::= { alarmModelTable 1 }

AlarmModelEntry ::= SEQUENCE {
   alarmModelIndex                 Unsigned32,
   alarmModelState                 Unsigned32,
   alarmModelNotificationId        OBJECT IDENTIFIER,
   alarmModelVarbindIndex          Unsigned32,
   alarmModelVarbindValue          Integer32,
   alarmModelDescription           SnmpAdminString,
   alarmModelSpecificPointer       RowPointer,
   alarmModelVarbindSubtree        OBJECT IDENTIFIER,
   alarmModelResourcePrefix        OBJECT IDENTIFIER,
   alarmModelRowStatus             RowStatus
   }

alarmModelIndex OBJECT-TYPE
   SYNTAX     Unsigned32 (1..4294967295)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "An integer that acts as an alarm Id
       to uniquely identify each alarm
       within the named alarm list. "
   ::= { alarmModelEntry 1 }

alarmModelState OBJECT-TYPE
   SYNTAX  Unsigned32 (1..4294967295)
   MAX-ACCESS not-accessible
   STATUS       current
   DESCRIPTION
        "A value of 1 MUST indicate a clear alarm state.
        The value of this object MUST be less than the
        alarmModelState of more severe alarm states for
        this alarm.  The value of this object MUST be more
        than the alarmModelState of less severe alarm states
        for this alarm."
    ::= { alarmModelEntry 2 }

alarmModelNotificationId OBJECT-TYPE
   SYNTAX      OBJECT IDENTIFIER
   MAX-ACCESS  read-create
   STATUS      current
   DESCRIPTION
       "The NOTIFICATION-TYPE object identifier of this alarm
       state transition.  If there is no notification associated
       with this alarm state, the value of this object MUST be
       '0.0'"
   DEFVAL { zeroDotZero }
   ::= { alarmModelEntry 3 }

alarmModelVarbindIndex  OBJECT-TYPE
   SYNTAX  Unsigned32
   MAX-ACCESS   read-create
   STATUS       current
   DESCRIPTION
     "The index into the varbind listing of the notification
     indicated by alarmModelNotificationId which helps
     signal that the given alarm has changed state.
     If there is no applicable varbind, the value of this
     object MUST be zero.

     Note that the value of alarmModelVarbindIndex acknowledges
     the existence of the first two obligatory varbinds in
     the InformRequest-PDU and SNMPv2-Trap-PDU (sysUpTime.0
     and snmpTrapOID.0).  That is, a value of 2 refers to
     the snmpTrapOID.0.

     If the incoming notification is instead an SNMPv1 Trap-PDU,
     then an appropriate value for sysUpTime.0 or snmpTrapOID.0
     shall be determined by using the rules in section 3.1 of
     [RFC3584]"
     DEFVAL { 0 }
    ::= { alarmModelEntry 4 }

alarmModelVarbindValue OBJECT-TYPE
   SYNTAX  Integer32
   MAX-ACCESS   read-create
   STATUS       current
   DESCRIPTION
     "The value that the varbind indicated by
     alarmModelVarbindIndex takes to indicate
     that the alarm has entered this state.

     If alarmModelVarbindIndex has a value of 0, so
     MUST alarmModelVarbindValue.
     "
     DEFVAL { 0 }
    ::= { alarmModelEntry 5 }

alarmModelDescription OBJECT-TYPE
    SYNTAX SnmpAdminString
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
      "A brief description of this alarm and state suitable
      to display to operators."
   DEFVAL { "" }
   ::= { alarmModelEntry 6 }

alarmModelSpecificPointer OBJECT-TYPE
   SYNTAX     RowPointer
   MAX-ACCESS read-create
   STATUS     current
   DESCRIPTION
     "If no additional, model-specific Alarm MIB is supported by
      the system the value of this object is `0.0'and attempts
      to set it to any other value MUST be rejected appropriately.

      When a model-specific Alarm MIB is supported, this object
      MUST refer to the first accessible object in a corresponding
      row of the model definition in one of these model-specific
      MIB and attempts to set this object to { 0 0 } or any other
      value MUST be rejected appropriately."
   DEFVAL { zeroDotZero }
   ::= { alarmModelEntry 7 }

  alarmModelVarbindSubtree  OBJECT-TYPE
     SYNTAX  OBJECT IDENTIFIER
     MAX-ACCESS   read-create
     STATUS       current
     DESCRIPTION
       "The name portion of each VarBind in the notification,
        in order, is compared to the value of this object.
        If the name is equal to or a subtree of the value
        of this object, for purposes of computing the value
        of AlarmActiveResourceID the 'prefix' will be the
        matching portion, and the 'indexes' will be any
        remainder.  The examination of varbinds ends with
        the first match.  If the value of this object is 0.0,
        then the first varbind, or in the case of v2, the
        first varbind after the timestamp and the trap
        OID, will always be matched.
       "
      DEFVAL { zeroDotZero }
     ::= { alarmModelEntry 8 }

  alarmModelResourcePrefix  OBJECT-TYPE
     SYNTAX  OBJECT IDENTIFIER
     MAX-ACCESS   read-create
     STATUS       current
     DESCRIPTION
       "The value of AlarmActiveResourceId is computed
        by appending any indexes extracted in accordance
        with the description of alarmModelVarbindSubtree
        onto the value of this object.  If this object's
        value is 0.0, then the 'prefix' extracted is used
        instead.
       "
     DEFVAL { zeroDotZero }
     ::= { alarmModelEntry 9 }

alarmModelRowStatus OBJECT-TYPE
   SYNTAX     RowStatus
   MAX-ACCESS read-create
   STATUS     current
   DESCRIPTION
    "Control for creating and deleting entries.  Entries may be
    modified while active.  Alarms whose alarmModelRowStatus is
    not active will not appear in either the alarmActiveTable
    or the alarmClearTable.  Setting this object to notInService
    cannot be used as an alarm suppression mechanism.  Entries
    that are notInService will disappear as described in RFC2579.

    This row can not be modified while it is being
    referenced by a value of alarmActiveModelPointer.  In these
    cases, an error of `inconsistentValue' will be returned to
    the manager.

    This entry may be deleted while it is being
    referenced by a value of alarmActiveModelPointer.  This results
    in the deletion of this entry and entries in the active alarms
    referencing this entry via an alarmActiveModelPointer.
    As all read-create objects in this table have a DEFVAL clause,
    there is no requirement that any object be explicitly set
    before this row can become active.  Note that a row consisting
    only of default values is not very meaningful."
   ::= { alarmModelEntry 10 }

-- Active Alarm Table --

alarmActiveLastChanged  OBJECT-TYPE
   SYNTAX      TimeTicks
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The value of sysUpTime at the time of the last
       creation or deletion of an entry in the alarmActiveTable.
       If the number of entries has been unchanged since the
       last re-initialization of the local network management
       subsystem, then this object contains a zero value."
   ::= { alarmActive 1 }

 alarmActiveOverflow  OBJECT-TYPE
     SYNTAX      Counter32
     UNITS       "active alarms"
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "The number of active alarms that have not been put into
         the alarmActiveTable since system restart as a result
         of extreme resource constraints."
     ::= { alarmActive 5 }

alarmActiveTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF AlarmActiveEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "A table of Active Alarms entries."
   ::= { alarmActive 2 }

alarmActiveEntry OBJECT-TYPE
   SYNTAX      AlarmActiveEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "Entries appear in this table when alarms are raised.  They
        are removed when the alarm is cleared.

        If under extreme resource constraint the system is unable to
        add any more entries into this table, then the
        alarmActiveOverflow statistic will be increased by one."
   INDEX       { alarmListName, alarmActiveDateAndTime,
                 alarmActiveIndex }
   ::= { alarmActiveTable 1 }

AlarmActiveEntry ::= SEQUENCE {
   alarmListName                    SnmpAdminString,
   alarmActiveDateAndTime           DateAndTime,
   alarmActiveIndex                 Unsigned32,
   alarmActiveEngineID              LocalSnmpEngineOrZeroLenStr,
   alarmActiveEngineAddressType     InetAddressType,
   alarmActiveEngineAddress         InetAddress,
   alarmActiveContextName           SnmpAdminString,
   alarmActiveVariables             Unsigned32,
   alarmActiveNotificationID        OBJECT IDENTIFIER,
   alarmActiveResourceId            ResourceId,
   alarmActiveDescription           SnmpAdminString,
   alarmActiveLogPointer            RowPointer,
   alarmActiveModelPointer          RowPointer,
   alarmActiveSpecificPointer       RowPointer }

alarmListName OBJECT-TYPE
   SYNTAX     SnmpAdminString (SIZE(0..32))
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
    "The name of the list of alarms.  This SHOULD be the same as
    nlmLogName if the Notification Log MIB [RFC3014] is supported.
    This SHOULD be the same as, or contain as a prefix, the
    applicable snmpNotifyFilterProfileName if the
    SNMP-NOTIFICATION-MIB DEFINITIONS [RFC3413] is supported.

    An implementation may allow multiple named alarm lists, up to
    some implementation-specific limit (which may be none).  A
    zero-length list name is reserved for creation and deletion
    by the managed system, and MUST be used as the default log
    name by systems that do not support named alarm lists."
   ::= { alarmActiveEntry 1 }

alarmActiveDateAndTime OBJECT-TYPE
   SYNTAX      DateAndTime
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "The local date and time when the error occurred.

       This object facilitates retrieving all instances of
       alarms that have been raised or have changed state
       since a given point in time.

       Implementations MUST include the offset from UTC,
       if available.  Implementation in environments in which
       the UTC offset is not available is NOT RECOMMENDED."
   ::= { alarmActiveEntry 2 }

alarmActiveIndex OBJECT-TYPE
   SYNTAX     Unsigned32 (1..4294967295)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "A strictly monotonically increasing integer which
       acts as the index of entries within the named alarm
       list.  It wraps back to 1 after it reaches its
       maximum value."
   ::= { alarmActiveEntry 3 }

alarmActiveEngineID OBJECT-TYPE
   SYNTAX      LocalSnmpEngineOrZeroLenStr
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The identification of the SNMP engine at which the alarm
        originated.  If the alarm is from an SNMPv1 system this
        object is a zero length string."
   ::= { alarmActiveEntry 4 }

alarmActiveEngineAddressType OBJECT-TYPE
   SYNTAX      InetAddressType
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
    "This object indicates what type of address is stored in
    the alarmActiveEngineAddress object - IPv4, IPv6, DNS, etc."
   ::= { alarmActiveEntry 5 }

alarmActiveEngineAddress OBJECT-TYPE
   SYNTAX      InetAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
    "The address of the SNMP engine on which the alarm is
    occurring.

    This object MUST always be instantiated, even if the list
    can contain alarms from only one engine."
   ::= { alarmActiveEntry 6 }

alarmActiveContextName OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The name of the SNMP MIB context from which the alarm came.
        For SNMPv1 alarms this is the community string from the Trap.
        Note that care MUST be taken when selecting community
        strings to ensure that these can be represented as a
        well-formed SnmpAdminString.  Community or Context names
        that are not well-formed SnmpAdminStrings will be mapped
        to zero length strings.

        If the alarm's source SNMP engine is known not to support
        multiple contexts, this object is a zero length string."
   ::= { alarmActiveEntry 7 }

alarmActiveVariables OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The number of variables in alarmActiveVariableTable for this
       alarm."
   ::= { alarmActiveEntry 8 }

alarmActiveNotificationID OBJECT-TYPE
   SYNTAX      OBJECT IDENTIFIER
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The NOTIFICATION-TYPE object identifier of the alarm
       state transition that is occurring."
   ::= { alarmActiveEntry 9 }

alarmActiveResourceId    OBJECT-TYPE
   SYNTAX      ResourceId
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This object identifies the resource under alarm.

      If there is no corresponding resource, then
      the value of this object MUST be 0.0."
   ::= { alarmActiveEntry 10 }

alarmActiveDescription    OBJECT-TYPE
   SYNTAX      SnmpAdminString
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This object provides a textual description of the
      active alarm.  This text is generated dynamically by the
      notification generator to provide useful information
      to the human operator.  This information SHOULD
      provide information allowing the operator to locate
      the resource for which this alarm is being generated.
      This information is not intended for consumption by
      automated tools."
   ::= { alarmActiveEntry 11 }

alarmActiveLogPointer OBJECT-TYPE
   SYNTAX     RowPointer
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "A pointer to the corresponding row in a
       notification logging MIB where the state change
       notification for this active alarm is logged.
       If no log entry applies to this active alarm,
       then this object MUST have the value of 0.0"
   ::= { alarmActiveEntry 12 }

alarmActiveModelPointer OBJECT-TYPE
   SYNTAX     RowPointer
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "A pointer to the corresponding row in the
       alarmModelTable for this active alarm.  This
       points not only to the alarm model being
       instantiated, but also to the specific alarm
       state that is active."
   ::= { alarmActiveEntry 13 }

alarmActiveSpecificPointer OBJECT-TYPE
   SYNTAX     RowPointer
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
     "If no additional, model-specific, Alarm MIB is supported by
     the system this object is `0.0'.  When a model-specific Alarm
     MIB is supported, this object is the instance pointer to the
     specific model-specific active alarm list."
   ::= { alarmActiveEntry 14 }

-- Active Alarm Variable Table --

alarmActiveVariableTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF AlarmActiveVariableEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "A table of variables to go with active alarm entries."
   ::= { alarmActive 3 }

alarmActiveVariableEntry OBJECT-TYPE
   SYNTAX      AlarmActiveVariableEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "Entries appear in this table when there are variables in
       the varbind list of a corresponding alarm in
       alarmActiveTable.

       Entries appear in this table as though
       the trap/notification had been transported using a
       SNMPv2-Trap-PDU, as defined in [RFC3416] - i.e., the
       alarmActiveVariableIndex 1 will always be sysUpTime
       and alarmActiveVariableIndex 2 will always be
       snmpTrapOID.

       If the incoming notification is instead an SNMPv1 Trap-PDU and
       the value of alarmModelVarbindIndex is 1 or 2, an appropriate
       value for sysUpTime.0 or snmpTrapOID.0 shall be determined
       by using the rules in section 3.1 of [RFC3584]."
   INDEX   {  alarmListName, alarmActiveIndex,
              alarmActiveVariableIndex }
   ::= { alarmActiveVariableTable 1 }

AlarmActiveVariableEntry ::= SEQUENCE {
   alarmActiveVariableIndex                 Unsigned32,
   alarmActiveVariableID                    OBJECT IDENTIFIER,
   alarmActiveVariableValueType             INTEGER,
   alarmActiveVariableCounter32Val          Counter32,
   alarmActiveVariableUnsigned32Val         Unsigned32,
   alarmActiveVariableTimeTicksVal          TimeTicks,
   alarmActiveVariableInteger32Val          Integer32,
   alarmActiveVariableOctetStringVal        OCTET STRING,
   alarmActiveVariableIpAddressVal          IpAddress,
   alarmActiveVariableOidVal                OBJECT IDENTIFIER,
   alarmActiveVariableCounter64Val          Counter64,
   alarmActiveVariableOpaqueVal             Opaque }

alarmActiveVariableIndex OBJECT-TYPE
   SYNTAX     Unsigned32 (1..4294967295)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "A strictly monotonically increasing integer, starting at
       1 for a given alarmActiveIndex, for indexing variables
       within the active alarm variable list. "
   ::= { alarmActiveVariableEntry 1 }

alarmActiveVariableID OBJECT-TYPE
   SYNTAX     OBJECT IDENTIFIER
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "The alarm variable's object identifier."
   ::= { alarmActiveVariableEntry 2 }

alarmActiveVariableValueType OBJECT-TYPE
   SYNTAX      INTEGER {
         counter32(1),
         unsigned32(2),
         timeTicks(3),
         integer32(4),
         ipAddress(5),
         octetString(6),
         objectId(7),
         counter64(8),
         opaque(9)
         }
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The type of the value.  One and only one of the value
       objects that follow is used for a given row in this table,
       based on this type."
   ::= { alarmActiveVariableEntry 3 }

alarmActiveVariableCounter32Val OBJECT-TYPE
   SYNTAX      Counter32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'counter32'."
   ::= { alarmActiveVariableEntry 4 }

alarmActiveVariableUnsigned32Val OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'unsigned32'."
   ::= { alarmActiveVariableEntry 5 }

alarmActiveVariableTimeTicksVal OBJECT-TYPE
   SYNTAX      TimeTicks
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'timeTicks'."
   ::= { alarmActiveVariableEntry 6 }

alarmActiveVariableInteger32Val OBJECT-TYPE
   SYNTAX      Integer32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'integer32'."
   ::= { alarmActiveVariableEntry 7 }

alarmActiveVariableOctetStringVal OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..65535))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'octetString'."
   ::= { alarmActiveVariableEntry 8 }

alarmActiveVariableIpAddressVal OBJECT-TYPE
   SYNTAX      IpAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'ipAddress'."
   ::= { alarmActiveVariableEntry 9 }

alarmActiveVariableOidVal OBJECT-TYPE
   SYNTAX      OBJECT IDENTIFIER
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'objectId'."
   ::= { alarmActiveVariableEntry 10 }

alarmActiveVariableCounter64Val OBJECT-TYPE
   SYNTAX      Counter64
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'counter64'."
   ::= { alarmActiveVariableEntry 11 }

alarmActiveVariableOpaqueVal OBJECT-TYPE
   SYNTAX      Opaque (SIZE(0..65535))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The value when alarmActiveVariableType is 'opaque'.

       Note that although RFC2578 [RFC2578] forbids the use
       of Opaque in 'standard' MIB modules, this particular
       usage is driven by the need to be able to accurately
       represent any well-formed notification, and justified
       by the need for backward compatibility."
   ::= { alarmActiveVariableEntry 12 }

-- Statistics --

alarmActiveStatsTable  OBJECT-TYPE
      SYNTAX  SEQUENCE OF AlarmActiveStatsEntry
      MAX-ACCESS  not-accessible
      STATUS  current
      DESCRIPTION
         "This table represents the alarm statistics
         information."
  ::= { alarmActive 4 }

alarmActiveStatsEntry OBJECT-TYPE
      SYNTAX  AlarmActiveStatsEntry
      MAX-ACCESS  not-accessible
      STATUS  current
      DESCRIPTION
         "Statistics on the current active alarms."
      INDEX   { alarmListName }

  ::= {  alarmActiveStatsTable 1 }

AlarmActiveStatsEntry ::=
      SEQUENCE {
           alarmActiveStatsActiveCurrent  Gauge32,
           alarmActiveStatsActives        ZeroBasedCounter32,
           alarmActiveStatsLastRaise      TimeTicks,
           alarmActiveStatsLastClear      TimeTicks
                }

alarmActiveStatsActiveCurrent OBJECT-TYPE
      SYNTAX Gauge32
      MAX-ACCESS read-only
      STATUS  current
      DESCRIPTION
         "The total number of currently active alarms on the system."
       ::= { alarmActiveStatsEntry 1 }

alarmActiveStatsActives OBJECT-TYPE
      SYNTAX ZeroBasedCounter32
      MAX-ACCESS read-only
      STATUS  current
      DESCRIPTION
         "The total number of active alarms since system restarted."
       ::= { alarmActiveStatsEntry 2 }

alarmActiveStatsLastRaise  OBJECT-TYPE
   SYNTAX      TimeTicks
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The value of sysUpTime at the time of the last
       alarm raise for this alarm list.
       If no alarm raises have occurred since the
       last re-initialization of the local network management
       subsystem, then this object contains a zero value."
 ::= { alarmActiveStatsEntry 3 }

alarmActiveStatsLastClear  OBJECT-TYPE
   SYNTAX      TimeTicks
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "The value of sysUpTime at the time of the last
       alarm clear for this alarm list.
       If no alarm clears have occurred since the
       last re-initialization of the local network management
       subsystem, then this object contains a zero value."
 ::= { alarmActiveStatsEntry 4 }

-- Alarm Clear

alarmClearMaximum OBJECT-TYPE
 SYNTAX Unsigned32
 MAX-ACCESS read-write
 STATUS current
 DESCRIPTION
   "This object specifies the maximum number of cleared
   alarms to store in the alarmClearTable.  When this
   number is reached, the cleared alarms with the
   earliest clear time will be removed from the table."
 ::= { alarmClear 1 }

alarmClearTable  OBJECT-TYPE
      SYNTAX  SEQUENCE OF AlarmClearEntry
      MAX-ACCESS  not-accessible
      STATUS  current
      DESCRIPTION
         "This table contains information on
         cleared alarms."
  ::= { alarmClear 2 }

alarmClearEntry OBJECT-TYPE
      SYNTAX  AlarmClearEntry
      MAX-ACCESS  not-accessible
      STATUS  current
      DESCRIPTION
         "Information on a cleared alarm."
      INDEX   { alarmListName, alarmClearDateAndTime,
alarmClearIndex }

  ::= {  alarmClearTable 1 }

AlarmClearEntry ::=
      SEQUENCE {
   alarmClearIndex                 Unsigned32,
   alarmClearDateAndTime           DateAndTime,
   alarmClearEngineID              LocalSnmpEngineOrZeroLenStr,
   alarmClearEngineAddressType     InetAddressType,
   alarmClearEngineAddress         InetAddress,
   alarmClearContextName           SnmpAdminString,
   alarmClearNotificationID        OBJECT IDENTIFIER,
   alarmClearResourceId            ResourceId,
   alarmClearLogIndex              Unsigned32,
   alarmClearModelPointer          RowPointer
   }

alarmClearIndex OBJECT-TYPE
   SYNTAX     Unsigned32 (1..4294967295)
   MAX-ACCESS not-accessible
   STATUS     current
   DESCRIPTION
       "An integer which acts as the index of entries within
       the named alarm list.  It wraps back to 1 after it
       reaches its maximum value.

       This object has the same value as the alarmActiveIndex that
       this alarm instance had when it was active."
   ::= { alarmClearEntry 1 }

alarmClearDateAndTime OBJECT-TYPE
   SYNTAX      DateAndTime
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
       "The local date and time when the alarm cleared.

       This object facilitates retrieving all instances of
       alarms that have been cleared since a given point in time.

       Implementations MUST include the offset from UTC,
       if available.  Implementation in environments in which
       the UTC offset is not available is NOT RECOMMENDED."
   ::= { alarmClearEntry 2 }

alarmClearEngineID OBJECT-TYPE
   SYNTAX      LocalSnmpEngineOrZeroLenStr
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The identification of the SNMP engine at which the alarm
        originated.  If the alarm is from an SNMPv1 system this
        object is a zero length string."
   ::= { alarmClearEntry 3 }

alarmClearEngineAddressType OBJECT-TYPE
   SYNTAX      InetAddressType
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
    "This object indicates what type of address is stored in
    the alarmActiveEngineAddress object - IPv4, IPv6, DNS, etc."
   ::= { alarmClearEntry 4 }

alarmClearEngineAddress OBJECT-TYPE
   SYNTAX      InetAddress
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
    "The Address of the SNMP engine on which the alarm was
    occurring.  This is used to identify the source of an SNMPv1
    trap, since an alarmActiveEngineId cannot be extracted from the
    SNMPv1 trap PDU.

    This object MUST always be instantiated, even if the list
    can contain alarms from only one engine."
   ::= { alarmClearEntry 5 }

alarmClearContextName OBJECT-TYPE
   SYNTAX      SnmpAdminString (SIZE(0..32))
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The name of the SNMP MIB context from which the alarm came.
       For SNMPv1 traps this is the community string from the Trap.
       Note that care needs to be taken when selecting community
       strings to ensure that these can be represented as a
       well-formed SnmpAdminString.  Community or Context names
       that are not well-formed SnmpAdminStrings will be mapped
       to zero length strings.

       If the alarm's source SNMP engine is known not to support
       multiple contexts, this object is a zero length string."
   ::= { alarmClearEntry 6 }

alarmClearNotificationID OBJECT-TYPE
   SYNTAX      OBJECT IDENTIFIER
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
       "The NOTIFICATION-TYPE object identifier of the alarm
       clear."
   ::= { alarmClearEntry 7 }

alarmClearResourceId    OBJECT-TYPE
   SYNTAX      ResourceId
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
      "This object identifies the resource that was under alarm.

      If there is no corresponding resource, then
      the value of this object MUST be 0.0."
   ::= { alarmClearEntry 8 }

alarmClearLogIndex OBJECT-TYPE
   SYNTAX     Unsigned32 (0..4294967295)
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "This number MUST be the same as the log index of the
       applicable row in the notification log MIB, if it exists.
       If no log index applies to the trap, then this object
       MUST have the value of 0."
   ::= { alarmClearEntry 9 }

alarmClearModelPointer OBJECT-TYPE
   SYNTAX     RowPointer
   MAX-ACCESS read-only
   STATUS     current
   DESCRIPTION
       "A pointer to the corresponding row in the
       alarmModelTable for this cleared alarm."
   ::= { alarmClearEntry 10 }

-- Notifications

alarmActiveState NOTIFICATION-TYPE
 OBJECTS     { alarmActiveModelPointer,
               alarmActiveResourceId }
 STATUS      current
 DESCRIPTION
    "An instance of the alarm indicated by
    alarmActiveModelPointer has been raised
    against the entity indicated by
    alarmActiveResourceId.

    The agent must throttle the generation of
    consecutive alarmActiveState traps so that there is at
    least a two-second gap between traps of this
    type against the same alarmActiveModelPointer and
    alarmActiveResourceId.  When traps are throttled,
    they are dropped, not queued for sending at a future time.

    A management application should periodically check
    the value of alarmActiveLastChanged to detect any
    missed alarmActiveState notification-events, e.g.,
    due to throttling or transmission loss."
 ::= { alarmNotifications 2 }

alarmClearState NOTIFICATION-TYPE
   OBJECTS     { alarmActiveModelPointer,
                 alarmActiveResourceId }
   STATUS      current
   DESCRIPTION
     "An instance of the alarm indicated by
     alarmActiveModelPointer has been cleared against
     the entity indicated by alarmActiveResourceId.

    The agent must throttle the generation of
    consecutive alarmActiveClear traps so that there is at
    least a two-second gap between traps of this
    type against the same alarmActiveModelPointer and
    alarmActiveResourceId.  When traps are throttled,
    they are dropped, not queued for sending at a future time.

    A management application should periodically check
    the value of alarmActiveLastChanged to detect any
    missed alarmClearState notification-events, e.g.,
    due to throttling or transmission loss."
   ::= { alarmNotifications 3 }

-- Conformance

alarmConformance OBJECT IDENTIFIER ::= { alarmMIB 2 }

alarmCompliances OBJECT IDENTIFIER ::= { alarmConformance 1 }

alarmCompliance MODULE-COMPLIANCE
      STATUS  current
      DESCRIPTION
          "The compliance statement for systems supporting
          the Alarm MIB."
      MODULE -- this module
          MANDATORY-GROUPS {
           alarmActiveGroup,
           alarmModelGroup
          }
      GROUP       alarmActiveStatsGroup
       DESCRIPTION
           "This group is optional."
      GROUP       alarmClearGroup
       DESCRIPTION
           "This group is optional."
      GROUP       alarmNotificationsGroup
       DESCRIPTION
           "This group is optional."
   ::= { alarmCompliances 1 }

alarmGroups OBJECT IDENTIFIER ::= { alarmConformance 2 }

alarmModelGroup OBJECT-GROUP
   OBJECTS {
       alarmModelLastChanged,
       alarmModelNotificationId,
       alarmModelVarbindIndex,
       alarmModelVarbindValue,
       alarmModelDescription,
       alarmModelSpecificPointer,
       alarmModelVarbindSubtree,
       alarmModelResourcePrefix,
       alarmModelRowStatus
      }
    STATUS   current
    DESCRIPTION
               "Alarm model group."
    ::= { alarmGroups 1}

alarmActiveGroup OBJECT-GROUP
        OBJECTS {
           alarmActiveLastChanged,
           alarmActiveOverflow,
           alarmActiveEngineID,
           alarmActiveEngineAddressType,
           alarmActiveEngineAddress,
           alarmActiveContextName,
           alarmActiveVariables,
           alarmActiveNotificationID,
           alarmActiveResourceId,
           alarmActiveDescription,
           alarmActiveLogPointer,
           alarmActiveModelPointer,
           alarmActiveSpecificPointer,
           alarmActiveVariableID,
           alarmActiveVariableValueType,
           alarmActiveVariableCounter32Val,
           alarmActiveVariableUnsigned32Val,
           alarmActiveVariableTimeTicksVal,
           alarmActiveVariableInteger32Val,
           alarmActiveVariableOctetStringVal,
           alarmActiveVariableIpAddressVal,
           alarmActiveVariableOidVal,
           alarmActiveVariableCounter64Val,
           alarmActiveVariableOpaqueVal
          }
          STATUS   current
          DESCRIPTION
               "Active Alarm list group."
          ::= { alarmGroups 2}

    alarmActiveStatsGroup  OBJECT-GROUP
          OBJECTS  {
                   alarmActiveStatsActives,
                   alarmActiveStatsActiveCurrent,
                   alarmActiveStatsLastRaise,
                   alarmActiveStatsLastClear
                    }
          STATUS   current
          DESCRIPTION
               "Active alarm summary group."
          ::= { alarmGroups 3}

alarmClearGroup  OBJECT-GROUP
          OBJECTS  {
   alarmClearMaximum,
   alarmClearEngineID,
   alarmClearEngineAddressType,
   alarmClearEngineAddress,
   alarmClearContextName,
   alarmClearNotificationID,
   alarmClearResourceId,
   alarmClearLogIndex,
   alarmClearModelPointer
                    }
          STATUS   current
          DESCRIPTION
               "Cleared alarm group."
          ::= { alarmGroups 4}

alarmNotificationsGroup NOTIFICATION-GROUP
   NOTIFICATIONS { alarmActiveState, alarmClearState }
   STATUS        current
   DESCRIPTION
           "The collection of notifications that can be used to
           model alarms for faults lacking pre-existing
           notification definitions."
   ::= { alarmGroups 6 }

END

-- 
--    Copyright (C) The Internet Society (2004).  This document is subject
--    to the rights, licenses and restrictions contained in BCP 78, and
--    except as set forth therein, the authors retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 

