-- extracted from rfc4404.txt
-- at Thu Feb 23 06:15:12 2006

   FCIP-MGMT-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       OBJECT-TYPE,
       MODULE-IDENTITY,
       Unsigned32,
       Counter32,
       mib-2               FROM SNMPv2-SMI
       TEXTUAL-CONVENTION,
       TruthValue, RowStatus, TimeStamp  FROM SNMPv2-TC
       InetAddressType,
       InetAddress,
       InetPortNumber FROM INET-ADDRESS-MIB
       FcNameIdOrZero FROM FC-MGMT-MIB
       InterfaceIndex FROM IF-MIB
       MODULE-COMPLIANCE,
       OBJECT-GROUP FROM SNMPv2-CONF
       SnmpAdminString FROM SNMP-FRAMEWORK-MIB;

   fcipMIB MODULE-IDENTITY
       LAST-UPDATED "200602060000Z"
       ORGANIZATION "IETF IPFC Working Group"
       CONTACT-INFO "Anil Rijhsinghani
                     Accton Technology Corporation
                     5 Mount Royal Ave
                     Marlboro, MA 01752 USA.
                     Ravi Natarajan
                     F5 Networks
                     2460 North First Street, Suite 100
                     San Jose, CA 95131 USA."
       DESCRIPTION
           "The module defines management information specific to
            FCIP devices.

            Copyright(C) The Internet Society (2006).  This version
            of this MIB module is part of RFC 4404; see the RFC
            itself for full legal notices."
       REVISION        "200602060000Z"
       DESCRIPTION
           "Initial version of this module, published as RFC 4404."
       ::= { mib-2 224 }

   fcipObjects       OBJECT IDENTIFIER ::= { fcipMIB 1 }
   fcipConformance   OBJECT IDENTIFIER ::= { fcipMIB 2 }
   fcipConfig        OBJECT IDENTIFIER ::= { fcipObjects 1 }


   -- ******************************************************************
   -- Textual conventions
   --

   FcipDomainIdInOctetForm ::= TEXTUAL-CONVENTION
       STATUS    current
       DESCRIPTION
           "The Domain ID of a FC entity in octet form
            to support the concatenation(000000h||Domain_ID)
            format defined in the FSPF routing protocol."
       REFERENCE
           "FC-SW-3 section 4.8"
       SYNTAX    OCTET STRING (SIZE(1))

   FcipEntityMode ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "The type of port mode provided by an FCIP Entity
            for an FCIP Link.  An FCIP Entity can be an E-Port
            mode for one of its FCIP Link Endpoints or a B-Port
            mode for another of its FCIP Link Endpoints."
       REFERENCE
           "FC-BB, rev 4.7, 2 May 1997, section 3."
       SYNTAX INTEGER {
                   ePortMode(1),
                   bPortMode(2)
                      }

   FcipEntityId  ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "The FCIP entity identifier as defined in RFC 3821."
       REFERENCE
           "RFC 3821, Section 7.1, FCIP Special Frame Format"
       SYNTAX OCTET STRING (SIZE(8))


   -- ******************************************************************
   -- The FCIP group
   --
   -- This group defines the global scalar objects applicable to FCIP
   -- devices only
   --

   fcipDynIpConfType   OBJECT-TYPE
       SYNTAX INTEGER {
                   slpv2(1),
                   none(2)
       }
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The type of discovery protocol used to discover remote
            FCIP entities.  The value of this object is persistent
            across system restarts."
       ::= { fcipConfig 1 }

   fcipDeviceWWN   OBJECT-TYPE
       SYNTAX FcNameIdOrZero
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The World Wide Name of this FCIP device."
       ::= { fcipConfig 2 }

   fcipEntitySACKOption   OBJECT-TYPE
       SYNTAX INTEGER {
                   enabled(1),
                   disabled(2)
       }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Indication of whether the TCP Selective Acknowledgement
            Option is enabled at this FCIP device to let the receiver
            acknowledge multiple lost packets in a single ACK for faster
            recovery."
       REFERENCE
           "The Selective Ack option is defined in RFC 2883."
       ::= { fcipConfig 3 }


   -- ******************************************************************
   -- The FCIP Entity Table
   --

   fcipEntityInstanceTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipEntityInstanceEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about this FCIP device's existing instances of
            FCIP entities."
       REFERENCE
           "RFC 3821, Section 5.4, FCIP Entity"
       ::= { fcipConfig 4 }

   fcipEntityInstanceEntry OBJECT-TYPE
       SYNTAX FcipEntityInstanceEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP entity table with information
            about a particular FCIP entity.  Once a row has been
            created, it is non-volatile across agent restarts until it
            is deleted."
       INDEX { fcipEntityId }
       ::= { fcipEntityInstanceTable 1 }

   FcipEntityInstanceEntry ::=
       SEQUENCE {
                   fcipEntityId                  FcipEntityId,
                   fcipEntityName                SnmpAdminString,
                   fcipEntityAddressType         InetAddressType,
                   fcipEntityAddress             InetAddress,
                   fcipEntityTcpConnPort         InetPortNumber,
                   fcipEntitySeqNumWrap          TruthValue,
                   fcipEntityPHBSupport          TruthValue,
                   fcipEntityStatus              RowStatus
              }

   fcipEntityId   OBJECT-TYPE
       SYNTAX FcipEntityId
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The FCIP entity identifier."
       REFERENCE
           "RFC 3821, Section 7.1, FCIP Special Frame Format"
       ::= { fcipEntityInstanceEntry 1 }

   fcipEntityName   OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..32))
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "An administratively-assigned name for this FCIP entity."
       ::= { fcipEntityInstanceEntry 2 }

   fcipEntityAddressType   OBJECT-TYPE
       SYNTAX InetAddressType
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The type of Internet address by which the entity is
            reachable.  Only address types IPv4 and IPv6 are supported."
       ::= { fcipEntityInstanceEntry 3 }

   fcipEntityAddress   OBJECT-TYPE
       SYNTAX InetAddress
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The Internet address for the entity, if configured.  The
            format of this address is determined by the value of the
            fcipEntityAddressType object."
       ::= { fcipEntityInstanceEntry 4 }

   fcipEntityTcpConnPort   OBJECT-TYPE
       SYNTAX InetPortNumber
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "A TCP port other than the FCIP Well-Known port on which the
            FCIP entity listens for new TCP connection requests.  It
            contains the value zero(0) if the FCIP Entity only listens
            on the Well-Known port."
       DEFVAL  { 0 }
       ::= { fcipEntityInstanceEntry 5 }

   fcipEntitySeqNumWrap   OBJECT-TYPE
       SYNTAX TruthValue
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "An indication of whether the FCIP Entity supports protection
            against sequence number wrap."
       REFERENCE
           "The PAWS option is defined in RFC 1323."
       ::= { fcipEntityInstanceEntry 6 }

   fcipEntityPHBSupport   OBJECT-TYPE
       SYNTAX TruthValue
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "An indication of whether the FCIP Entity supports PHB IP
            quality of service (QoS)."
       REFERENCE
           "Per hop behavior is defined in RFC 2474, definition of the
            Differentiated Services Field."
       ::= { fcipEntityInstanceEntry 7 }

   fcipEntityStatus   OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS   read-create
       STATUS   current
       DESCRIPTION
           "This object specifies the operational status of the row.

            When a management station sets the status to active(1), then
            the values for the objects fcipEntityName,
            fcipEntityAddressType, and fcipEntityAddress should be
            supplied as part of the set request.  The values of the
            objects fcipEntityName, fcipEntityAddressType, and
            fcipEntityAddress can be changed if the row status is in
            active state.  The object fcipEntityTcpConnPort takes the
            default value zero(0), if no value is supplied at the time
            of row creation.

            Setting the status to destroy(6) deletes the specified FCIP
            entity instance row from the table.  It also deletes all the
            rows corresponding to the specified FCIP entity from the
            fcipLinkTable and fcipTcpConnTable tables."
       ::= { fcipEntityInstanceEntry 8 }

   -- ******************************************************************
   -- The FCIP Link Table
   --

   fcipLinkTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipLinkEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about FCIP links that exist on this device."
       ::= { fcipConfig 5 }

   fcipLinkEntry OBJECT-TYPE
       SYNTAX FcipLinkEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP link table containing
            information about a particular FCIP link.  The values of the
            read-create objects in this table are persistent across
            system restarts."
       INDEX { fcipEntityId, fcipLinkIndex }
       ::= { fcipLinkTable 1 }

   FcipLinkEntry ::=
       SEQUENCE {
                   fcipLinkIndex                       Unsigned32,
                   fcipLinkIfIndex                     InterfaceIndex,
                   fcipLinkCost                        Unsigned32,
                   fcipLinkLocalFcipEntityMode         FcipEntityMode,
                   fcipLinkLocalFcipEntityAddressType  InetAddressType,
                   fcipLinkLocalFcipEntityAddress      InetAddress,
                   fcipLinkRemFcipEntityWWN            FcNameIdOrZero,
                   fcipLinkRemFcipEntityId             FcipEntityId,
                   fcipLinkRemFcipEntityAddressType    InetAddressType,
                   fcipLinkRemFcipEntityAddress        InetAddress,
                   fcipLinkStatus                      RowStatus,
                   fcipLinkCreateTime                  TimeStamp
   }

   fcipLinkIndex     OBJECT-TYPE
       SYNTAX Unsigned32 (1..4294967295)
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "An arbitrary integer that uniquely identifies one FCIP link
            within an FCIP entity."
       ::= { fcipLinkEntry 1 }

   fcipLinkIfIndex     OBJECT-TYPE
       SYNTAX InterfaceIndex
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The ifIndex value of the virtual interface corresponding to
            the FCIP Link running over TCP/IP."
       ::= { fcipLinkEntry 2 }

   fcipLinkCost     OBJECT-TYPE
       SYNTAX Unsigned32
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The FSPF cost associated with this FCIP Link."
       DEFVAL  { 0 }
       ::= { fcipLinkEntry 3 }

   fcipLinkLocalFcipEntityMode   OBJECT-TYPE
       SYNTAX FcipEntityMode
       MAX-ACCESS   read-only
       STATUS   current
       DESCRIPTION
           "The mode of the local end of the FCIP link."
       ::= { fcipLinkEntry 4 }

   fcipLinkLocalFcipEntityAddressType   OBJECT-TYPE
       SYNTAX InetAddressType
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The type of Internet address contained in the corresponding
            instance of fcipLinkLocalFcipEntityAddress.  Only address
            types IPv4 and IPv6 are supported."
       ::= { fcipLinkEntry 5 }

   fcipLinkLocalFcipEntityAddress   OBJECT-TYPE
       SYNTAX InetAddress
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The Internet address for the local end of this FCIP Link.
            The format of this object is determined by the value of the
            fcipLinkLocalFcipEntityAddressType object."
       ::= { fcipLinkEntry 6 }

   fcipLinkRemFcipEntityWWN   OBJECT-TYPE
       SYNTAX FcNameIdOrZero
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The World Wide Name of the remote FC Fabric Entity."
       REFERENCE
           "RFC 3821, Section 7.1, FCIP Special Frame Format"
       ::= { fcipLinkEntry 7 }

   fcipLinkRemFcipEntityId   OBJECT-TYPE
       SYNTAX FcipEntityId
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The remote FCIP entity's identifier."
       REFERENCE
           "RFC 3821, Section 7.1, FCIP Special Frame Format"
       ::= { fcipLinkEntry 8 }

   fcipLinkRemFcipEntityAddressType   OBJECT-TYPE
       SYNTAX InetAddressType
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The type of Internet address contained in the corresponding
            instance of fcipLinkRemFcipEntityAddress.  Only address
            types IPv4 and IPv6 are supported."
       ::= { fcipLinkEntry 9 }

   fcipLinkRemFcipEntityAddress   OBJECT-TYPE
       SYNTAX InetAddress
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The Internet address for the remote end of this FCIP Link.
            The format of this object is determined by the value of the
            fcipLinkRemFcipEntityAddressType object."
       ::= { fcipLinkEntry 10 }

   fcipLinkStatus   OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS   read-create
       STATUS   current
       DESCRIPTION
           "This object specifies the operational status of the row.

            The values of objects fcipLinkLocalFcipEntityAddressType,
            fcipLinkLocalFcipEntityAddress, fcipLinkRemFcipEntityWWN,
            fcipLinkRemFcipEntityId, fcipLinkRemFcipEntityAddressType,
            and fcipLinkRemFcipEntityAddress can be changed if the row
            is in active(1) state.  The object fcipLinkCost is set to
            the value zero(0) if no value is supplied at the time of row
            creation.

            Setting the status to destroy(6) deletes the specified FCIP
            link from the table.  It also deletes all rows corresponding
            to the specified FCIP link from the fcipTcpConnTable table."
       ::= { fcipLinkEntry 11 }

   fcipLinkCreateTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of sysUpTime when this entry was last created."
       ::= { fcipLinkEntry 12 }


   -- ******************************************************************
   -- The TCP Connection Table
   --

   fcipTcpConnTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipTcpConnEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about existing TCP connections.  Each FCIP link
            within an FCIP entity manages one or more TCP connections.
            The FCIP entity employs a Data Engine for each TCP
            connection for handling FC frame encapsulation,
            de-encapsulation, and transmission of FCIP frames on the
            connection."
       ::= { fcipConfig 6 }

   fcipTcpConnEntry OBJECT-TYPE
       SYNTAX FcipTcpConnEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP TCP Connection table containing
            information about a particular TCP connection."
       INDEX { fcipEntityId,
               fcipLinkIndex,
               fcipTcpConnLocalPort,
               fcipTcpConnRemPort}
       ::= { fcipTcpConnTable 1 }

   FcipTcpConnEntry ::=
       SEQUENCE {
                   fcipTcpConnLocalPort      InetPortNumber,
                   fcipTcpConnRemPort        InetPortNumber,
                   fcipTcpConnRWSize         Unsigned32,
                   fcipTcpConnMSS            Unsigned32
   }

   fcipTcpConnLocalPort     OBJECT-TYPE
       SYNTAX InetPortNumber
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The local port number for this TCP connection."
       ::= { fcipTcpConnEntry 1 }

   fcipTcpConnRemPort     OBJECT-TYPE
       SYNTAX InetPortNumber
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "The remote port number for this TCP connection."
       ::= { fcipTcpConnEntry 2 }

   fcipTcpConnRWSize     OBJECT-TYPE
       SYNTAX Unsigned32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The default maximum TCP Receiver Window size for this TCP
            connection."
       ::= { fcipTcpConnEntry 3 }

   fcipTcpConnMSS     OBJECT-TYPE
       SYNTAX Unsigned32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The TCP Maximum Segment Size (MSS) for this TCP connection."
       ::= { fcipTcpConnEntry 4 }

   -- ******************************************************************
   -- The Dynamic Route Table
   --

   fcipDynamicRouteTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipDynamicRouteEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about dynamically discovered routing
            information.  The FCIP device may use the SLPv2 protocol in
            conjunction with other protocols (say, FSPF) for dynamically
            discovering other FCIP entities and may populate this table
            with FCIP link information for each Destination Address
            Identifier."
       ::= { fcipConfig 7 }

   fcipDynamicRouteEntry OBJECT-TYPE
       SYNTAX FcipDynamicRouteEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP Dynamic Route Table containing
            information about a particular FCIP route."
       INDEX { fcipEntityId, fcipDynamicRouteDID }
       ::= { fcipDynamicRouteTable 1 }

   FcipDynamicRouteEntry ::=
       SEQUENCE {
                   fcipDynamicRouteDID          FcipDomainIdInOctetForm,
                   fcipDynamicRouteLinkIndex    Unsigned32
               }

   fcipDynamicRouteDID    OBJECT-TYPE
       SYNTAX FcipDomainIdInOctetForm
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "8-bit ID of a Fibre Channel Domain that is reachable from
            this FCIP device."
       ::= { fcipDynamicRouteEntry  1 }

   fcipDynamicRouteLinkIndex    OBJECT-TYPE
       SYNTAX Unsigned32 (1..4294967295)
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The FCIP Link used to reach the domain specified by the
            corresponding instance of fcipDynamicRouteDID.  The link
            identified by a value of this object is the same FCIP link
            as identified by the same value of fcipLinkIndex for the
            same FCIP entity."
       ::= { fcipDynamicRouteEntry  2 }


   -- ******************************************************************
   -- The Static Route Table
   --

   fcipStaticRouteTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipStaticRouteEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about static route entries configured by the
            Network Admin.  In the absence of dynamic discovery of
            remote FCIP entities, the Network Manager will figure out
            all remote FCIP devices that are reachable from this device
            and populate this table with FCIP link information for each
            Domain ID.  At any time, both static and dynamic routing
            can be active, and an entry in the static route table for a
            given DID takes precedence over the entry in the dynamic
            route table for the same Domain ID."
       ::= { fcipConfig 8 }

   fcipStaticRouteEntry OBJECT-TYPE
       SYNTAX FcipStaticRouteEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP Static Route Table containing
            information about a particular FCIP route.  The values of
            the read-create objects in this table are persistent across
            system restarts."
       INDEX { fcipEntityId, fcipStaticRouteDID }
       ::= { fcipStaticRouteTable 1 }

   FcipStaticRouteEntry ::=
       SEQUENCE {
                   fcipStaticRouteDID           FcipDomainIdInOctetForm,
                   fcipStaticRouteLinkIndex     Unsigned32,
                   fcipStaticRouteStatus        RowStatus
               }

   fcipStaticRouteDID    OBJECT-TYPE
       SYNTAX FcipDomainIdInOctetForm
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "8-bit ID of a Fibre Channel Domain that is reachable from
            this FCIP device."
       ::= { fcipStaticRouteEntry  1 }

   fcipStaticRouteLinkIndex    OBJECT-TYPE
       SYNTAX Unsigned32 (1..4294967295)
       MAX-ACCESS read-create
       STATUS current
       DESCRIPTION
           "The FCIP Link used to reach the domain specified by the
            corresponding instance of fcipStaticRouteDID.  The link
            identified by a value of this object is the same FCIP link
            as identified by the same value of fcipLinkIndex for the
            same FCIP entity."
       ::= { fcipStaticRouteEntry  2 }

   fcipStaticRouteStatus   OBJECT-TYPE
       SYNTAX RowStatus
       MAX-ACCESS   read-create
       STATUS   current
       DESCRIPTION
           "This object specifies the operational status of the row.

            When a management station sets the status to active(1),
            the values for the object fcipStaticRouteLinkIndex should be
            supplied as part of the set request.

            Setting the status to destroy(6) deletes the specified FCIP
            static route entry from the table."
       ::= { fcipStaticRouteEntry  3 }


   -- ******************************************************************
   -- The FCIP Discovery Domain Table
   --

   fcipDiscoveryDomainTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipDiscoveryDomainEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Information about FCIP Discovery Domains.  Each FCIP
            Discovery Domain is associated with one or more FCIP
            entities."
       ::= { fcipConfig 9 }

   fcipDiscoveryDomainEntry OBJECT-TYPE
       SYNTAX FcipDiscoveryDomainEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP Discovery Domain Table
            containing information about a particular FCIP Discovery
            Domain that is associated with one or more FCIP entities.
            The values of the read-write object fcipDiscoveryDomainName
            are persistent across system restarts."
       INDEX { fcipEntityId, fcipDiscoveryDomainIndex }
       ::= { fcipDiscoveryDomainTable 1 }

   FcipDiscoveryDomainEntry ::=
       SEQUENCE {
           fcipDiscoveryDomainIndex        Unsigned32,
           fcipDiscoveryDomainName         SnmpAdminString
       }

   fcipDiscoveryDomainIndex OBJECT-TYPE
       SYNTAX     Unsigned32 (1..4294967295)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
           "An integer that uniquely identifies an FCIP Discovery Domain
            associated with this FCIP entity."
       ::= { fcipDiscoveryDomainEntry 1 }

   fcipDiscoveryDomainName   OBJECT-TYPE
       SYNTAX SnmpAdminString (SIZE (0..128))
       MAX-ACCESS read-write
       STATUS current
       DESCRIPTION
           "The name of this FCIP Discovery Domain."
       REFERENCE
           "RFC 3822, Section 4.1.1, FCIP Discovery Domains"
       ::= { fcipDiscoveryDomainEntry 2 }

   -- ******************************************************************
   -- The FCIP Link Errors
   --

   fcipLinkErrorsTable OBJECT-TYPE
       SYNTAX SEQUENCE OF FcipLinkErrorsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A list of error counters for FCIP Links.  Each counter
            records the number of times a particular error happened that
            caused a TCP connection to close down."
       REFERENCE
           "RFC 3821, Section 5.2, FCIP Link"
       ::= { fcipConfig 10 }

   fcipLinkErrorsEntry OBJECT-TYPE
       SYNTAX FcipLinkErrorsEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A conceptual row of the FCIP Link Errors Table containing
            error counters for an FCIP Link."
       INDEX { fcipEntityId, fcipLinkIndex }
       ::= { fcipLinkErrorsTable 1 }

   FcipLinkErrorsEntry ::=
       SEQUENCE {
           fcipLinkFcipLossofFcSynchs            Counter32,
           fcipLinkFcipEncapErrors               Counter32,
           fcipLinkFcipNotReceivedSfResps        Counter32,
           fcipLinkFcipSfRespMismatches          Counter32,
           fcipLinkFcipSfInvalidNonces           Counter32,
           fcipLinkFcipReceivedSfDuplicates      Counter32,
           fcipLinkFcipSfInvalidWWNs             Counter32,
           fcipLinkFcipBB2LkaTimeOuts            Counter32,
           fcipLinkFcipSntpExpiredTimeStamps     Counter32,
           fcipLinkTcpTooManyErrors              Counter32,
           fcipLinkTcpExcessiveDroppedDatagrams  Counter32,
           fcipLinkTcpSaParamMismatches          Counter32
       }

   fcipLinkFcipLossofFcSynchs OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times FC synchronization was lost on this FCIP
            Link.  The last discontinuity of this counter is indicated
            by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 1 }

   fcipLinkFcipEncapErrors OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of FCIP frames received with encapsulation errors
            such as improper header, format, or length.  The last
            discontinuity of this counter is indicated by
            fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 2 }

   fcipLinkFcipNotReceivedSfResps OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times an FCIP Special Frame Response was
            expected but not received on this FCIP Link.  The last
            discontinuity of this counter is indicated by
            fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 3 }

   fcipLinkFcipSfRespMismatches OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times FCIP Special Frame Bytes mismatch
            happened on this FCIP Link.  The last discontinuity of this
            counter is indicated by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 4 }

   fcipLinkFcipSfInvalidNonces OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times FCIP Special Frame Invalid Connection
            Nonce happened on this FCIP Link.  The last discontinuity
            of this counter is indicated by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 5 }

   fcipLinkFcipReceivedSfDuplicates OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times duplicate FCIP Special Frames were
            received on this FCIP Link.  The last discontinuity of this
            counter is indicated by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 6 }

   fcipLinkFcipSfInvalidWWNs OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times FCIP Special Frames with invalid
            destination FC Fabric Entity WWN were received on this FCIP
            Link.  The last discontinuity of this counter is indicated
            by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 7 }

   fcipLinkFcipBB2LkaTimeOuts OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of FC Keep Alive Time-outs that occurred on
            this FCIP Link.  The last discontinuity of this counter
            is indicated by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 8 }

   fcipLinkFcipSntpExpiredTimeStamps OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of frames discarded due to an expired Simple
            Network Time Protocol (SNTP) timestamp on this FCIP Link.
            The last discontinuity of this counter is indicated by
            fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 9 }

   fcipLinkTcpTooManyErrors OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of TCP connections that closed down on this
            FCIP Link due to too many errors on the connection.  The
            last discontinuity of this counter is indicated by
            fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 10  }

   fcipLinkTcpExcessiveDroppedDatagrams OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of TCP connections that closed down on this
            FCIP Link due to an excessive number of dropped FCIP
            packets.  The last discontinuity of this counter is
            indicated by fcipLinkCreateTime."
       ::= { fcipLinkErrorsEntry 11  }

   fcipLinkTcpSaParamMismatches OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "The number of times TCP connections with Security
            Association parameter mismatches were closed down on this
            FCIP Link.  The last discontinuity of this counter is
            indicated by fcipLinkCreateTime."
       REFERENCE
           "RFC 3821, Section 9.4.2, TCP Connection Security
            Associations (SAs)"
       ::= { fcipLinkErrorsEntry 12  }


   -- ******************************************************************
   -- Conformance Statements
   --

   fcipCompliances   OBJECT IDENTIFIER ::= { fcipConformance 1 }
   fcipGroups        OBJECT IDENTIFIER ::= { fcipConformance 2 }

   fcipCompliance MODULE-COMPLIANCE
       STATUS current
       DESCRIPTION
           "Compliance statement for FCIP MIB."
       MODULE       -- this module
           MANDATORY-GROUPS {
               fcipEntityScalarGroup,
               fcipEntityInstanceGroup,
               fcipLinkGroup,
               fcipTcpConnGroup,
               fcipDiscoveryDomainGroup,
               fcipLinkErrorsGroup

           }

           GROUP   fcipDynamicRouteGroup
           DESCRIPTION
               "This group is mandatory only for systems that do not
                have these objects in any other FC MIB.  It may be
                implemented even in that case for convenience."

           GROUP   fcipStaticRouteGroup
           DESCRIPTION
               "This group is mandatory only for systems that do not
                have these objects in any other FC MIB.  It may be
                implemented even in that case for convenience."

          OBJECT   fcipEntityAddressType
          SYNTAX   INTEGER { ipv4(1), ipv6(2) }
          DESCRIPTION
              "Only IPv4 and IPv6 address types need to be supported for
               addressing FCIP entities."

          OBJECT   fcipEntityAddress
          SYNTAX   InetAddress (SIZE(4|16))
          DESCRIPTION
              "Size of FCIP entity's IP address depends on address type.
               FCIP entity address size is four if the IP address is
               IPv4 and sixteen if the IP address type is IPv6."

          OBJECT   fcipLinkLocalFcipEntityAddressType
          SYNTAX   INTEGER { ipv4(1), ipv6(2) }
          DESCRIPTION
              "Only IPv4 and IPv6 address types need to be supported for
               addressing the local FCIP entities."

          OBJECT   fcipLinkLocalFcipEntityAddress
          SYNTAX   InetAddress (SIZE(4|16))
          DESCRIPTION
              "Size of FCIP entity's IP address depends on address type.
               FCIP entity address size is four if the IP address is
               IPv4 and sixteen if the IP address type is IPv6."

          OBJECT   fcipLinkRemFcipEntityAddressType
          SYNTAX   INTEGER { ipv4(1), ipv6(2) }
          DESCRIPTION
              "Only IPv4 and IPv6 address types need to be supported for
               addressing the remote FCIP entities."

          OBJECT   fcipLinkRemFcipEntityAddress
          SYNTAX   InetAddress (SIZE(4|16))
          DESCRIPTION
              "Size of FCIP entity's IP address depends on the address
               type.  FCIP entity address size is four if the IP address
               is IPv4 and sixteen if the IP address type is IPv6."

       ::= { fcipCompliances 1 }

   fcipEntityScalarGroup OBJECT-GROUP
       OBJECTS {   fcipDynIpConfType,
                   fcipDeviceWWN,
                   fcipEntitySACKOption
       }
       STATUS current
       DESCRIPTION
           "Collection of scalar objects applicable to all FCIP
            instances."
   ::= { fcipGroups 1 }

   fcipEntityInstanceGroup OBJECT-GROUP
       OBJECTS {
                   fcipEntityName,
                   fcipEntityAddressType,
                   fcipEntityAddress,
                   fcipEntityTcpConnPort,
                   fcipEntitySeqNumWrap,
                   fcipEntityPHBSupport,
                   fcipEntityStatus
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            instances."
   ::= { fcipGroups 2 }

   fcipLinkGroup OBJECT-GROUP
       OBJECTS {
                   fcipLinkIfIndex,
                   fcipLinkCost,
                   fcipLinkLocalFcipEntityMode,
                   fcipLinkLocalFcipEntityAddressType,
                   fcipLinkLocalFcipEntityAddress,
                   fcipLinkRemFcipEntityWWN,
                   fcipLinkRemFcipEntityId,
                   fcipLinkRemFcipEntityAddressType,
                   fcipLinkRemFcipEntityAddress,
                   fcipLinkStatus,
                   fcipLinkCreateTime
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            Links."
   ::= { fcipGroups 3 }

   fcipTcpConnGroup OBJECT-GROUP
       OBJECTS {
                   fcipTcpConnRWSize,
                   fcipTcpConnMSS
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            TCP connections."
   ::= { fcipGroups 4 }

   fcipDiscoveryDomainGroup OBJECT-GROUP
       OBJECTS {
                   fcipDiscoveryDomainName
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            Discovery Domains."
   ::= { fcipGroups 5 }

   fcipLinkErrorsGroup OBJECT-GROUP
       OBJECTS {
           fcipLinkFcipLossofFcSynchs,
           fcipLinkFcipEncapErrors,
           fcipLinkFcipNotReceivedSfResps,
           fcipLinkFcipSfRespMismatches,
           fcipLinkFcipSfInvalidNonces,
           fcipLinkFcipReceivedSfDuplicates,
           fcipLinkFcipSfInvalidWWNs,
           fcipLinkFcipBB2LkaTimeOuts,
           fcipLinkFcipSntpExpiredTimeStamps,
           fcipLinkTcpTooManyErrors,
           fcipLinkTcpExcessiveDroppedDatagrams,
           fcipLinkTcpSaParamMismatches
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            link errors."
   ::= { fcipGroups 6 }
   fcipDynamicRouteGroup OBJECT-GROUP
       OBJECTS {
                   fcipDynamicRouteLinkIndex
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            dynamic routes."
   ::= { fcipGroups 7 }

   fcipStaticRouteGroup OBJECT-GROUP
       OBJECTS {
                   fcipStaticRouteLinkIndex,
                   fcipStaticRouteStatus
       }
       STATUS current
       DESCRIPTION
           "A collection of objects providing information about FCIP
            static routes."
   ::= { fcipGroups 8 }

   END

-- 
--    Copyright (C) The Internet Society (2006).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

