-- extracted from rfc4069.txt
-- at Thu May  5 06:25:23 2005

   VDSL-LINE-EXT-SCM-MIB DEFINITIONS ::= BEGIN

   IMPORTS

   MODULE-IDENTITY,
   OBJECT-TYPE,
   Integer32,
   transmission,
   Unsigned32                      FROM SNMPv2-SMI         -- [RFC2578]
   TEXTUAL-CONVENTION,
   TruthValue,
   RowStatus                       FROM SNMPv2-TC          -- [RFC2579]
   MODULE-COMPLIANCE,
   OBJECT-GROUP                    FROM SNMPv2-CONF        -- [RFC2580]
   ifIndex                         FROM IF-MIB             -- [RFC2863]
   vdslLineConfProfileName         FROM VDSL-LINE-MIB;     -- [RFC3728]

   vdslExtSCMMIB MODULE-IDENTITY
      LAST-UPDATED "200504280000Z" --     April 28, 2005
      ORGANIZATION "ADSLMIB Working Group"
      CONTACT-INFO "WG-email:  adslmib@ietf.org
            Info:      https://www1.ietf.org/mailman/listinfo/adslmib

            Chair:     Mike Sneed
                       Sand Channel Systems
            Postal:    P.O. Box 37324
                       Raleigh NC 27627-732
            Email:     sneedmike@hotmail.com
            Phone:     +1 206 600 7022

            Co-Chair/Co-editor:
                       Bob Ray
                       PESA Switching Systems, Inc.
            Postal:    330-A Wynn Drive
                       Huntsville, AL 35805
                       USA
            Email:     rray@pesa.com
            Phone:     +1 256 726 9200 ext.  142
            Co-editor: Menachem Dodge
                       ECI Telecom Ltd.
            Postal:    30 Hasivim St.
                       Petach Tikva 49517,
                       Israel
            Email:     mbdodge@ieee.org
            Phone:     +972 3 926 8421
           "

   DESCRIPTION
      "The VDSL-LINE-MIB found in RFC 3728 defines objects for the
      management of a pair of VDSL transceivers at each end of the VDSL
      line.  The VDSL-LINE-MIB configures and monitors the line code
      independent parameters (TC layer) of the VDSL line.  This MIB
      module is an optional extension of the VDSL-LINE-MIB and defines
      objects for configuration and monitoring of the line code specific
      (LCS) elements (PMD layer) for VDSL lines using SCM coding.  The
      objects in this extension MIB MUST NOT be used for VDSL lines
      using Multiple Carrier Modulation (MCM) line coding.  If an object
      in this extension MIB is referenced by a line which does not use
      SCM, it has no effect on the operation of that line.

      Naming Conventions:

         Vtuc -- VDSL transceiver at near (Central) end of line
         Vtur -- VDSL transceiver at Remote end of line
         Vtu  -- One of either Vtuc or Vtur
         Curr -- Current
         Atn  -- Attenuation
         LCS  -- Line Code Specific
         Max  -- Maximum
         Mgn  -- Margin
         PSD  -- Power Spectral Density
         Rx   -- Receive
         Snr  -- Signal to Noise Ratio
         Tx   -- Transmit

      Copyright (C) The Internet Society (2005).  This version
      of this MIB module is part of RFC 4069: see the RFC
      itself for full legal notices."
              REVISION "200504280000Z" --     April 28, 2005
              DESCRIPTION "Initial version, published as RFC 4069."
          ::= { transmission 228 }

          vdslLineExtSCMMib    OBJECT IDENTIFIER ::= { vdslExtSCMMIB 1 }
          vdslLineExtSCMMibObjects OBJECT IDENTIFIER ::=
                                                 { vdslLineExtSCMMib 1 }
   --
   -- textual conventions used in this MIB
   --

   VdslSCMBandId ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
          "This data type is used as the syntax for the VDSL SCM Band
           Identity.  Attributes with this syntax identify the SCM Band
           referred to.  Specified as an INTEGER, the possible values
           are:

           optionalBand (1)  -- the optional Band range [25kHz - 138kHz]
           firstDownstreamBand (2)  -- first Downstream Band
           firstUpstreamBand (3)    -- first Upstream Band
           secondDownstreamBand (4) -- second Downstream Band
           secondUpstreamBand (5)   -- second Upstream Band
           thirdDownstreamBand (6)  -- third Downstream Band
           thirdUpstreamBand (7)    -- third Upstream Band"


       SYNTAX      INTEGER       {  optionalBand (1),
                                    firstDownstreamBand (2),
                                    firstUpstreamBand (3),
                                    secondDownstreamBand (4),
                                    secondUpstreamBand (5),
                                    thirdDownstreamBand (6),
                                    thirdUpstreamBand(7) }

   --
   -- Single carrier modulation (SCM) configuration profile tables
   --

   vdslLineSCMConfProfileBandTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineSCMConfProfileBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "This table contains transmit band descriptor configuration
           information for a VDSL line.  Each entry in this table
           reflects the configuration for one of possibly many bands
           of a single carrier modulation (SCM) VDSL line.  For each
           profile which is associated with a VDSL line using SCM
           line coding, five entries in this table will exist, one for
           each of the five bands.  Bands which are not in use will be
           marked as unused.  These entries are defined by a manager
           and can be used to configure the VDSL line.  If an entry in
           this table is referenced by a line which does not use SCM,
           it has no effect on the operation of that line."
       ::= { vdslLineExtSCMMibObjects 1 }

   vdslLineSCMConfProfileBandEntry OBJECT-TYPE
       SYNTAX       VdslLineSCMConfProfileBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "Each entry consists of a list of parameters that
           represents the configuration of a single carrier
           modulation VDSL modem transmit band.

           A default profile with an index of 'DEFVAL', will
           always exist and its parameters will be set to vendor
           specific values, unless otherwise specified in this
           document.

           All read-create objects defined in this MIB module SHOULD be
           stored persistently."

       INDEX { vdslLineConfProfileName,
        vdslLineSCMConfProfileBandId }
       ::= { vdslLineSCMConfProfileBandTable 1 }

   VdslLineSCMConfProfileBandEntry ::=
       SEQUENCE
          {
          vdslLineSCMConfProfileBandId                VdslSCMBandId,
          vdslLineSCMConfProfileBandInUse             TruthValue,
          vdslLineSCMConfProfileBandCenterFrequency   Unsigned32,
          vdslLineSCMConfProfileBandSymbolRate        Unsigned32,
          vdslLineSCMConfProfileBandConstellationSize Unsigned32,
          vdslLineSCMConfProfileBandTransmitPSDLevel  Unsigned32,
          vdslLineSCMConfProfileBandRowStatus         RowStatus
          }

   vdslLineSCMConfProfileBandId OBJECT-TYPE
       SYNTAX      VdslSCMBandId
       MAX-ACCESS  not-accessible
       STATUS  current
       DESCRIPTION
          "The BandId for this entry, which specifies which band
           is being referred to."
       ::= { vdslLineSCMConfProfileBandEntry 1 }

   vdslLineSCMConfProfileBandInUse OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-create
       STATUS  current
       DESCRIPTION
          "Indicates whether this band is in use.
           If set to True this band is in use."
       ::= { vdslLineSCMConfProfileBandEntry 2 }

   vdslLineSCMConfProfileBandCenterFrequency OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "Hz"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Specifies the center frequency in Hz"
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMConfProfileBandEntry 3 }

   vdslLineSCMConfProfileBandSymbolRate OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "baud"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The requested symbol rate in baud."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMConfProfileBandEntry 4 }

   vdslLineSCMConfProfileBandConstellationSize OBJECT-TYPE
       SYNTAX       Unsigned32 (0..16)
       UNITS        "log2"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "Specifies the constellation size."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMConfProfileBandEntry 5 }

   vdslLineSCMConfProfileBandTransmitPSDLevel OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "-0.25 dBm/Hz"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "The requested transmit power spectral density for the VDSL
           modem.  The Actual value in -0.25 dBm/Hz."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMConfProfileBandEntry 6  }

   vdslLineSCMConfProfileBandRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
          "This object is used to create a new row or modify or
           delete an existing row in this table.

           A profile activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.

           None of the columns in this row may be modified while the
           row is in the `active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."

       ::= { vdslLineSCMConfProfileBandEntry 7 }

   --
   -- SCM physical band
   --

   vdslLineSCMPhysBandTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineSCMPhysBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
          "This table provides one row for each SCM Vtu band.  This
           table is read only as it reflects the current physical
           parameters of each band.  For each ifIndex which is
           associated with a VDSL line using SCM line coding, five
           entries in this table will exist, one for each of the
           five bands.  Bands which are not in use will be marked
           as unused."
       ::= { vdslLineExtSCMMibObjects 2 }

   vdslLineSCMPhysBandEntry OBJECT-TYPE
       SYNTAX        VdslLineSCMPhysBandEntry
       MAX-ACCESS    not-accessible
       STATUS        current
       DESCRIPTION
          "An entry in the vdslLineSCMPhysBandTable."
       INDEX { ifIndex,
               vdslLineSCMPhysBandId  }
       ::= { vdslLineSCMPhysBandTable 1 }

   VdslLineSCMPhysBandEntry ::=
       SEQUENCE
           {
           vdslLineSCMPhysBandId                    VdslSCMBandId,
           vdslLineSCMPhysBandInUse                 TruthValue,
           vdslLineSCMPhysBandCurrCenterFrequency   Unsigned32,
           vdslLineSCMPhysBandCurrSymbolRate        Unsigned32,
           vdslLineSCMPhysBandCurrConstellationSize Unsigned32,
           vdslLineSCMPhysBandCurrPSDLevel          Unsigned32,
           vdslLineSCMPhysBandCurrSnrMgn            Integer32,
           vdslLineSCMPhysBandCurrAtn               Unsigned32
           }

   vdslLineSCMPhysBandId OBJECT-TYPE
       SYNTAX      VdslSCMBandId
       MAX-ACCESS  not-accessible
       STATUS  current
       DESCRIPTION
           "The BandId for this entry, which specifies which band
            is being referred to."
       ::= { vdslLineSCMPhysBandEntry 1 }

   vdslLineSCMPhysBandInUse OBJECT-TYPE
       SYNTAX      TruthValue
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
          "Indicates whether this band is in use.
           If set to True this band is in use."
       ::= { vdslLineSCMPhysBandEntry 2 }

   vdslLineSCMPhysBandCurrCenterFrequency OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "Hz"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current center frequency in Hz for this band."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMPhysBandEntry 3 }

   vdslLineSCMPhysBandCurrSymbolRate    OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "baud"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current value of the symbol rate in baud for this
           band."
      REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
      ::= { vdslLineSCMPhysBandEntry 4 }

   vdslLineSCMPhysBandCurrConstellationSize OBJECT-TYPE
       SYNTAX       Unsigned32 (0..16)
       UNITS        "log2"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The current constellation size on this band."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMPhysBandEntry 5 }

   vdslLineSCMPhysBandCurrPSDLevel    OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "- 0.25 dBm/Hz"
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "The transmit power spectral density for the
           VDSL modem."
       REFERENCE    "T1E1.4/2000-011R3"    -- Part 2, SCM
       ::= { vdslLineSCMPhysBandEntry 6 }

   vdslLineSCMPhysBandCurrSnrMgn OBJECT-TYPE
       SYNTAX        Integer32
       UNITS         "0.25 dB"
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
          "Noise margin as seen by this Vtu and band with respect
           to its received signal in 0.25 dB."
       ::= { vdslLineSCMPhysBandEntry 7 }

   vdslLineSCMPhysBandCurrAtn OBJECT-TYPE
       SYNTAX        Unsigned32 (0..255)
       UNITS         "0.25 dB"
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
          "Measured difference in the total power transmitted by
           the peer Vtu on this band and the total power received
           by this Vtu on this band in 0.25 dB."
       ::= { vdslLineSCMPhysBandEntry 8 }

   -- conformance information

   vdslLineExtSCMConformance OBJECT IDENTIFIER ::=
                                               { vdslLineExtSCMMib 2 }
   vdslLineExtSCMGroups OBJECT IDENTIFIER ::=
                                       { vdslLineExtSCMConformance 1 }
   vdslLineExtSCMCompliances OBJECT IDENTIFIER ::=
                                       { vdslLineExtSCMConformance 2 }

   vdslLineExtSCMMibCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
          "The compliance statement for SNMP entities which
           manage VDSL interfaces."

       MODULE  -- this module

       MANDATORY-GROUPS
       {
         vdslLineExtSCMGroup
       }

       ::= { vdslLineExtSCMCompliances 1 }

   -- units of conformance

   vdslLineExtSCMGroup    OBJECT-GROUP
       OBJECTS
           {
           vdslLineSCMConfProfileBandInUse,
           vdslLineSCMConfProfileBandTransmitPSDLevel,
           vdslLineSCMConfProfileBandSymbolRate,
           vdslLineSCMConfProfileBandConstellationSize,
           vdslLineSCMConfProfileBandCenterFrequency,
           vdslLineSCMConfProfileBandRowStatus,
           vdslLineSCMPhysBandInUse,
           vdslLineSCMPhysBandCurrPSDLevel,
           vdslLineSCMPhysBandCurrSymbolRate,
           vdslLineSCMPhysBandCurrConstellationSize,
           vdslLineSCMPhysBandCurrCenterFrequency,
           vdslLineSCMPhysBandCurrSnrMgn,
           vdslLineSCMPhysBandCurrAtn

           }
       STATUS      current
       DESCRIPTION
          "A collection of objects providing configuration
           information for a VDSL line based upon single carrier
           modulation modem."
       ::= { vdslLineExtSCMGroups 1 }

   END

-- 
--    Copyright (C) The Internet Society (2005).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 

