-- extracted from rfc4780.txt
-- at Tue May  1 06:08:36 2007

SIP-SERVER-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Unsigned32,
    Gauge32,
    mib-2
          FROM SNMPv2-SMI             -- RFC 2578

    TruthValue,
    TimeStamp, DateAndTime
          FROM SNMPv2-TC              -- RFC 2579

    MODULE-COMPLIANCE,
    OBJECT-GROUP
          FROM SNMPv2-CONF            -- RFC 2580

    SnmpAdminString
          FROM SNMP-FRAMEWORK-MIB     -- RFC 3411

    applIndex
          FROM NETWORK-SERVICES-MIB   -- RFC 2788

    InetAddressType,
    InetAddress
          FROM INET-ADDRESS-MIB;      -- RFC 4001

sipServerMIB MODULE-IDENTITY
    LAST-UPDATED   "200704200000Z"
    ORGANIZATION   "IETF Session Initiation Protocol
                    Working Group"
    CONTACT-INFO
       "SIP WG email: sip@ietf.org

           Co-editor: Kevin Lingle
                      Cisco Systems, Inc.
              postal: 7025 Kit Creek Road
                      P.O. Box 14987
                      Research Triangle Park, NC 27709
                      USA
             email:   klingle@cisco.com
             phone:   +1 919 476 2029

           Co-editor: Joon Maeng
               email: jmaeng@austin.rr.com

           Co-editor: Jean-Francois Mule
                      CableLabs
              postal: 858 Coal Creek Circle
                      Louisville, CO 80027
                      USA
               email: jf.mule@cablelabs.com
               phone: +1 303 661 9100

           Co-editor: Dave Walker
               email: drwalker@rogers.com
          "
    DESCRIPTION
       "Session Initiation Protocol (SIP) Server MIB module.  SIP is an
        application-layer signaling protocol for creating, modifying,
        and terminating multimedia sessions with one or more
        participants.  These sessions include Internet multimedia
        conferences and Internet telephone calls.  SIP is defined in
        RFC 3261 (June 2002).

        This MIB is defined for the management of SIP Proxy, Redirect,
        and Registrar Servers.
        A Proxy Server acts as both a client and a server.  It accepts
        requests from other clients, either responding to them or
        passing them on to other servers, possibly after modification.

        A Redirect Server accepts requests from clients and returns
        zero or more addresses to that client.  Unlike a User Agent
        Server, it does not accept calls.

        A Registrar is a server that accepts REGISTER requests.  A
        Registrar is typically co-located with a Proxy or Redirect
        Server.

        Copyright (C) The IETF Trust (2007).  This version of
        this MIB module is part of RFC 4780; see the RFC itself for
        full legal notices."
    REVISION        "200704200000Z"
    DESCRIPTION
       "Initial version of the IETF SIP-SERVER-MIB module.  This
       version published as part of RFC 4780."
  ::= { mib-2 151 }

-- Top-Level Components of this MIB.

sipServerMIBObjects     OBJECT IDENTIFIER ::= { sipServerMIB 1 }
sipServerMIBConformance OBJECT IDENTIFIER ::= { sipServerMIB 2 }

--
-- These groups contain objects common to all SIP servers.
--
sipServerCfg            OBJECT IDENTIFIER ::= { sipServerMIBObjects 1 }

--
-- Common Server Configuration Objects
--
sipServerCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains configuration objects applicable to SIP
        Redirect and Proxy Servers."
    ::= { sipServerCfg 1 }

sipServerCfgEntry OBJECT-TYPE
    SYNTAX      SipServerCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of common configuration.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through
        the common framework of the NETWORK-SERVICES-MIB (RFC 2788).
        The same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex }
    ::= { sipServerCfgTable 1 }

SipServerCfgEntry ::=
    SEQUENCE {
        sipServerCfgHostAddressType       InetAddressType,
        sipServerCfgHostAddress           InetAddress
    }

sipServerCfgHostAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only

    STATUS      current
    DESCRIPTION
       "The type of Internet address by which the SIP server is
        reachable."
    REFERENCE
       "RFC 3261, Section 19.1.1"
    ::= { sipServerCfgEntry 1 }

sipServerCfgHostAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the host portion of a SIP URI that is assigned to the
        SIP server.  It MAY contain a fully qualified domain name or
        an IP address.  The length of the value will depend on the type
        of address specified.  The type of address given by this object
        is controlled by sipServerCfgHostAddressType."
    REFERENCE
       "RFC 3261, Section 19.1.1"
    ::= { sipServerCfgEntry 2 }

--
-- This group contains MIB objects
-- related to SIP Proxy Servers.
--
sipServerProxyCfg      OBJECT IDENTIFIER ::= { sipServerMIBObjects 3 }
sipServerProxyStats    OBJECT IDENTIFIER ::= { sipServerMIBObjects 4 }

--
-- Proxy Server Configuration
--
sipServerProxyCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerProxyCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains configuration objects applicable to SIP
        Proxy Servers."
    ::= { sipServerProxyCfg 1 }

sipServerProxyCfgEntry OBJECT-TYPE
    SYNTAX      SipServerProxyCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of common proxy configuration.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex }
    ::= { sipServerProxyCfgTable 1 }

SipServerProxyCfgEntry ::=
    SEQUENCE {
        sipServerCfgProxyStatefulness     INTEGER,
        sipServerCfgProxyRecursion        TruthValue,
        sipServerCfgProxyRecordRoute      TruthValue,
        sipServerCfgProxyAuthMethod       BITS,
        sipServerCfgProxyAuthDefaultRealm SnmpAdminString
    }

sipServerCfgProxyStatefulness OBJECT-TYPE
    SYNTAX      INTEGER {
                  stateless(1),
                  transactionStateful(2),
                  callStateful(3)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the default mode of operation for the
        Proxy Server entity.

        A stateless proxy is a logical entity that does not maintain
        the client or server transaction state machines when it
        processes requests.  A stateless proxy forwards every request it
        receives downstream and every response it receives upstream.  If
        the value of this object is stateless(1), the proxy defaults to
        stateless operations.

        A transaction stateful proxy, or simply a 'stateful proxy', is
        a logical entity that maintains the client and server
        transaction state machines during the processing of a request.
        A (transaction) stateful proxy is not the same as a call
        stateful proxy.  If the value of this object is
        transactionStateful(2), the proxy is stateful on a transaction
        basis.

        A call stateful proxy is a logical entity if it retains state
        for a dialog from the initiating INVITE to the terminating BYE
        request.  A call stateful proxy is always transaction stateful,
        but the converse is not necessarily true.  If the value of this
        object is callStateful(3), the proxy is call stateful."

    REFERENCE
        "RFC 3261, Section 16"
    ::= { sipServerProxyCfgEntry 1 }

sipServerCfgProxyRecursion OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects whether or not the Proxy performs a
        recursive search on the Contacts provided in 3xx redirects.

        If the value of this object is 'true', a recursive search is
        performed.  If the value is 'false', no search is performed,
        and the 3xx response is sent upstream towards the source of
        the request."
    REFERENCE
       "RFC 3261 Sections 16.5 and 16.6"
    ::= { sipServerProxyCfgEntry 2 }

sipServerCfgProxyRecordRoute OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This object reflects whether or not the proxy adds itself to
        the Record-Route header as a default action.  This header is
        used to list the proxies that insist on being in the signaling
        path for subsequent requests related to the call leg.

        If the value of this object is 'true', the proxy adds itself to
        the end of the Record-Route header, creating the header if
        required.  If the value is 'false', the proxy does not add
        itself to the Record-Route header."
    REFERENCE
       "RFC 3261, Section 20.30"
    ::= { sipServerProxyCfgEntry 3 }

--
-- Security
--
sipServerCfgProxyAuthMethod OBJECT-TYPE
    SYNTAX      BITS {
                  none(0),
                  tls(1),
                  digest(2)
                }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the authentication methods that MAY be
        used to authenticate request originators.

        bit 0  no authentication is performed
        bit 1  TLS is used
        bit 2  HTTP Digest is used."
    REFERENCE
       "RFC 3261 Sections 22, 23, 26, 26.2.3"
    ::= { sipServerProxyCfgEntry 4 }

sipServerCfgProxyAuthDefaultRealm OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the default realm value used in
        Proxy-Authenticate headers.  Note that this MAY need to be
        stored per user, in which case, this default value is ignored.
       "
    REFERENCE
       "RFC 3261, Section 22.1"
    ::= { sipServerProxyCfgEntry 5 }

--
-- Proxy Server Statistics
--
sipServerProxyStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerProxyStatsEntry
    MAX-ACCESS  not-accessible

    STATUS      current
    DESCRIPTION
       "This table contains the statistics objects applicable to all
        SIP Proxy Servers in this system."
    ::= { sipServerProxyStats 1 }

sipServerProxyStatsEntry OBJECT-TYPE
    SYNTAX      SipServerProxyStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of summary statistics.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex }
    ::= { sipServerProxyStatsTable 1 }

SipServerProxyStatsEntry ::=
    SEQUENCE {
        sipServerProxyStatProxyReqFailures Counter32,
        sipServerProxyStatsDisconTime      TimeStamp
    }

sipServerProxyStatProxyReqFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains the number of occurrences of unsupported
        options being specified in received Proxy-Require headers.
        Such occurrences result in a 420 Bad Extension status code
        being returned.

        Discontinuities in the value of this counter can occur at
        re-initialization of the SIP entity or service.  A Management
        Station can detect discontinuities in this counter by
        monitoring the sipServerProxyStatsDisconTime object in the same
        row."
    ::= { sipServerProxyStatsEntry 1 }

sipServerProxyStatsDisconTime OBJECT-TYPE
 SYNTAX      TimeStamp
 MAX-ACCESS  read-only
 STATUS      current
 DESCRIPTION
    "The value of the sysUpTime object when the counters for the server
     statistics objects in this row last experienced a discontinuity."
 ::= { sipServerProxyStatsEntry 2 }

--
-- This group contains MIB objects related to SIP Registrars.
--
sipServerRegCfg         OBJECT IDENTIFIER ::= { sipServerMIBObjects 5 }
sipServerRegStats       OBJECT IDENTIFIER ::= { sipServerMIBObjects 6 }

--
-- Registrar Configuration
--
sipServerRegCfgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerRegCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains configuration objects applicable to SIP
        Registrars."
    ::= { sipServerRegCfg 1 }

sipServerRegCfgEntry OBJECT-TYPE
    SYNTAX      SipServerRegCfgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of common Registrar configuration.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex }
    ::= { sipServerRegCfgTable 1 }

SipServerRegCfgEntry ::=
    SEQUENCE {
        sipServerRegMaxContactExpiryDuration  Unsigned32,
        sipServerRegMaxUsers                  Unsigned32,
        sipServerRegCurrentUsers              Gauge32,
        sipServerRegDfltRegActiveInterval     Unsigned32
    }

sipServerRegMaxContactExpiryDuration OBJECT-TYPE
    SYNTAX      Unsigned32 (0..4294967295)
    UNITS      "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the maximum expiry that may be requested
        by a User Agent for a particular Contact.  User Agents can
        specify expiry using either an Expiry header in a REGISTER
        request, or using an Expires parameter in a Contact header in
        a REGISTER request.  If the value requested by the User Agent
        is greater than the value of this object, then the contact
        information is given the duration specified by this object, and
        that duration is indicated to the User Agent in the response."
    ::= { sipServerRegCfgEntry 1 }

sipServerRegMaxUsers OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the maximum number of users that the
        Registrar supports.  The current number of users is reflected
        by sipServerRegCurrentUsers."
    ::= { sipServerRegCfgEntry 2 }

sipServerRegCurrentUsers OBJECT-TYPE
    SYNTAX      Gauge32 (0..4294967295)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the number of users currently registered
        with the Registrar."
    ::= { sipServerRegCfgEntry 3 }

sipServerRegDfltRegActiveInterval OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    UNITS      "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object reflects the default time interval the Registrar
        considers registrations to be active.  The value is used to
        compute the Expires header in the REGISTER response.  If a user
        agent requests a time interval shorter than specified by this
        object, the Registrar SHOULD honor that request.  If a Contact
        entry does not have an 'expires' parameter, the value of the
        Expires header field is used instead.  If a Contact entry has no
        'expires' parameter and no Expires header field is present,
        the value of this object is used as the default value."
    REFERENCE
       "RFC 3261, Section 10.2"
    ::= { sipServerRegCfgEntry 4 }
--
-- Per User Information
--
sipServerRegUserTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerRegUserEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains information on all users registered to each
        Registrar in this system."
    ::= { sipServerRegCfg 2 }

sipServerRegUserEntry OBJECT-TYPE
    SYNTAX      SipServerRegUserEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This entry contains information for a single user registered to
        this Registrar.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex, sipServerRegUserIndex }
    ::= { sipServerRegUserTable 1 }

SipServerRegUserEntry ::=
    SEQUENCE {
        sipServerRegUserIndex                  Unsigned32,
        sipServerRegUserUri                    SnmpAdminString,
        sipServerRegUserAuthenticationFailures Counter32,
        sipServerRegUserDisconTime             TimeStamp
    }

sipServerRegUserIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This object uniquely identifies a conceptual row in the table."
    ::= { sipServerRegUserEntry 1 }

sipServerRegUserUri OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains the user's address-of-record.  It is the
        main form by which the Registrar knows the user.  The format is
        typically 'user@domain'.  It is contained in the To header for
        all REGISTER requests."
    ::= { sipServerRegUserEntry 2 }

sipServerRegUserAuthenticationFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains a count of the number of times the user
        has failed authentication.

        Discontinuities in the value of this counter can occur due to
        successful user authentications and at re-initialization of
        the SIP entity or service.  A Management Station can detect
        discontinuities in this counter by monitoring the
        sipServerRegUserDisconTime object in the same row."
    ::= { sipServerRegUserEntry 3 }

sipServerRegUserDisconTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The value of the sysUpTime object when the counters for the
        user registration statistics objects in this row last
        experienced a discontinuity."
    ::= { sipServerRegUserEntry 4 }
--
-- Per Contact Information
--
sipServerRegContactTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerRegContactEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains information on every location where a
        registered user (specified by sipServerRegUserIndex) wishes to
        be found (i.e., the user has provided contact information to
        each SIP Registrar in this system)."
    ::= { sipServerRegCfg 3 }

sipServerRegContactEntry OBJECT-TYPE
    SYNTAX      SipServerRegContactEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This entry contains information for a single Contact.  Multiple
        contacts may exist for a single user.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."

    INDEX { applIndex,
            sipServerRegUserIndex,
            sipServerRegContactIndex
          }
    ::= { sipServerRegContactTable 1 }

SipServerRegContactEntry ::=
    SEQUENCE {
        sipServerRegContactIndex        Unsigned32,
        sipServerRegContactDisplayName  SnmpAdminString,
        sipServerRegContactURI          SnmpAdminString,
        sipServerRegContactLastUpdated  TimeStamp,
        sipServerRegContactExpiry       DateAndTime,
        sipServerRegContactPreference   SnmpAdminString
    }

sipServerRegContactIndex OBJECT-TYPE
    SYNTAX      Unsigned32 (1..4294967295)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "Along with the sipServerRegUserIndex, this object uniquely
        identifies a conceptual row in the table."
    ::= { sipServerRegContactEntry 1 }

sipServerRegContactDisplayName OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains the display name for the Contact.  For
        example, 'Santa at Home', or 'Santa on his Sled', corresponding
        to contact URIs of sip:BigGuy@example.com or
        sip:sclaus817@example.com, respectively."
    ::= { sipServerRegContactEntry 2 }

sipServerRegContactURI OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains either a SIP URI where the user can be
        contacted.  This URI is normally returned to a client from a
        Redirect Server, or is used as the RequestURI in a SIP request
        line for requests forwarded by a proxy."
    ::= { sipServerRegContactEntry 3 }

sipServerRegContactLastUpdated OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object indicates the time when this contact information
        was accepted.  If the contact information is updated via a
        subsequent REGISTER of the same information, this object is
        also updated."
    ::= { sipServerRegContactEntry 4 }

sipServerRegContactExpiry OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains the date and time when the contact
        information will no longer be valid.  Such times may be
        specified by the user at registration (i.e., Expires header or
        expiry parameter in the Contact information), or a system
        default can be applied."
    ::= { sipServerRegContactEntry 5 }

sipServerRegContactPreference OBJECT-TYPE
    SYNTAX      SnmpAdminString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object indicates a relative preference for the particular
        Contact header field value compared to other bindings for this
        address-of-record.  A registering user may provide this
        preference as a 'qvalue' parameter in the Contact header.

        The format of this item is a decimal number between 0 and 1
        (for example 0.9).  Higher values indicate locations preferred
        by the user."
    REFERENCE
       "RFC 3261, Section 10.2.1.2, 16.6, and 20.10"
    ::= { sipServerRegContactEntry 6 }

--
-- Registrar Statistics
--
sipServerRegStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF SipServerRegStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "This table contains the summary statistics objects applicable
        to all SIP Registrars in this system."
    ::= { sipServerRegStats 1 }

sipServerRegStatsEntry OBJECT-TYPE
    SYNTAX      SipServerRegStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
       "A row of summary statistics.

        Each row represents those objects for a particular SIP server
        present in this system.  applIndex is used to uniquely identify
        these instances of SIP servers and correlate them through the
        common framework of the NETWORK-SERVICES-MIB (RFC 2788).  The
        same value of applIndex used in the corresponding
        SIP-COMMON-MIB is used here."
    INDEX { applIndex }
    ::= { sipServerRegStatsTable 1 }

SipServerRegStatsEntry ::=
    SEQUENCE {
        sipServerRegStatsAcceptedRegs     Counter32,
        sipServerRegStatsRejectedRegs     Counter32,
        sipServerRegStatsDisconTime       TimeStamp
    }

sipServerRegStatsAcceptedRegs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains a count of the number of REGISTER requests
        that have been accepted (status code 200) by the Registrar.
        This includes additions of new contact information, refreshing
        contact information, as well as requests for deletion of
        contact information.

        Discontinuities in the value of this counter can occur at
        re-initialization of the SIP entity or service.  A Management
        Station can detect discontinuities in this counter by
        monitoring the sipServerRegStatsDisconTime object in the same
        row."
    ::= { sipServerRegStatsEntry 1 }

sipServerRegStatsRejectedRegs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This object contains a count of the number REGISTER requests
        that have been rejected by the Registrar.

        Discontinuities in the value of this counter can occur at
        re-initialization of the SIP entity or service.  A Management
        Station can detect discontinuities in this counter by
        monitoring the sipServerRegStatsDisconTime object in the same
        row."
  ::= { sipServerRegStatsEntry 2 }

sipServerRegStatsDisconTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The value of the sysUpTime object when the counters for the
        registrar statistics objects in this row last experienced a
        discontinuity."
 ::= { sipServerRegStatsEntry 3 }

--
-- Conformance
--
sipServerMIBCompliances
         OBJECT IDENTIFIER ::= { sipServerMIBConformance 1 }

sipServerMIBGroups
         OBJECT IDENTIFIER ::= { sipServerMIBConformance 2 }

--
-- Compliance Statements
--
sipServerProxyServerCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
       "The compliance statement for SIP entities acting as Proxy
        Servers."
    MODULE -- this module
        MANDATORY-GROUPS { sipServerConfigGroup,
                           sipServerProxyConfigGroup,
                           sipServerProxyStatsGroup
                         }
    ::= { sipServerMIBCompliances 1 }

sipRedirectServerCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
       "The compliance statement for SIP entities acting as Redirect
        Servers."
    MODULE -- this module
        MANDATORY-GROUPS { sipServerConfigGroup }
    ::= { sipServerMIBCompliances 2 }

sipServerRegistrarServerCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
       "The compliance statement for SIP entities acting as
        Registrars."
    MODULE -- this module
        MANDATORY-GROUPS { sipServerConfigGroup,
                           sipServerRegistrarConfigGroup,
                           sipServerRegistrarStatsGroup }
    GROUP sipServerRegistrarUsersGroup
    DESCRIPTION
       "This is an optional group."
    ::= { sipServerMIBCompliances 3 }

--
-- Units of Conformance
--
sipServerConfigGroup OBJECT-GROUP
    OBJECTS {
            sipServerCfgHostAddressType,
            sipServerCfgHostAddress

    }
    STATUS      current
    DESCRIPTION
       "A collection of objects providing configuration common to SIP
        Proxy and Redirect servers."
    ::= { sipServerMIBGroups 1 }

sipServerProxyConfigGroup OBJECT-GROUP
    OBJECTS {
            sipServerCfgProxyStatefulness,
            sipServerCfgProxyRecursion,
            sipServerCfgProxyRecordRoute,
            sipServerCfgProxyAuthMethod,
            sipServerCfgProxyAuthDefaultRealm
    }
    STATUS      current
    DESCRIPTION
       "A collection of objects providing configuration for SIP Proxy
        servers."
    ::= { sipServerMIBGroups 2 }

sipServerProxyStatsGroup OBJECT-GROUP
    OBJECTS {
            sipServerProxyStatProxyReqFailures,
            sipServerProxyStatsDisconTime
    }
    STATUS      current
    DESCRIPTION
       "A collection of objects providing statistics for SIP Proxy
        servers."
    ::= { sipServerMIBGroups 3 }

sipServerRegistrarConfigGroup OBJECT-GROUP
    OBJECTS {
            sipServerRegMaxContactExpiryDuration,
            sipServerRegMaxUsers,
            sipServerRegCurrentUsers,
            sipServerRegDfltRegActiveInterval
    }
    STATUS      current
    DESCRIPTION
       "A collection of objects providing configuration for SIP
        Registrars."
    ::= { sipServerMIBGroups 4 }

sipServerRegistrarStatsGroup OBJECT-GROUP
    OBJECTS {
            sipServerRegStatsAcceptedRegs,
            sipServerRegStatsRejectedRegs,
            sipServerRegStatsDisconTime
    }
    STATUS      current
    DESCRIPTION
       "A collection of objects providing statistics for SIP
        Registrars."
    ::= { sipServerMIBGroups 5 }

sipServerRegistrarUsersGroup OBJECT-GROUP
    OBJECTS {
            sipServerRegUserUri,
            sipServerRegUserAuthenticationFailures,
            sipServerRegUserDisconTime,
            sipServerRegContactDisplayName,
            sipServerRegContactURI,
            sipServerRegContactLastUpdated,
            sipServerRegContactExpiry,
            sipServerRegContactPreference
    }
    STATUS      current
    DESCRIPTION
       "A collection of objects related to registered users."
    ::= { sipServerMIBGroups 6 }

END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

