-- extracted from rfc4188.txt
-- at Fri Sep 30 06:36:21 2005

   BRIDGE-MIB DEFINITIONS ::= BEGIN

   -- ---------------------------------------------------------- --
   -- MIB for IEEE 802.1D devices
   -- ---------------------------------------------------------- --
   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
       Counter32, Integer32, TimeTicks, mib-2
           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION, MacAddress
           FROM SNMPv2-TC
       MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
           FROM SNMPv2-CONF
       InterfaceIndex FROM IF-MIB
       ;

   dot1dBridge MODULE-IDENTITY
       LAST-UPDATED "200509190000Z"
       ORGANIZATION "IETF Bridge MIB Working Group"
       CONTACT-INFO
           "Email: bridge-mib@ietf.org

                    K.C. Norseth (Editor)
                    L-3 Communications
               Tel: +1 801-594-2809
             Email: kenyon.c.norseth@L-3com.com
            Postal: 640 N. 2200 West.
                    Salt Lake City, Utah 84116-0850
                    Les Bell (Editor)
                    3Com Europe Limited
             Phone: +44 1442 438025
             Email: elbell@ntlworld.com
            Postal: 3Com Centre, Boundary Way
                    Hemel Hempstead
                    Herts.  HP2 7YU
                    UK

            Send comments to <bridge-mib@ietf.org>"
       DESCRIPTION
           "The Bridge MIB module for managing devices that support
           IEEE 802.1D.

           Copyright (C) The Internet Society (2005).  This version of
           this MIB module is part of RFC 4188; see the RFC itself for
           full legal notices."
       REVISION     "200509190000Z"
       DESCRIPTION
            "Third revision, published as part of RFC 4188.

            The MIB module has been converted to SMIv2 format.
            Conformance statements have been added and some
            description and reference clauses have been updated.

            The object dot1dStpPortPathCost32 was added to
            support IEEE 802.1t and the permissible values of
            dot1dStpPriority and dot1dStpPortPriority have been
            clarified for bridges supporting IEEE 802.1t or
            IEEE 802.1w.

            The interpretation of dot1dStpTimeSinceTopologyChange
            has been clarified for bridges supporting the Rapid
            Spanning Tree Protocol (RSTP)."
       REVISION     "199307310000Z"
       DESCRIPTION
            "Second revision, published as part of RFC 1493."
       REVISION     "199112310000Z"
       DESCRIPTION
            "Initial revision, published as part of RFC 1286."
       ::= { mib-2 17 }


   -- ---------------------------------------------------------- --
   -- Textual Conventions
   -- ---------------------------------------------------------- --

   BridgeId ::= TEXTUAL-CONVENTION
       STATUS      current
       DESCRIPTION
           "The Bridge-Identifier, as used in the Spanning Tree
           Protocol, to uniquely identify a bridge.  Its first two
           octets (in network byte order) contain a priority value,
           and its last 6 octets contain the MAC address used to
           refer to a bridge in a unique fashion (typically, the
           numerically smallest MAC address of all ports on the
           bridge)."
       SYNTAX      OCTET STRING (SIZE (8))

   Timeout ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "d"
       STATUS      current
       DESCRIPTION
           "A Spanning Tree Protocol (STP) timer in units of 1/100
           seconds.  Several objects in this MIB module represent
           values of timers used by the Spanning Tree Protocol.
           In this MIB, these timers have values in units of
           hundredths of a second (i.e., 1/100 secs).

           These timers, when stored in a Spanning Tree Protocol's
           BPDU, are in units of 1/256 seconds.  Note, however, that
           802.1D-1998 specifies a settable granularity of no more
           than one second for these timers.  To avoid ambiguity,
           a conversion algorithm is defined below for converting
           between the different units, which ensures a timer's
           value is not distorted by multiple conversions.

           To convert a Timeout value into a value in units of
           1/256 seconds, the following algorithm should be used:

               b = floor( (n * 256) / 100)

           where:
               floor   =  quotient [ignore remainder]
               n is the value in 1/100 second units
               b is the value in 1/256 second units

           To convert the value from 1/256 second units back to
           1/100 seconds, the following algorithm should be used:

               n = ceiling( (b * 100) / 256)

           where:
               ceiling = quotient [if remainder is 0], or
                         quotient + 1 [if remainder is nonzero]
               n is the value in 1/100 second units
               b is the value in 1/256 second units

           Note: it is important that the arithmetic operations are
           done in the order specified (i.e., multiply first,
           divide second)."
       SYNTAX      Integer32

   -- ---------------------------------------------------------- --
   -- subtrees in the Bridge MIB
   -- ---------------------------------------------------------- --

   dot1dNotifications  OBJECT IDENTIFIER ::= { dot1dBridge 0 }

   dot1dBase           OBJECT IDENTIFIER ::= { dot1dBridge 1 }
   dot1dStp            OBJECT IDENTIFIER ::= { dot1dBridge 2 }

   dot1dSr             OBJECT IDENTIFIER ::= { dot1dBridge 3 }
   -- documented in RFC 1525

   dot1dTp             OBJECT IDENTIFIER ::= { dot1dBridge 4 }
   dot1dStatic         OBJECT IDENTIFIER ::= { dot1dBridge 5 }

   -- Subtrees used by Bridge MIB Extensions:
   --      pBridgeMIB  MODULE-IDENTITY   ::= { dot1dBridge 6 }
   --      qBridgeMIB  MODULE-IDENTITY   ::= { dot1dBridge 7 }
   -- Note that the practice of registering related MIB modules
   -- below dot1dBridge has been discouraged since there is no
   -- robust mechanism to track such registrations.

   dot1dConformance    OBJECT IDENTIFIER ::= { dot1dBridge 8 }

   -- ---------------------------------------------------------- --
   -- the dot1dBase subtree
   -- ---------------------------------------------------------- --
   -- Implementation of the dot1dBase subtree is mandatory for all
   -- bridges.
   -- ---------------------------------------------------------- --

   dot1dBaseBridgeAddress OBJECT-TYPE

       SYNTAX      MacAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The MAC address used by this bridge when it must be
           referred to in a unique fashion.  It is recommended
           that this be the numerically smallest MAC address of
           all ports that belong to this bridge.  However, it is only
           required to be unique.  When concatenated with
           dot1dStpPriority, a unique BridgeIdentifier is formed,
           which is used in the Spanning Tree Protocol."
       REFERENCE
           "IEEE 802.1D-1998: clauses 14.4.1.1.3 and 7.12.5"
       ::= { dot1dBase 1 }

   dot1dBaseNumPorts OBJECT-TYPE
       SYNTAX      Integer32
       UNITS       "ports"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of ports controlled by this bridging
           entity."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.4.1.1.3"
       ::= { dot1dBase 2 }

   dot1dBaseType OBJECT-TYPE
       SYNTAX      INTEGER {
                       unknown(1),
                       transparent-only(2),
                       sourceroute-only(3),
                       srt(4)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Indicates what type of bridging this bridge can
           perform.  If a bridge is actually performing a
           certain type of bridging, this will be indicated by
           entries in the port table for the given type."
       ::= { dot1dBase 3 }

   -- ---------------------------------------------------------- --
   -- The Generic Bridge Port Table
   -- ---------------------------------------------------------- --
   dot1dBasePortTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Dot1dBasePortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table that contains generic information about every
           port that is associated with this bridge.  Transparent,
           source-route, and srt ports are included."
       ::= { dot1dBase 4 }

   dot1dBasePortEntry OBJECT-TYPE
       SYNTAX      Dot1dBasePortEntry
       MAX-ACCESS  not-accessible
       STATUS      current

       DESCRIPTION
           "A list of information for each port of the bridge."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.4.2, 14.6.1"
       INDEX  { dot1dBasePort }
       ::= { dot1dBasePortTable 1 }

   Dot1dBasePortEntry ::=
       SEQUENCE {
           dot1dBasePort
               Integer32,
           dot1dBasePortIfIndex
               InterfaceIndex,
           dot1dBasePortCircuit
               OBJECT IDENTIFIER,
           dot1dBasePortDelayExceededDiscards
               Counter32,
           dot1dBasePortMtuExceededDiscards
               Counter32
       }

   dot1dBasePort OBJECT-TYPE
       SYNTAX      Integer32 (1..65535)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The port number of the port for which this entry
           contains bridge management information."
       ::= { dot1dBasePortEntry 1 }

   dot1dBasePortIfIndex OBJECT-TYPE
       SYNTAX      InterfaceIndex
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The value of the instance of the ifIndex object,
           defined in IF-MIB, for the interface corresponding
           to this port."
       ::= { dot1dBasePortEntry 2 }

   dot1dBasePortCircuit OBJECT-TYPE
       SYNTAX      OBJECT IDENTIFIER
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "For a port that (potentially) has the same value of
           dot1dBasePortIfIndex as another port on the same bridge.
           This object contains the name of an object instance
           unique to this port.  For example, in the case where
           multiple ports correspond one-to-one with multiple X.25
           virtual circuits, this value might identify an (e.g.,
           the first) object instance associated with the X.25
           virtual circuit corresponding to this port.

           For a port which has a unique value of
           dot1dBasePortIfIndex, this object can have the value
           { 0 0 }."
       ::= { dot1dBasePortEntry 3 }

   dot1dBasePortDelayExceededDiscards OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of frames discarded by this port due
           to excessive transit delay through the bridge.  It
           is incremented by both transparent and source
           route bridges."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.6.1.1.3"
       ::= { dot1dBasePortEntry 4 }

   dot1dBasePortMtuExceededDiscards OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of frames discarded by this port due
           to an excessive size.  It is incremented by both
           transparent and source route bridges."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.6.1.1.3"
       ::= { dot1dBasePortEntry 5 }

   -- ---------------------------------------------------------- --
   -- the dot1dStp subtree
   -- ---------------------------------------------------------- --
   -- Implementation of the dot1dStp subtree is optional.  It is
   -- implemented by those bridges that support the Spanning Tree
   -- Protocol.
   -- ---------------------------------------------------------- --
   dot1dStpProtocolSpecification OBJECT-TYPE
       SYNTAX      INTEGER {
                       unknown(1),
                       decLb100(2),
                       ieee8021d(3)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "An indication of what version of the Spanning Tree
           Protocol is being run.  The value 'decLb100(2)'
           indicates the DEC LANbridge 100 Spanning Tree protocol.
           IEEE 802.1D implementations will return 'ieee8021d(3)'.
           If future versions of the IEEE Spanning Tree Protocol
           that are incompatible with the current version
           are released a new value will be defined."
       ::= { dot1dStp 1 }

   dot1dStpPriority OBJECT-TYPE
       SYNTAX      Integer32 (0..65535)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The value of the write-able portion of the Bridge ID
           (i.e., the first two octets of the (8 octet long) Bridge
           ID).  The other (last) 6 octets of the Bridge ID are
           given by the value of dot1dBaseBridgeAddress.
           On bridges supporting IEEE 802.1t or IEEE 802.1w,
           permissible values are 0-61440, in steps of 4096."
       REFERENCE
           "IEEE 802.1D-1998 clause 8.10.2, Table 8-4,
           IEEE 802.1t clause 8.10.2, Table 8-4, clause 14.3."
       ::= { dot1dStp 2 }

   dot1dStpTimeSinceTopologyChange OBJECT-TYPE
       SYNTAX      TimeTicks
       UNITS       "centi-seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The time (in hundredths of a second) since the
           last time a topology change was detected by the
           bridge entity.
           For RSTP, this reports the time since the tcWhile
           timer for any port on this Bridge was nonzero."
       REFERENCE
           "IEEE 802.1D-1998 clause 14.8.1.1.,
           IEEE 802.1w clause 14.8.1.1."
       ::= { dot1dStp 3 }

   dot1dStpTopChanges OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of topology changes detected by
           this bridge since the management entity was last
           reset or initialized."
       REFERENCE
           "IEEE 802.1D-1998 clause 14.8.1.1."
       ::= { dot1dStp 4 }

   dot1dStpDesignatedRoot OBJECT-TYPE
       SYNTAX      BridgeId
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The bridge identifier of the root of the spanning
           tree, as determined by the Spanning Tree Protocol,
           as executed by this node.  This value is used as
           the Root Identifier parameter in all Configuration
           Bridge PDUs originated by this node."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.1"
       ::= { dot1dStp 5 }

   dot1dStpRootCost OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The cost of the path to the root as seen from
           this bridge."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.2"
       ::= { dot1dStp 6 }

   dot1dStpRootPort OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The port number of the port that offers the lowest
           cost path from this bridge to the root bridge."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.3"
       ::= { dot1dStp 7 }

   dot1dStpMaxAge OBJECT-TYPE
       SYNTAX      Timeout
       UNITS       "centi-seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum age of Spanning Tree Protocol information
           learned from the network on any port before it is
           discarded, in units of hundredths of a second.  This is
           the actual value that this bridge is currently using."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.4"
       ::= { dot1dStp 8 }

   dot1dStpHelloTime OBJECT-TYPE
       SYNTAX      Timeout
       UNITS       "centi-seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The amount of time between the transmission of
           Configuration bridge PDUs by this node on any port when
           it is the root of the spanning tree, or trying to become
           so, in units of hundredths of a second.  This is the
           actual value that this bridge is currently using."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.5"
       ::= { dot1dStp 9 }

   dot1dStpHoldTime OBJECT-TYPE
       SYNTAX      Integer32
       UNITS       "centi-seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This time value determines the interval length
           during which no more than two Configuration bridge
           PDUs shall be transmitted by this node, in units
           of hundredths of a second."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.14"
       ::= { dot1dStp 10 }

   dot1dStpForwardDelay OBJECT-TYPE
       SYNTAX      Timeout
       UNITS       "centi-seconds"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This time value, measured in units of hundredths of a
           second, controls how fast a port changes its spanning
           state when moving towards the Forwarding state.  The
           value determines how long the port stays in each of the
           Listening and Learning states, which precede the
           Forwarding state.  This value is also used when a
           topology change has been detected and is underway, to
           age all dynamic entries in the Forwarding Database.
           [Note that this value is the one that this bridge is
           currently using, in contrast to
           dot1dStpBridgeForwardDelay, which is the value that this
           bridge and all others would start using if/when this
           bridge were to become the root.]"
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.6"
       ::= { dot1dStp 11 }

   dot1dStpBridgeMaxAge OBJECT-TYPE
       SYNTAX      Timeout (600..4000)
       UNITS       "centi-seconds"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The value that all bridges use for MaxAge when this
           bridge is acting as the root.  Note that 802.1D-1998
           specifies that the range for this parameter is related
           to the value of dot1dStpBridgeHelloTime.  The
           granularity of this timer is specified by 802.1D-1998 to
           be 1 second.  An agent may return a badValue error if a
           set is attempted to a value that is not a whole number
           of seconds."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.8"
       ::= { dot1dStp 12 }

   dot1dStpBridgeHelloTime OBJECT-TYPE
       SYNTAX      Timeout (100..1000)
       UNITS       "centi-seconds"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The value that all bridges use for HelloTime when this
           bridge is acting as the root.  The granularity of this
           timer is specified by 802.1D-1998 to be 1 second.  An
           agent may return a badValue error if a set is attempted
           to a value that is not a whole number of seconds."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.9"
       ::= { dot1dStp 13 }

   dot1dStpBridgeForwardDelay OBJECT-TYPE
       SYNTAX      Timeout (400..3000)
       UNITS       "centi-seconds"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The value that all bridges use for ForwardDelay when
           this bridge is acting as the root.  Note that
           802.1D-1998 specifies that the range for this parameter
           is related to the value of dot1dStpBridgeMaxAge.  The
           granularity of this timer is specified by 802.1D-1998 to
           be 1 second.  An agent may return a badValue error if a
           set is attempted to a value that is not a whole number
           of seconds."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.3.10"
       ::= { dot1dStp 14 }

   -- ---------------------------------------------------------- --
   -- The Spanning Tree Port Table
   -- ---------------------------------------------------------- --

   dot1dStpPortTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Dot1dStpPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table that contains port-specific information
           for the Spanning Tree Protocol."
       ::= { dot1dStp 15 }

   dot1dStpPortEntry OBJECT-TYPE
       SYNTAX      Dot1dStpPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A list of information maintained by every port about
           the Spanning Tree Protocol state for that port."
       INDEX   { dot1dStpPort }
       ::= { dot1dStpPortTable 1 }

   Dot1dStpPortEntry ::=
       SEQUENCE {
           dot1dStpPort
               Integer32,
           dot1dStpPortPriority
               Integer32,
           dot1dStpPortState
               INTEGER,
           dot1dStpPortEnable
               INTEGER,
           dot1dStpPortPathCost
               Integer32,
           dot1dStpPortDesignatedRoot
               BridgeId,
           dot1dStpPortDesignatedCost
               Integer32,
           dot1dStpPortDesignatedBridge
               BridgeId,
           dot1dStpPortDesignatedPort
               OCTET STRING,
           dot1dStpPortForwardTransitions
               Counter32,
           dot1dStpPortPathCost32
               Integer32
       }

   dot1dStpPort OBJECT-TYPE
       SYNTAX      Integer32 (1..65535)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The port number of the port for which this entry
           contains Spanning Tree Protocol management information."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.8.2.1.2"
       ::= { dot1dStpPortEntry 1 }

   dot1dStpPortPriority OBJECT-TYPE
       SYNTAX      Integer32 (0..255)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The value of the priority field that is contained in
           the first (in network byte order) octet of the (2 octet
           long) Port ID.  The other octet of the Port ID is given
           by the value of dot1dStpPort.
           On bridges supporting IEEE 802.1t or IEEE 802.1w,
           permissible values are 0-240, in steps of 16."
       REFERENCE
           "IEEE 802.1D-1998 clause 8.10.2, Table 8-4,
           IEEE 802.1t clause 8.10.2, Table 8-4, clause 14.3."
       ::= { dot1dStpPortEntry 2 }

   dot1dStpPortState OBJECT-TYPE
       SYNTAX      INTEGER {
                       disabled(1),
                       blocking(2),
                       listening(3),
                       learning(4),
                       forwarding(5),
                       broken(6)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The port's current state, as defined by application of
           the Spanning Tree Protocol.  This state controls what
           action a port takes on reception of a frame.  If the
           bridge has detected a port that is malfunctioning, it
           will place that port into the broken(6) state.  For
           ports that are disabled (see dot1dStpPortEnable), this
           object will have a value of disabled(1)."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.2"
       ::= { dot1dStpPortEntry 3 }

   dot1dStpPortEnable OBJECT-TYPE
       SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                   }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The enabled/disabled status of the port."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.2"
       ::= { dot1dStpPortEntry 4 }

   dot1dStpPortPathCost OBJECT-TYPE
       SYNTAX      Integer32 (1..65535)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The contribution of this port to the path cost of
           paths towards the spanning tree root which include
           this port.  802.1D-1998 recommends that the default
           value of this parameter be in inverse proportion to
           the speed of the attached LAN.

           New implementations should support dot1dStpPortPathCost32.
           If the port path costs exceeds the maximum value of this
           object then this object should report the maximum value,
           namely 65535.  Applications should try to read the
           dot1dStpPortPathCost32 object if this object reports
           the maximum value."
       REFERENCE "IEEE 802.1D-1998: clause 8.5.5.3"
           ::= { dot1dStpPortEntry 5 }

   dot1dStpPortDesignatedRoot OBJECT-TYPE
       SYNTAX      BridgeId
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The unique Bridge Identifier of the Bridge
           recorded as the Root in the Configuration BPDUs
           transmitted by the Designated Bridge for the
           segment to which the port is attached."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.4"
       ::= { dot1dStpPortEntry 6 }

   dot1dStpPortDesignatedCost OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The path cost of the Designated Port of the segment
           connected to this port.  This value is compared to the
           Root Path Cost field in received bridge PDUs."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.5"
       ::= { dot1dStpPortEntry 7 }

   dot1dStpPortDesignatedBridge OBJECT-TYPE
       SYNTAX      BridgeId
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The Bridge Identifier of the bridge that this
           port considers to be the Designated Bridge for
           this port's segment."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.6"
       ::= { dot1dStpPortEntry 8 }

   dot1dStpPortDesignatedPort OBJECT-TYPE
       SYNTAX      OCTET STRING (SIZE (2))
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The Port Identifier of the port on the Designated
           Bridge for this port's segment."
       REFERENCE
           "IEEE 802.1D-1998: clause 8.5.5.7"
       ::= { dot1dStpPortEntry 9 }

   dot1dStpPortForwardTransitions OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of times this port has transitioned
           from the Learning state to the Forwarding state."
       ::= { dot1dStpPortEntry 10 }

   dot1dStpPortPathCost32 OBJECT-TYPE
       SYNTAX      Integer32 (1..200000000)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The contribution of this port to the path cost of
           paths towards the spanning tree root which include
           this port.  802.1D-1998 recommends that the default
           value of this parameter be in inverse proportion to
           the speed of the attached LAN.

           This object replaces dot1dStpPortPathCost to support
           IEEE 802.1t."
       REFERENCE
           "IEEE 802.1t clause 8.10.2, Table 8-5."
       ::= { dot1dStpPortEntry 11 }

   -- ---------------------------------------------------------- --
   -- the dot1dTp subtree
   -- ---------------------------------------------------------- --
   -- Implementation of the dot1dTp subtree is optional.  It is
   -- implemented by those bridges that support the transparent
   -- bridging mode.  A transparent or SRT bridge will implement
   -- this subtree.
   -- ---------------------------------------------------------- --

   dot1dTpLearnedEntryDiscards OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of Forwarding Database entries that
           have been or would have been learned, but have been
           discarded due to a lack of storage space in the
           Forwarding Database.  If this counter is increasing, it
           indicates that the Forwarding Database is regularly
           becoming full (a condition that has unpleasant
           performance effects on the subnetwork).  If this counter
           has a significant value but is not presently increasing,
           it indicates that the problem has been occurring but is
           not persistent."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.7.1.1.3"
       ::= { dot1dTp 1 }

   dot1dTpAgingTime OBJECT-TYPE
       SYNTAX      Integer32 (10..1000000)
       UNITS       "seconds"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The timeout period in seconds for aging out
           dynamically-learned forwarding information.
           802.1D-1998 recommends a default of 300 seconds."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.7.1.1.3"
       ::= { dot1dTp 2 }


   -- ---------------------------------------------------------- --
   --  The Forwarding Database for Transparent Bridges
   -- ---------------------------------------------------------- --

   dot1dTpFdbTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Dot1dTpFdbEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table that contains information about unicast
           entries for which the bridge has forwarding and/or
           filtering information.  This information is used
           by the transparent bridging function in
           determining how to propagate a received frame."
       ::= { dot1dTp 3 }

   dot1dTpFdbEntry OBJECT-TYPE
       SYNTAX      Dot1dTpFdbEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Information about a specific unicast MAC address
           for which the bridge has some forwarding and/or
           filtering information."
       INDEX   { dot1dTpFdbAddress }
       ::= { dot1dTpFdbTable 1 }

   Dot1dTpFdbEntry ::=
       SEQUENCE {
           dot1dTpFdbAddress
               MacAddress,
           dot1dTpFdbPort
               Integer32,
           dot1dTpFdbStatus
               INTEGER
       }

   dot1dTpFdbAddress OBJECT-TYPE
       SYNTAX      MacAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "A unicast MAC address for which the bridge has
           forwarding and/or filtering information."
       REFERENCE
           "IEEE 802.1D-1998: clause 7.9.1, 7.9.2"
       ::= { dot1dTpFdbEntry 1 }

   dot1dTpFdbPort OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Either the value '0', or the port number of the port on
           which a frame having a source address equal to the value
           of the corresponding instance of dot1dTpFdbAddress has
           been seen.  A value of '0' indicates that the port
           number has not been learned, but that the bridge does
           have some forwarding/filtering information about this
           address (e.g., in the dot1dStaticTable).  Implementors
           are encouraged to assign the port value to this object
           whenever it is learned, even for addresses for which the
           corresponding value of dot1dTpFdbStatus is not
           learned(3)."
       ::= { dot1dTpFdbEntry 2 }

   dot1dTpFdbStatus OBJECT-TYPE
       SYNTAX      INTEGER {
                       other(1),
                       invalid(2),
                       learned(3),
                       self(4),
                       mgmt(5)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The status of this entry.  The meanings of the
           values are:
               other(1) - none of the following.  This would
                   include the case where some other MIB object
                   (not the corresponding instance of
                   dot1dTpFdbPort, nor an entry in the
                   dot1dStaticTable) is being used to determine if
                   and how frames addressed to the value of the
                   corresponding instance of dot1dTpFdbAddress are
                   being forwarded.
               invalid(2) - this entry is no longer valid (e.g.,
                   it was learned but has since aged out), but has
                   not yet been flushed from the table.
               learned(3) - the value of the corresponding instance
                   of dot1dTpFdbPort was learned, and is being
                   used.
               self(4) - the value of the corresponding instance of
                   dot1dTpFdbAddress represents one of the bridge's
                   addresses.  The corresponding instance of
                   dot1dTpFdbPort indicates which of the bridge's
                   ports has this address.
               mgmt(5) - the value of the corresponding instance of
                   dot1dTpFdbAddress is also the value of an
                   existing instance of dot1dStaticAddress."
       ::= { dot1dTpFdbEntry 3 }

   -- ---------------------------------------------------------- --
   --  Port Table for Transparent Bridges
   -- ---------------------------------------------------------- --

   dot1dTpPortTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Dot1dTpPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table that contains information about every port that
           is associated with this transparent bridge."
       ::= { dot1dTp 4 }

   dot1dTpPortEntry OBJECT-TYPE
       SYNTAX      Dot1dTpPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A list of information for each port of a transparent
           bridge."
       INDEX   { dot1dTpPort }
       ::= { dot1dTpPortTable 1 }

   Dot1dTpPortEntry ::=
       SEQUENCE {
           dot1dTpPort
               Integer32,
           dot1dTpPortMaxInfo
               Integer32,
           dot1dTpPortInFrames
               Counter32,
           dot1dTpPortOutFrames
               Counter32,
           dot1dTpPortInDiscards
               Counter32
       }

   dot1dTpPort OBJECT-TYPE
       SYNTAX      Integer32 (1..65535)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The port number of the port for which this entry
           contains Transparent bridging management information."
       ::= { dot1dTpPortEntry 1 }

   -- It would be nice if we could use ifMtu as the size of the
   -- largest INFO field, but we can't because ifMtu is defined
   -- to be the size that the (inter-)network layer can use, which
   -- can differ from the MAC layer (especially if several layers
   -- of encapsulation are used).

   dot1dTpPortMaxInfo OBJECT-TYPE
       SYNTAX      Integer32
       UNITS       "bytes"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The maximum size of the INFO (non-MAC) field that
           this port will receive or transmit."
       ::= { dot1dTpPortEntry 2 }

   dot1dTpPortInFrames OBJECT-TYPE
       SYNTAX      Counter32
       UNITS       "frames"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of frames that have been received by this
           port from its segment.  Note that a frame received on the
           interface corresponding to this port is only counted by
           this object if and only if it is for a protocol being
           processed by the local bridging function, including
           bridge management frames."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.6.1.1.3"
       ::= { dot1dTpPortEntry 3 }

   dot1dTpPortOutFrames OBJECT-TYPE
       SYNTAX      Counter32
       UNITS       "frames"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of frames that have been transmitted by this
           port to its segment.  Note that a frame transmitted on
           the interface corresponding to this port is only counted
           by this object if and only if it is for a protocol being
           processed by the local bridging function, including
           bridge management frames."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.6.1.1.3"
       ::= { dot1dTpPortEntry 4 }

   dot1dTpPortInDiscards OBJECT-TYPE
       SYNTAX      Counter32
       UNITS       "frames"
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Count of received valid frames that were discarded
           (i.e., filtered) by the Forwarding Process."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.6.1.1.3"
       ::= { dot1dTpPortEntry 5 }

   -- ---------------------------------------------------------- --
   -- The Static (Destination-Address Filtering) Database
   -- ---------------------------------------------------------- --
   -- Implementation of this subtree is optional.
   -- ---------------------------------------------------------- --

   dot1dStaticTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Dot1dStaticEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table containing filtering information configured
           into the bridge by (local or network) management
           specifying the set of ports to which frames received
           from specific ports and containing specific destination
           addresses are allowed to be forwarded.  The value of
           zero in this table, as the port number from which frames
           with a specific destination address are received, is
           used to specify all ports for which there is no specific
           entry in this table for that particular destination
           address.  Entries are valid for unicast and for
           group/broadcast addresses."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.7.2"
       ::= { dot1dStatic 1 }

   dot1dStaticEntry OBJECT-TYPE
       SYNTAX      Dot1dStaticEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Filtering information configured into the bridge by
           (local or network) management specifying the set of
           ports to which frames received from a specific port and
           containing a specific destination address are allowed to
           be forwarded."
       REFERENCE
           "IEEE 802.1D-1998: clause 14.7.2"
       INDEX   { dot1dStaticAddress, dot1dStaticReceivePort }
       ::= { dot1dStaticTable 1 }

   Dot1dStaticEntry ::=
       SEQUENCE {
           dot1dStaticAddress       MacAddress,
           dot1dStaticReceivePort   Integer32,
           dot1dStaticAllowedToGoTo OCTET STRING,
           dot1dStaticStatus        INTEGER
       }

   dot1dStaticAddress OBJECT-TYPE
       SYNTAX      MacAddress
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The destination MAC address in a frame to which this
           entry's filtering information applies.  This object can
           take the value of a unicast address, a group address, or
           the broadcast address."
       REFERENCE
           "IEEE 802.1D-1998: clause 7.9.1, 7.9.2"
       ::= { dot1dStaticEntry 1 }

   dot1dStaticReceivePort OBJECT-TYPE
       SYNTAX      Integer32 (0..65535)
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "Either the value '0', or the port number of the port
           from which a frame must be received in order for this
           entry's filtering information to apply.  A value of zero
           indicates that this entry applies on all ports of the
           bridge for which there is no other applicable entry."
       ::= { dot1dStaticEntry 2 }

   dot1dStaticAllowedToGoTo OBJECT-TYPE
       SYNTAX      OCTET STRING (SIZE (0..512))
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The set of ports to which frames received from a
           specific port and destined for a specific MAC address,
           are allowed to be forwarded.  Each octet within the
           value of this object specifies a set of eight ports,
           with the first octet specifying ports 1 through 8, the
           second octet specifying ports 9 through 16, etc.  Within
           each octet, the most significant bit represents the
           lowest numbered port, and the least significant bit
           represents the highest numbered port.  Thus, each port
           of the bridge is represented by a single bit within the
           value of this object.  If that bit has a value of '1',
           then that port is included in the set of ports; the port
           is not included if its bit has a value of '0'.  (Note
           that the setting of the bit corresponding to the port
           from which a frame is received is irrelevant.)  The
           default value of this object is a string of ones of
           appropriate length.
           The value of this object may exceed the required minimum
           maximum message size of some SNMP transport (484 bytes,
           in the case of SNMP over UDP, see RFC 3417, section 3.2).
           SNMP engines on bridges supporting a large number of
           ports must support appropriate maximum message sizes."
       ::= { dot1dStaticEntry 3 }

   dot1dStaticStatus OBJECT-TYPE
       SYNTAX      INTEGER {
                       other(1),
                       invalid(2),
                       permanent(3),
                       deleteOnReset(4),
                       deleteOnTimeout(5)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object indicates the status of this entry.
           The default value is permanent(3).
               other(1) - this entry is currently in use but the
                   conditions under which it will remain so are
                   different from each of the following values.
               invalid(2) - writing this value to the object
                   removes the corresponding entry.
               permanent(3) - this entry is currently in use and
                   will remain so after the next reset of the
                   bridge.
               deleteOnReset(4) - this entry is currently in use
                   and will remain so until the next reset of the
                   bridge.
               deleteOnTimeout(5) - this entry is currently in use
                   and will remain so until it is aged out."
       ::= { dot1dStaticEntry 4 }

   -- ---------------------------------------------------------- --
   -- Notifications for use by Bridges
   -- ---------------------------------------------------------- --
   -- Notifications for the Spanning Tree Protocol
   -- ---------------------------------------------------------- --

   newRoot NOTIFICATION-TYPE
       -- OBJECTS     { }
       STATUS      current
       DESCRIPTION
           "The newRoot trap indicates that the sending agent has
           become the new root of the Spanning Tree; the trap is
           sent by a bridge soon after its election as the new
           root, e.g., upon expiration of the Topology Change Timer,
           immediately subsequent to its election.  Implementation
           of this trap is optional."
       ::= { dot1dNotifications 1 }

   topologyChange NOTIFICATION-TYPE
       -- OBJECTS     { }
       STATUS      current
       DESCRIPTION
           "A topologyChange trap is sent by a bridge when any of
           its configured ports transitions from the Learning state
           to the Forwarding state, or from the Forwarding state to
           the Blocking state.  The trap is not sent if a newRoot
           trap is sent for the same transition.  Implementation of
           this trap is optional."
       ::= { dot1dNotifications 2 }

   -- ---------------------------------------------------------- --
   -- IEEE 802.1D MIB - Conformance Information
   -- ---------------------------------------------------------- --

   dot1dGroups         OBJECT IDENTIFIER ::= { dot1dConformance 1 }
   dot1dCompliances    OBJECT IDENTIFIER ::= { dot1dConformance 2 }

   -- ---------------------------------------------------------- --
   -- units of conformance
   -- ---------------------------------------------------------- --

   -- ---------------------------------------------------------- --
   -- the dot1dBase group
   -- ---------------------------------------------------------- --

   dot1dBaseBridgeGroup OBJECT-GROUP
       OBJECTS {
           dot1dBaseBridgeAddress,
           dot1dBaseNumPorts,
           dot1dBaseType
       }
       STATUS      current
       DESCRIPTION
           "Bridge level information for this device."
       ::= { dot1dGroups 1 }

   dot1dBasePortGroup OBJECT-GROUP
       OBJECTS {
           dot1dBasePort,
           dot1dBasePortIfIndex,
           dot1dBasePortCircuit,
           dot1dBasePortDelayExceededDiscards,
           dot1dBasePortMtuExceededDiscards
       }
       STATUS      current
       DESCRIPTION
           "Information for each port on this device."
       ::= { dot1dGroups 2 }

   -- ---------------------------------------------------------- --
   -- the dot1dStp group
   -- ---------------------------------------------------------- --

   dot1dStpBridgeGroup OBJECT-GROUP
       OBJECTS {
           dot1dStpProtocolSpecification,
           dot1dStpPriority,
           dot1dStpTimeSinceTopologyChange,
           dot1dStpTopChanges,
           dot1dStpDesignatedRoot,
           dot1dStpRootCost,
           dot1dStpRootPort,
           dot1dStpMaxAge,
           dot1dStpHelloTime,
           dot1dStpHoldTime,
           dot1dStpForwardDelay,
           dot1dStpBridgeMaxAge,
           dot1dStpBridgeHelloTime,
           dot1dStpBridgeForwardDelay
       }
       STATUS      current
       DESCRIPTION
           "Bridge level Spanning Tree data for this device."
       ::= { dot1dGroups 3 }

   dot1dStpPortGroup OBJECT-GROUP
       OBJECTS {
           dot1dStpPort,
           dot1dStpPortPriority,
           dot1dStpPortState,
           dot1dStpPortEnable,
           dot1dStpPortPathCost,
           dot1dStpPortDesignatedRoot,
           dot1dStpPortDesignatedCost,
           dot1dStpPortDesignatedBridge,
           dot1dStpPortDesignatedPort,
           dot1dStpPortForwardTransitions
       }
       STATUS      current
       DESCRIPTION
           "Spanning Tree data for each port on this device."
       ::= { dot1dGroups 4 }

   dot1dStpPortGroup2 OBJECT-GROUP
       OBJECTS {
           dot1dStpPort,
           dot1dStpPortPriority,
           dot1dStpPortState,
           dot1dStpPortEnable,
           dot1dStpPortDesignatedRoot,
           dot1dStpPortDesignatedCost,
           dot1dStpPortDesignatedBridge,
           dot1dStpPortDesignatedPort,
           dot1dStpPortForwardTransitions,
           dot1dStpPortPathCost32
       }
       STATUS      current
       DESCRIPTION
           "Spanning Tree data for each port on this device."
       ::= { dot1dGroups 5 }

   dot1dStpPortGroup3 OBJECT-GROUP
       OBJECTS {
           dot1dStpPortPathCost32
       }
       STATUS      current
       DESCRIPTION
           "Spanning Tree data for devices supporting 32-bit
            path costs."
       ::= { dot1dGroups 6 }

   -- ---------------------------------------------------------- --
   -- the dot1dTp group
   -- ---------------------------------------------------------- --

   dot1dTpBridgeGroup OBJECT-GROUP
       OBJECTS {
           dot1dTpLearnedEntryDiscards,
           dot1dTpAgingTime
       }
       STATUS      current
       DESCRIPTION
           "Bridge level Transparent Bridging data."
       ::= { dot1dGroups 7 }

   dot1dTpFdbGroup OBJECT-GROUP
       OBJECTS {
           dot1dTpFdbAddress,
           dot1dTpFdbPort,
           dot1dTpFdbStatus
       }

       STATUS      current
       DESCRIPTION
           "Filtering Database information for the Bridge."
       ::= { dot1dGroups 8 }

   dot1dTpGroup OBJECT-GROUP
       OBJECTS {
           dot1dTpPort,
           dot1dTpPortMaxInfo,
           dot1dTpPortInFrames,
           dot1dTpPortOutFrames,
           dot1dTpPortInDiscards
       }
       STATUS      current
       DESCRIPTION
           "Dynamic Filtering Database information for each port of
           the Bridge."
       ::= { dot1dGroups 9 }

   -- ---------------------------------------------------------- --
   -- The Static (Destination-Address Filtering) Database
   -- ---------------------------------------------------------- --

   dot1dStaticGroup OBJECT-GROUP
       OBJECTS {
           dot1dStaticAddress,
           dot1dStaticReceivePort,
           dot1dStaticAllowedToGoTo,
           dot1dStaticStatus
       }
       STATUS      current
       DESCRIPTION
           "Static Filtering Database information for each port of
           the Bridge."
       ::= { dot1dGroups 10 }

   -- ---------------------------------------------------------- --
   -- The Trap Notification Group
   -- ---------------------------------------------------------- --

   dot1dNotificationGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           newRoot,
           topologyChange
       }
       STATUS      current
       DESCRIPTION
           "Group of objects describing notifications (traps)."
       ::= { dot1dGroups 11 }

   -- ---------------------------------------------------------- --
   -- compliance statements
   -- ---------------------------------------------------------- --

   bridgeCompliance1493 MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for device support of bridging
           services, as per RFC1493."

       MODULE
           MANDATORY-GROUPS {
               dot1dBaseBridgeGroup,
               dot1dBasePortGroup
           }

       GROUP   dot1dStpBridgeGroup
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
           that support the Spanning Tree Protocol."

       GROUP   dot1dStpPortGroup
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
           that support the Spanning Tree Protocol."

       GROUP   dot1dTpBridgeGroup
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
           that support the transparent bridging mode.  A
           transparent or SRT bridge will implement this group."

       GROUP   dot1dTpFdbGroup
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
           that support the transparent bridging mode.  A
           transparent or SRT bridge will implement this group."

       GROUP   dot1dTpGroup
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
           that support the transparent bridging mode.  A
           transparent or SRT bridge will implement this group."

       GROUP   dot1dStaticGroup
       DESCRIPTION
           "Implementation of this group is optional."

       GROUP dot1dNotificationGroup
       DESCRIPTION
           "Implementation of this group is optional."
       ::= { dot1dCompliances 1 }

   bridgeCompliance4188 MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for device support of bridging
           services.  This supports 32-bit Path Cost values and the
           more restricted bridge and port priorities, as per IEEE
           802.1t.

           Full support for the 802.1D management objects requires that
           the SNMPv2-MIB [RFC3418] objects sysDescr, and sysUpTime, as
           well as the IF-MIB [RFC2863] objects ifIndex, ifType,
           ifDescr, ifPhysAddress, and ifLastChange are implemented."

       MODULE
           MANDATORY-GROUPS {
               dot1dBaseBridgeGroup,
               dot1dBasePortGroup
           }

       GROUP   dot1dStpBridgeGroup
       DESCRIPTION
           "Implementation of this group is mandatory for
           bridges that support the Spanning Tree Protocol."

       OBJECT dot1dStpPriority
       SYNTAX Integer32 (0|4096|8192|12288|16384|20480|24576
                        |28672|32768|36864|40960|45056|49152
                        |53248|57344|61440)
       DESCRIPTION
           "The possible values defined by IEEE 802.1t."

       GROUP   dot1dStpPortGroup2
       DESCRIPTION
           "Implementation of this group is mandatory for
           bridges that support the Spanning Tree Protocol."

       GROUP   dot1dStpPortGroup3
       DESCRIPTION
           "Implementation of this group is mandatory for bridges
            that support the Spanning Tree Protocol and 32-bit path
            costs.  In particular, this includes devices supporting
            IEEE 802.1t and IEEE 802.1w."

       OBJECT dot1dStpPortPriority
       SYNTAX Integer32 (0|16|32|48|64|80|96|112|128
                        |144|160|176|192|208|224|240)
       DESCRIPTION
           "The possible values defined by IEEE 802.1t."

       GROUP   dot1dTpBridgeGroup
       DESCRIPTION
           "Implementation of this group is mandatory for
           bridges that support the transparent bridging
           mode.  A transparent or SRT bridge will implement
           this group."

       GROUP   dot1dTpFdbGroup
       DESCRIPTION
           "Implementation of this group is mandatory for
           bridges that support the transparent bridging
           mode.  A transparent or SRT bridge will implement
           this group."

       GROUP   dot1dTpGroup
       DESCRIPTION
           "Implementation of this group is mandatory for
           bridges that support the transparent bridging
           mode.  A transparent or SRT bridge will implement
           this group."

       GROUP   dot1dStaticGroup
       DESCRIPTION
           "Implementation of this group is optional."

       GROUP dot1dNotificationGroup
       DESCRIPTION
           "Implementation of this group is optional."

       ::= { dot1dCompliances 2 }

   END

-- 
--    Copyright (C) The Internet Society (2005).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 

