-- extracted from rfc4983.txt
-- at Thu Aug 23 06:08:58 2007

T11-FC-RSCN-MIB DEFINITIONS ::= BEGIN

-- The Fibre Channel RSCN MIB
--
-- for the monitoring of registrations by Nx_Ports to receive
-- Registered State Change Notifications (RSCNs), and the
-- monitoring of RSCN usage.
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Counter32, mib-2                     FROM SNMPv2-SMI   -- [RFC2578]
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP                   FROM SNMPv2-CONF  -- [RFC2580]
    TruthValue                           FROM SNMPv2-TC    -- [RFC2579]
    fcmInstanceIndex, fcmSwitchIndex,
    FcNameIdOrZero, FcAddressIdOrZero    FROM FC-MGMT-MIB  -- [RFC4044]
    T11NsGs4RejectReasonCode   FROM T11-FC-NAME-SERVER-MIB -- [RFC4438]
    T11FabricIndex                       FROM T11-TC-MIB;  -- [RFC4439]

t11FcRscnMIB  MODULE-IDENTITY
    LAST-UPDATED "200701080000Z"
    ORGANIZATION "For the initial versions, T11.
                  For later versions, the IETF's IMSS Working Group."
    CONTACT-INFO
            "     Claudio DeSanti
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  EMail: cds@cisco.com

                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  EMail: kzm@cisco.com"

    DESCRIPTION
           "The MIB module for the management of registrations
           by Nx_Ports to receive RSCNs (Registered State Change
           Notifications) on a Fibre Channel Fabric, as defined
           in FC-LS, and for the monitoring of RSCNs sent/received
           or rejected in a Fibre Channel Fabric.

           Copyright (C) The Internet Society (2007).  This version of
           this MIB module is part of RFC 4983;  see the RFC itself for
           full legal notices."
    REVISION    "200701080000Z"
    DESCRIPTION
           "Initial version of this MIB module, published as RFC 4983."
    ::= { mib-2 161 }

t11FcRscnNotifications  OBJECT IDENTIFIER ::= { t11FcRscnMIB 0 }
t11FcRscnObjects        OBJECT IDENTIFIER ::= { t11FcRscnMIB 1 }
t11FcRscnConformance    OBJECT IDENTIFIER ::= { t11FcRscnMIB 2 }
t11FcRscnRegistrations  OBJECT IDENTIFIER ::= { t11FcRscnObjects 1 }
t11FcRscnStats          OBJECT IDENTIFIER ::= { t11FcRscnObjects 2 }
t11FcRscnInformation    OBJECT IDENTIFIER ::= { t11FcRscnObjects 3 }


-- State Change Registration Table

t11FcRscnRegTable  OBJECT-TYPE
    SYNTAX         SEQUENCE OF T11FcRscnRegEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
           "A table of Nx_Ports that have registered to receive
           RSCNs on all Fabrics configured on one or more Fibre
           Channel switches."
    ::= { t11FcRscnRegistrations 1 }

t11FcRscnRegEntry  OBJECT-TYPE
    SYNTAX        T11FcRscnRegEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry containing information about one Nx_Port that
           has registered with a particular switch (identified by
           values of fcmInstanceIndex and fcmSwitchIndex) for a
           particular Fabric (identified by a t11FcRscnFabricIndex
           value)."
    INDEX   { fcmInstanceIndex, fcmSwitchIndex, t11FcRscnFabricIndex,
              t11FcRscnRegFcId }
    ::= { t11FcRscnRegTable 1 }

T11FcRscnRegEntry ::= SEQUENCE {
    t11FcRscnFabricIndex         T11FabricIndex,
    t11FcRscnRegFcId             FcAddressIdOrZero,
    t11FcRscnRegType             BITS
}

t11FcRscnFabricIndex OBJECT-TYPE
    SYNTAX      T11FabricIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
           "An index value that uniquely identifies a particular
           Fabric.

           In a Fabric conformant to FC-SW-4, multiple Virtual Fabrics
           can operate within one (or more) physical infrastructures.
           In such a case, this index value is used to uniquely
           identify a particular Fabric within a physical
           infrastructure.

           In a Fabric that has (or can have) only a single Fabric
           operating within the physical infrastructure, the
           value of this Fabric Index will always be 1."
    REFERENCE
          "ANSI INCITS 418-2006, Fibre Channel - Switch Fabric - 4
          (FC-SW-4), December 2006."
    ::= { t11FcRscnRegEntry 1 }

t11FcRscnRegFcId  OBJECT-TYPE
    SYNTAX        FcAddressIdOrZero (SIZE (3))
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "The Fibre Channel Address Identifier of the
           registering Nx_Port."
    ::= { t11FcRscnRegEntry 2 }

t11FcRscnRegType  OBJECT-TYPE
    SYNTAX        BITS {
                      fromFabricController(0),
                      fromNxPort(1)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "This object indicates the type of registration
           desired by the registering Nx_Port, one bit per type:

           'fromFabricController' -- RSCNs generated for events
                                  detected by the Fabric Controller.

           'fromNxPorts'          -- RSCNs generated for events
                                  detected by the affected Nx_Port."
    REFERENCE
          "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 40."
    ::= { t11FcRscnRegEntry 3 }


-- Statistics

t11FcRscnStatsTable  OBJECT-TYPE
    SYNTAX         SEQUENCE OF T11FcRscnStatsEntry
    MAX-ACCESS     not-accessible
    STATUS         current
    DESCRIPTION
           "The RSCN-related statistics on all Fabrics configured
           on one or more Fibre Channel switches.

           Two levels of statistics are included:

              1) counters at the message-type level, for:
                 - the number of SCRs received/rejected,
                 - the number of RSCNs sent/received/rejected,
                 - the number of SW_RSCNs sent/received/rejected.

              2) counters of sent/received RSCNs per 'Event
                 Qualifier' value.  Note that if and when several
                 RSCN events are coalesced into a single RSCN
                 message, then that message may be counted in
                 more than one of these counters."
    ::= { t11FcRscnStats 1 }

t11FcRscnStatsEntry  OBJECT-TYPE
    SYNTAX        T11FcRscnStatsEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry containing statistics for a particular Fabric
           (identified by a t11FcRscnFabricIndex value) on a particular
           switch (identified by values of fcmInstanceIndex and
           fcmSwitchIndex)."
    INDEX  { fcmInstanceIndex, fcmSwitchIndex, t11FcRscnFabricIndex }
    ::= { t11FcRscnStatsTable 1 }

T11FcRscnStatsEntry ::= SEQUENCE {
    t11FcRscnInScrs                    Counter32,
    t11FcRscnInRscns                   Counter32,
    t11FcRscnOutRscns                  Counter32,
    t11FcRscnInSwRscns                 Counter32,
    t11FcRscnOutSwRscns                Counter32,
    t11FcRscnScrRejects                Counter32,
    t11FcRscnRscnRejects               Counter32,
    t11FcRscnSwRscnRejects             Counter32,
    t11FcRscnInUnspecifiedRscns        Counter32,
    t11FcRscnOutUnspecifiedRscns       Counter32,
    t11FcRscnInChangedAttribRscns      Counter32,
    t11FcRscnOutChangedAttribRscns     Counter32,
    t11FcRscnInChangedServiceRscns     Counter32,
    t11FcRscnOutChangedServiceRscns    Counter32,
    t11FcRscnInChangedSwitchRscns      Counter32,
    t11FcRscnOutChangedSwitchRscns     Counter32,
    t11FcRscnInRemovedRscns            Counter32,
    t11FcRscnOutRemovedRscns           Counter32
}

t11FcRscnInScrs  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of SCRs received from Nx_Ports
           by this switch on this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 1 }


t11FcRscnInRscns  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of RSCNs received from Nx_Ports
           by this switch on this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 2 }

t11FcRscnOutRscns  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of RSCNs transmitted to Nx_Ports
           by this switch on this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 3 }


t11FcRscnInSwRscns  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of SW_RSCNs received by this switch from
           other switches on this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 4 }

t11FcRscnOutSwRscns  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of SW_RSCNs transmitted by this switch
           from other switches on this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 5 }

t11FcRscnScrRejects  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of SCRs rejected by this switch on
           this Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 6 }

t11FcRscnRscnRejects OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of RSCNs rejected by this switch on this
           Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 7 }

t11FcRscnSwRscnRejects  OBJECT-TYPE
    SYNTAX         Counter32
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
           "The number of SW_RSCN rejected by this switch on this
           Fabric.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    ::= { t11FcRscnStatsEntry 8 }

t11FcRscnInUnspecifiedRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) received by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0000'b
           meaning 'Event is not specified'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 9 }

t11FcRscnOutUnspecifiedRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) sent by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0000'b
           meaning 'Event is not specified'.
           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 10 }

t11FcRscnInChangedAttribRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) received by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0002'b
           meaning 'Changed Port Attribute'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 11 }

t11FcRscnOutChangedAttribRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) sent by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0002'b
           meaning 'Changed Port Attribute'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 12 }

t11FcRscnInChangedServiceRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) received by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0003'b
           meaning 'Changed Service Object'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 13 }

t11FcRscnOutChangedServiceRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) sent by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0003'b
           meaning 'Changed Service Object'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 14 }

t11FcRscnInChangedSwitchRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) received by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0004'b
           meaning 'Changed Switch Configuration'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 15 }

t11FcRscnOutChangedSwitchRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) sent by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0004'b
           meaning 'Changed Switch Configuration'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 16 }

t11FcRscnInRemovedRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) received by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0005'b
           meaning 'Removed Object'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 17 }

t11FcRscnOutRemovedRscns  OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The number of Registered State Change Notifications
           (RSCNs) sent by this switch on this Fabric which
           contained an RSCN Event Qualifier value of '0005'b
           meaning 'Removed Object'.

           This counter has no discontinuities other than
           those that all Counter32s have when sysUpTime=0."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
          (FC-LS), July 2007, Table 36."
    ::= { t11FcRscnStatsEntry 18 }

--
-- Notification Control Table
--
t11FcRscnNotifyControlTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcRscnNotifyControlEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A table of control information for notifications
           generated due to the rejection of an SCR or RSCN."
    ::= { t11FcRscnInformation 1 }

t11FcRscnNotifyControlEntry OBJECT-TYPE
    SYNTAX       T11FcRscnNotifyControlEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Each entry contains notification control information
           concerning the rejection of RSCN/SCRs for a particular
           Fabric (identified by the value of t11FcRscnFabricIndex)
           by a particular switch (identified by values of
           fcmInstanceIndex and fcmSwitchIndex)."
    INDEX  { fcmInstanceIndex, fcmSwitchIndex, t11FcRscnFabricIndex }
    ::= { t11FcRscnNotifyControlTable 1 }

T11FcRscnNotifyControlEntry ::= SEQUENCE {
     t11FcRscnIlsRejectNotifyEnable     TruthValue,
     t11FcRscnElsRejectNotifyEnable     TruthValue,
     t11FcRscnRejectedRequestString     OCTET STRING,
     t11FcRscnRejectedRequestSource     FcNameIdOrZero,
     t11FcRscnRejectReasonCode          T11NsGs4RejectReasonCode,
     t11FcRscnRejectReasonCodeExp       OCTET STRING,
     t11FcRscnRejectReasonVendorCode    OCTET STRING
}

t11FcRscnIlsRejectNotifyEnable OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "This object specifies if a t11FcRscnIlsRejectReqNotify
           notification should be generated when this switch
           rejects an SW_RSCN on this Fabric.

           Values written to this object should be retained
           over agent reboots."
    DEFVAL { false }
    ::= { t11FcRscnNotifyControlEntry 1 }

t11FcRscnElsRejectNotifyEnable OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
           "This object specifies if a t11FcRscnElsRejectReqNotify
           notification should be generated when this switch
           rejects an RSCN or SCR on this Fabric.

           Values written to this object should be retained
           over agent reboots."
    DEFVAL { false }
    ::= { t11FcRscnNotifyControlEntry 2 }

t11FcRscnRejectedRequestString OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The binary content of the RSCN, SCR, or SW_RSCN that
           was most recently rejected by this switch on this Fabric.
           The value is formatted as an octet string (in network
           byte order) as described in the relevant Fibre Channel
           standard, containing the payload (which is typically a
           list of affected ports and error codes) of the rejected
           RSCN or SCR as described in FC-LS, or the rejected
           SW_RSCN as described in FC-SW-4.

           This object contains the zero-length string if and when
           the RSCN/SCR/SW_RSCN payload is unavailable.  When the
           length of this object is 255 octets, it contains the
           first 255 octets of the payload (in network byte order)."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
           (FC-LS), July 2007, Tables 34 & 39.

           ANSI INCITS 418-2006, Fibre Channel - Switch Fabric - 4
           (FC-SW-4), December 2006, Table 45."
    ::= { t11FcRscnNotifyControlEntry 3 }

t11FcRscnRejectedRequestSource OBJECT-TYPE
    SYNTAX       FcNameIdOrZero
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The WWN that was the source of the RSCN, SCR, or
           SW_RSCN that was most recently rejected by this switch
           on this Fabric."
    ::= { t11FcRscnNotifyControlEntry 4 }

t11FcRscnRejectReasonCode OBJECT-TYPE
    SYNTAX        T11NsGs4RejectReasonCode
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "This object contains the Reason Code of the most recent
           rejection by this switch of an RSCN, SCR or SW_RSCN on
           this Fabric."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
           (FC-LS), July 2007, Table 146.

           ANSI INCITS 418-2006, Fibre Channel - Switch Fabric - 4
           (FC-SW-4), December 2006, Table 5."
    ::= { t11FcRscnNotifyControlEntry 5 }

t11FcRscnRejectReasonCodeExp OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(1))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "This object contains the Reason Code Explanation
           of the most recent rejection by this switch of an
           RSCN, SCR or SW_RSCN on this Fabric."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
           (FC-LS), July 2007, Table 147.

           ANSI INCITS 418-2006, Fibre Channel - Switch Fabric - 4
           (FC-SW-4), December 2006, Table 6."
    ::= { t11FcRscnNotifyControlEntry 6 }

t11FcRscnRejectReasonVendorCode OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(1))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "This object contains the Reason Vendor Specific
           Code of the most recent rejection by this switch
           of an RSCN, SCR or SW_RSCN on this Fabric."
    REFERENCE
           "ANSI INCITS 433-2007, Fibre Channel - Link Services
           (FC-LS), July 2007, Table 148.

           ANSI INCITS 418-2006, Fibre Channel - Switch Fabric - 4
           (FC-SW-4), December 2006, Section 6.1.3."
    ::= { t11FcRscnNotifyControlEntry 7 }


-- Notifications

t11FcRscnElsRejectReqNotify NOTIFICATION-TYPE
    OBJECTS { t11FcRscnRejectedRequestString,
              t11FcRscnRejectedRequestSource,
              t11FcRscnRejectReasonCode,
              t11FcRscnRejectReasonCodeExp,
              t11FcRscnRejectReasonVendorCode }
    STATUS  current
    DESCRIPTION
           "This notification is generated when a switch rejects
           an SCR or RSCN.

           The value of t11FcRscnRejectedRequestString indicates the
           binary content of the rejected request if available, or
           the zero-length string otherwise.  The source of the
           rejected request is given by t11FcRscnRejectedRequestSource,
           and the reason for rejection is given by the values of
           t11FcRscnRejectReasonCode, t11FcRscnRejectReasonCodeExp
           and t11FcRscnRejectReasonVendorCode."
    ::= { t11FcRscnNotifications 1 }

t11FcRscnIlsRejectReqNotify NOTIFICATION-TYPE
    OBJECTS { t11FcRscnRejectedRequestString,
              t11FcRscnRejectedRequestSource,
              t11FcRscnRejectReasonCode,
              t11FcRscnRejectReasonCodeExp,
              t11FcRscnRejectReasonVendorCode }
    STATUS  current
    DESCRIPTION
           "This notification is generated when a switch rejects
           an SW_RSCN.

           The value of t11FcRscnRejectedRequestString indicates the
           binary content of the rejected request if available, or
           the zero-length string otherwise.  The source of the
           rejected request is given by t11FcRscnRejectedRequestSource,
           and the reason for rejection is given by the values of
           t11FcRscnRejectReasonCode, t11FcRscnRejectReasonCodeExp
           and t11FcRscnRejectReasonVendorCode."
    ::= { t11FcRscnNotifications 2 }

-- Conformance
t11FcRscnCompliances OBJECT IDENTIFIER ::= { t11FcRscnConformance 1 }
t11FcRscnGroups      OBJECT IDENTIFIER ::= { t11FcRscnConformance 2 }
t11FcRscnCompliance MODULE-COMPLIANCE
    STATUS    current
    DESCRIPTION
           "The compliance statement for entities that implement
           this MIB."
    MODULE
        MANDATORY-GROUPS { t11FcRscnRegistrationGroup,
                           t11FcRscnNotifyControlGroup,
                           t11FcRscnNotifyGroup }

    GROUP   t11FcRscnStatsGroup
    DESCRIPTION
            "These counters, containing RSCN-related statistics, are
            mandatory only for those systems that count such events."

    OBJECT       t11FcRscnIlsRejectNotifyEnable
    MIN-ACCESS   read-only
    DESCRIPTION
            "Write access is not required."

    OBJECT       t11FcRscnElsRejectNotifyEnable
    MIN-ACCESS   read-only
    DESCRIPTION
            "Write access is not required."

    ::= { t11FcRscnCompliances 1 }


-- Units of conformance

t11FcRscnRegistrationGroup  OBJECT-GROUP
    OBJECTS { t11FcRscnRegType }
    STATUS  current
    DESCRIPTION
           "A collection of objects for monitoring RSCN
           registrations."
    ::= { t11FcRscnGroups 1 }

t11FcRscnStatsGroup   OBJECT-GROUP
    OBJECTS { t11FcRscnInScrs,
              t11FcRscnInRscns,
              t11FcRscnOutRscns,
              t11FcRscnInSwRscns,
              t11FcRscnOutSwRscns,
              t11FcRscnScrRejects,
              t11FcRscnRscnRejects,
              t11FcRscnSwRscnRejects,
              t11FcRscnInUnspecifiedRscns,
              t11FcRscnOutUnspecifiedRscns,
              t11FcRscnInChangedAttribRscns,
              t11FcRscnOutChangedAttribRscns,
              t11FcRscnInChangedServiceRscns,
              t11FcRscnOutChangedServiceRscns,
              t11FcRscnInChangedSwitchRscns,
              t11FcRscnOutChangedSwitchRscns,
              t11FcRscnInRemovedRscns,
              t11FcRscnOutRemovedRscns
            }
    STATUS  current
    DESCRIPTION
           "A collection of objects for collecting RSCN-related
           statistics."
    ::= { t11FcRscnGroups 2 }

t11FcRscnNotifyControlGroup  OBJECT-GROUP
    OBJECTS { t11FcRscnIlsRejectNotifyEnable,
              t11FcRscnElsRejectNotifyEnable,
              t11FcRscnRejectedRequestString,
              t11FcRscnRejectedRequestSource,
              t11FcRscnRejectReasonCode,
              t11FcRscnRejectReasonCodeExp,
              t11FcRscnRejectReasonVendorCode
            }
    STATUS  current
    DESCRIPTION
           "A collection of notification control and
           notification information objects."
    ::= { t11FcRscnGroups 3 }

t11FcRscnNotifyGroup   NOTIFICATION-GROUP
    NOTIFICATIONS { t11FcRscnIlsRejectReqNotify,
                    t11FcRscnElsRejectReqNotify
                  }
    STATUS        current
    DESCRIPTION
           "A collection of notifications for monitoring
           ILS and ELS rejections by the RSCN module."
    ::= { t11FcRscnGroups 4 }

END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.

