-- extracted from rfc4780.txt
-- at Tue May  1 06:08:36 2007

SIP-TC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    mib-2
          FROM SNMPv2-SMI        -- RFC 2578

    TEXTUAL-CONVENTION
          FROM SNMPv2-TC;        -- RFC 2579

sipTC MODULE-IDENTITY
    LAST-UPDATED "200704200000Z"
    ORGANIZATION "IETF Session Initiation Protocol Working Group"
    CONTACT-INFO
             "SIP WG email: sip@ietf.org

              Co-editor  Kevin Lingle
                         Cisco Systems, Inc.
              postal:    7025 Kit Creek Road
                         P.O. Box 14987
                         Research Triangle Park, NC 27709
                         USA
              email:     klingle@cisco.com
              phone:     +1 919 476 2029

              Co-editor  Joon Maeng
              email:     jmaeng@austin.rr.com

              Co-editor  Jean-Francois Mule
                         CableLabs
              postal:    858 Coal Creek Circle
                         Louisville, CO 80027
                         USA
              email:     jf.mule@cablelabs.com
              phone:     +1 303 661 9100

              Co-editor  Dave Walker
              email:     drwalker@rogers.com"
    DESCRIPTION
       "Session Initiation Protocol (SIP) MIB TEXTUAL-CONVENTION
        module used by other SIP-related MIB Modules.

        Copyright (C) The IETF Trust (2007).  This version of
        this MIB module is part of RFC 4780; see the RFC itself for
        full legal notices."
    REVISION     "200704200000Z"
    DESCRIPTION
       "Initial version of the IETF SIP-TC-MIB module.  This version
        published as part of RFC 4780."
     ::= { mib-2 148 }

--
-- Textual Conventions
--

SipTCTransportProtocol ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "This convention is a bit map.  Each bit represents a transport
        protocol.  If a bit has value 1, then that selected transport
        protocol is in some way dependent on the context of the object
        using this convention.  If a bit has value 0, then that
        transport protocol is not selected.  Combinations of bits can
        be set when multiple transport protocols are selected.

        bit 0: a protocol other than those defined here
        bit 1: User Datagram Protocol
        bit 2: Transmission Control Protocol
        bit 3: Stream Control Transmission Protocol
        bit 4: Transport Layer Security Protocol over TCP
        bit 5: Transport Layer Security Protocol over SCTP
       "
    REFERENCE "RFC 3261, Section 18 and RFC 4168"
    SYNTAX      BITS {
                  other(0),  -- none of the following
                  udp(1),
                  tcp(2),
                  sctp(3),   -- RFC4168
                  tlsTcp(4),
                  tlsSctp(5) -- RFC 4168
                }

SipTCEntityRole ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "This convention defines the role of a SIP entity.  Examples of
        SIP entities are proxies, user agents, redirect servers,
        registrars, or combinations of the above.

        User Agent (UA): A logical entity that can act as both a user
        agent client and user agent server.
        User Agent Client (UAC): A logical entity that creates a new
        request, and then uses the client transaction state machinery
        to send it.  The role of UAC lasts only for the duration of
        that transaction.  In other words, if a piece of software
        initiates a request, it acts as a UAC for the duration of that
        transaction.  If it receives a request later, it assumes the
        role of a user agent server for the processing of that
        transaction.

        User Agent Server (UAS): A logical entity that generates a
        response to a SIP request.  The response accepts, rejects,
        or redirects the request.  This role lasts only for the
        duration of that transaction.  In other words, if a piece of
        software responds to a request, it acts as a UAS for the
        duration of that transaction.  If it generates a request
        later, it assumes the role of a user agent client for the
        processing of that transaction.

        Proxy, Proxy Server: An intermediary entity that acts as both
        a server and a client for the purpose of making requests on
        behalf of other clients.  A proxy server primarily plays the
        role of routing, which means its job is to ensure that a
        request is sent to another entity 'closer' to the targeted
        user.  Proxies are also useful for enforcing policy.  A proxy
        interprets and, if necessary, rewrites specific parts of a
        request message before forwarding it.

        Redirect Server: A redirect server is a user agent server that
        generates 3xx responses to requests it receives, directing the
        client to contact an alternate set of URIs.

        Registrar: A registrar is a server that accepts REGISTER
        requests and places the information it receives in those
        requests into the location service for the domain it handles."
    REFERENCE
       "RFC 3261, Section 6"
    SYNTAX      BITS {
                  other(0),
                  userAgent(1),
                  proxyServer(2),
                  redirectServer(3),
                  registrarServer(4)
                }

SipTCOptionTagHeaders ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "This convention defines the header fields that use the option
        tags per Section 19.2 of RFC 3261.  These tags are used in
        Require (Section 20.32), Proxy-Require (Section 20.29),
        Supported (Section 20.37), and Unsupported (Section 20.40)
        header fields."
    REFERENCE
       "RFC 3261, Sections 19.2, 20.32, 20.29, 20.37, and 20.40"
    SYNTAX      BITS {
                  require(0),       -- Require header
                  proxyRequire(1),  -- Proxy-Require header
                  supported(2),     -- Supported header
                  unsupported(3)    -- Unsupported header
                }

SipTCMethodName ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
       "This TEXTUAL-CONVENTION is a string that uniquely identifies a
        SIP method.  The scope of uniqueness is the context of all
        defined SIP methods.

        Experimental support of extension methods is acceptable and
        expected.  Extension methods are those defined in
        Internet-Draft documents but not yet allocated and
        officially sanctioned by IANA.

        To support experimental extension methods, any object using
        this TEXTUAL-CONVENTION as syntax MAY return/accept a method
        identifier value other than those sanctioned by IANA.  That
        system MUST ensure no collisions with officially assigned
        method names."
    REFERENCE
       "RFC 3261, Section 27.4"
    SYNTAX      OCTET STRING (SIZE (1..100))

END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

