-- extracted from rfc3970.txt
-- at Wed Jan  5 06:23:38 2005

   TE-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE,
       NOTIFICATION-TYPE, mib-2,
       Integer32, Gauge32, Counter32,
       Counter64, Unsigned32, TimeTicks     FROM SNMPv2-SMI

       RowStatus, StorageType, TimeStamp,
       TruthValue                           FROM SNMPv2-TC

       SnmpAdminString                      FROM SNMP-FRAMEWORK-MIB

       MODULE-COMPLIANCE, OBJECT-GROUP,
       NOTIFICATION-GROUP                   FROM SNMPv2-CONF

       TeHopAddress, TeHopAddressType,
       MplsBitRate                          FROM MPLS-TC-STD-MIB;

   teMIB MODULE-IDENTITY
       LAST-UPDATED "200501040000Z"         -- 01 January 2005
       ORGANIZATION "IETF Traffic Engineering Working Group"
       CONTACT-INFO "
                     Editor:         Kireeti Kompella
                             Postal: Juniper Networks, Inc.
                                     1194 Mathilda Ave
                                     Sunnyvale, CA 94089
                             Tel:    +1 408 745 2000
                             E-mail: kireeti@juniper.net

                     The IETF Traffic Engineering Working Group is
                     chaired by Jim Boyle and Ed Kern.

                     WG Mailing List information:

                       General Discussion: te-wg@ops.ietf.org
                         To Subscribe:     te-wg-request@ops.ietf.org
                            In Body:       subscribe
                         Archive:          ftp://ops.ietf.org/pub/lists

                     Comments on the MIB module should be sent to the
                     mailing list.  The archives for this mailing list
                     should be consulted for previous discussion on
                     this MIB.
                    "
       DESCRIPTION  "The Traffic Engineering MIB module.

                     Copyright (C) The Internet Society (2005).  This
                     version of this MIB module is part of RFC 3970;
                     see the RFC itself for full legal notices.
                    "

       -- revision history

       REVISION     "200501040000Z"         -- 01 January 2005
       DESCRIPTION  "Initial version, published as RFC 3970."
       ::= { mib-2 122 }

   -- Top level objects

   teMIBNotifications  OBJECT IDENTIFIER ::= { teMIB 0 }
   teMIBObjects        OBJECT IDENTIFIER ::= { teMIB 1 }
   teMIBConformance    OBJECT IDENTIFIER ::= { teMIB 2 }

   -- ****************************************************************
   --
   -- TE MIB Objects
   --

   -- TE Info

   teInfo OBJECT IDENTIFIER ::= { teMIBObjects 1 }

   teDistProtocol   OBJECT-TYPE
       SYNTAX       BITS {
                        other(0),
                        isis(1),
                        ospf(2)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "IGP used to distribute Traffic Engineering
                    information and topology to each device for the
                    purpose of automatic path computation.  More than
                    one IGP may be used to distribute TE information.
                   "
       ::= { teInfo 1 }

   teSignalingProto OBJECT-TYPE
       SYNTAX       BITS {
                        other(0),
                        rsvpte(1),
                        crldp(2),
                        static(3)    -- static configuration
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "Traffic Engineering signaling protocols supported
                    by this device.  More than one protocol may be
                    supported.
                   "
       REFERENCE   "For a description of RSVP-TE, see RFC 3209;
                    for CR-LDP, see RFC 3212.
                   "
       ::= { teInfo 2 }

   teNotificationEnable OBJECT-TYPE
       SYNTAX       TruthValue
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION "If this object is true, then it enables the
                    generation of notifications from this MIB module.
                    Otherwise notifications are not generated.
                   "
       DEFVAL { false }
       ::= { teInfo 3 }

   teNextTunnelIndex OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "An integer that may be used as a new Index in the
                    teTunnelTable.

                    The special value of 0 indicates that no more new
                    entries can be created in that table.

                    When this MIB module is used for configuration, this
                    object always contains a legal value (if non-zero)
                    for an index that is not currently used in that
                    table.  The Command Generator (Network Management
                    Application) reads this variable and uses the
                    (non-zero) value read when creating a new row with
                    an SNMP SET.  When the SET is performed, the Command
                    Responder (agent) must determine whether the value
                    is indeed still unused; Two Network Management
                    Applications may attempt to create a row
                    (configuration entry) simultaneously and use the
                    same value.  If it is currently unused, the SET
                    succeeds, and the Command Responder (agent) changes
                    the value of this object according to an
                    implementation-specific algorithm.  If the value is
                    in use, however, the SET fails.  The Network
                    Management Application must then re-read this
                    variable to obtain a new usable value.
                   "
       ::= { teInfo 4 }

   teNextPathHopIndex OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "An integer that may be used as a new Index in the
                    tePathHopTable.

                    The special value of 0 indicates that no more new
                    entries can be created in that table.

                    When this MIB module is used for configuration, this
                    object always contains a legal value (if non-zero)
                    for an index that is not currently used in that
                    table.  The Command Generator (Network Management
                    Application) reads this variable and uses the
                    (non-zero) value read when creating a new row with
                    an SNMP SET.  When the SET is performed, the Command
                    Responder (agent) must determine whether the value
                    is indeed still unused; Two Network Management
                    Applications may attempt to create a row
                    (configuration entry) simultaneously and use the
                    same value.  If it is currently unused, the SET
                    succeeds, and the Command Responder (agent) changes
                    the value of this object according to an
                    implementation-specific algorithm.  If the value is
                    in use, however, the SET fails.  The Network
                    Management Application must then re-read this
                    variable to obtain a new usable value.
                   "
       ::= { teInfo 5 }

   teConfiguredTunnels OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "Number of currently configured Tunnels."
       ::= { teInfo 6 }

   teActiveTunnels  OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "Number of currently active Tunnels."
       ::= { teInfo 7 }

   tePrimaryTunnels OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "Number of currently active Tunnels running on
                    their primary paths.
                   "
       ::= { teInfo 8 }

   teAdminGroupTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF TeAdminGroupEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "A mapping of configured administrative groups.  Each
                    entry represents an Administrative Group and
                    provides a name and index for the group.
                    Administrative groups are used to label links in the
                    Traffic Engineering topology in order to place
                    constraints (include and exclude) on Tunnel paths.

                    A groupName can only be linked to one group number.
                    The groupNumber is the number assigned to the
                    administrative group used in constraints,
                    such as tePathIncludeAny or tePathIncludeAll.
                   "
       ::= { teInfo 9 }

   teAdminGroupEntry OBJECT-TYPE
       SYNTAX       TeAdminGroupEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "A mapping between a configured group number and
                    its human-readable name.  The group number should
                    be between 1 and 32, inclusive.  Group number n
                    represents bit number (n-1) in the bit vector for
                    Include/Exclude constraints.

                    All entries in this table MUST be kept in stable
                    storage so that they will re-appear in case of a
                    restart/reboot.
                   "
       INDEX       { teAdminGroupNumber }
       ::= { teAdminGroupTable 1 }

   TeAdminGroupEntry ::=
       SEQUENCE {
           teAdminGroupNumber    Integer32,
           teAdminGroupName      SnmpAdminString,
           teAdminGroupRowStatus RowStatus
       }

   teAdminGroupNumber OBJECT-TYPE
       SYNTAX       Integer32 (1..32)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Index of the administrative group."
       ::= { teAdminGroupEntry 1 }

   teAdminGroupName OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (1..32))
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "Name of the administrative group."
       ::= { teAdminGroupEntry 2 }

   teAdminGroupRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The status of this conceptual row.

                    The value of this object has no effect on whether
                    other objects in this conceptual row can be
                    modified.
                   "
       ::= { teAdminGroupEntry 3 }

   -- Tunnel Table

   teTunnelTable    OBJECT-TYPE
       SYNTAX       SEQUENCE OF TeTunnelEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Table of Configured Traffic Tunnels."
       ::= { teMIBObjects 2 }

   teTunnelEntry    OBJECT-TYPE
       SYNTAX       TeTunnelEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Entry containing information about a particular
                    Traffic Tunnel.
                   "
       INDEX       { teTunnelIndex }
       ::= { teTunnelTable 1 }

   TeTunnelEntry ::=
       SEQUENCE {
           teTunnelIndex                   Unsigned32,
           teTunnelName                    SnmpAdminString,
           teTunnelNextPathIndex           Unsigned32,
        -- Conceptual row information:
           teTunnelRowStatus               RowStatus,
           teTunnelStorageType             StorageType,
        -- Address information:
           teTunnelSourceAddressType       TeHopAddressType,
           teTunnelSourceAddress           TeHopAddress,
           teTunnelDestinationAddressType  TeHopAddressType,
           teTunnelDestinationAddress      TeHopAddress,
        -- State/performance information:
           teTunnelState                   INTEGER,
           teTunnelDiscontinuityTimer      TimeStamp,
           teTunnelOctets                  Counter64,
           teTunnelPackets                 Counter64,
           teTunnelLPOctets                Counter32,
           teTunnelLPPackets               Counter32,
           teTunnelAge                     TimeTicks,
           teTunnelTimeUp                  TimeTicks,
           teTunnelPrimaryTimeUp           TimeTicks,
           teTunnelTransitions             Counter32,
           teTunnelLastTransition          TimeTicks,
           teTunnelPathChanges             Counter32,
           teTunnelLastPathChange          TimeTicks,
           teTunnelConfiguredPaths         Gauge32,
           teTunnelStandbyPaths            Gauge32,
           teTunnelOperationalPaths        Gauge32
       }

   teTunnelIndex    OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4294967295)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "A unique index that identifies a Tunnel.  If the TE
                    Tunnel is considered an interface, then this index
                    must match the interface index of the corresponding
                    interface.  Otherwise, this index must be at least
                    2^24, so that it does not overlap with any existing
                    interface index.
                   "
       ::= { teTunnelEntry 1 }

   teTunnelName     OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE (1..32))
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "Name of the Traffic Tunnel.

                    Note that the name of a Tunnel MUST be unique.
                    When a SET request contains a name that is already
                    in use for another entry, then the implementation
                    must return an inconsistentValue error.

                    The value of this object cannot be changed if the
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { teTunnelEntry 2 }

   teTunnelNextPathIndex  OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "An integer that may be used as a new Index for the
                    next Path in this Tunnel.

                    The special value of 0 indicates that no more Paths
                    can be created for this Tunnel, or that no more new
                    entries can be created in tePathTable.
                    When this MIB module is used for configuration, this
                    object always contains a legal value (if non-zero)
                    for an index that is not currently used in that
                    table.  The Command Generator (Network Management
                    Application) reads this variable and uses the
                    (non-zero) value read when creating a new row with
                    an SNMP SET.  When the SET is performed, the Command
                    Responder (agent) must determine whether the value
                    is indeed still unused; Two Network Management
                    Applications may attempt to create a row
                    (configuration entry) simultaneously and use the
                    same value.  If it is currently unused, the SET
                    succeeds, and the Command Responder (agent) changes
                    the value of this object according to an
                    implementation-specific algorithm.  If the value is
                    in use, however, the SET fails.  The Network
                    Management Application must then re-read this
                    variable to obtain a new usable value.
                   "
       ::= { teTunnelEntry 3 }

   teTunnelRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The status of this conceptual row.

                    When the value of this object is 'active', then
                    the values for the corresponding objects
                    teTunnelName, teTunnelSourceAddressType,
                    teTunnelSourceAddress,
                    teTunnelDestinationAddressType, and
                    teTunnelDestinationAddress cannot be changed.
                   "
       ::= { teTunnelEntry 4 }

   teTunnelStorageType OBJECT-TYPE
       SYNTAX       StorageType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The storage type for this conceptual row.

                    Conceptual rows having the value 'permanent' need
                    not allow write-access to any columnar objects
                    in the row.
                   "
       ::= { teTunnelEntry 5 }

   teTunnelSourceAddressType OBJECT-TYPE
       SYNTAX       TeHopAddressType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The type of Traffic Engineered Tunnel hop address
                    for the source of this Tunnel.  Typically, this
                    address type is IPv4 or IPv6, with a prefix length
                    of 32 or 128, respectively.  If the TE Tunnel path
                    is being computed by a path computation server,
                    however, it is possible to use more flexible source
                    address types, such as AS numbers or prefix lengths
                    less than host address lengths.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { teTunnelEntry 6 }

   teTunnelSourceAddress OBJECT-TYPE
       SYNTAX       TeHopAddress
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The Source Traffic Engineered Tunnel hop address of
                    this Tunnel.

                    The type of this address is determined by the value
                    of the corresponding teTunnelSourceAddressType.

                    Note that the source and destination addresses of a
                    Tunnel can be different address types.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { teTunnelEntry 7 }

   teTunnelDestinationAddressType OBJECT-TYPE
       SYNTAX       TeHopAddressType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The type of Traffic Engineered Tunnel hop address
                    for the destination of this Tunnel.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.

                   "
       ::= { teTunnelEntry 8 }

   teTunnelDestinationAddress OBJECT-TYPE
       SYNTAX       TeHopAddress
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The Destination Traffic Engineered Tunnel hop
                    address of this Tunnel.

                    The type of this address is determined by the value
                    of the corresponding teTunnelDestinationAddressType.

                    Note that source and destination addresses of a
                    Tunnel can be different address types.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { teTunnelEntry 9 }

   teTunnelState    OBJECT-TYPE
       SYNTAX       INTEGER {
                        unknown(1),
                        up(2),
                        down(3),
                        testing(4)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The operational state of the Tunnel."
       ::= { teTunnelEntry 10 }

   teTunnelDiscontinuityTimer OBJECT-TYPE
       SYNTAX       TimeStamp
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The value of sysUpTime on the most recent occasion
                    at which any one or more of this tunnel's counters
                    suffered a discontinuity.  The relevant counters
                    are teTunnelOctets, teTunnelPackets,
                    teTunnelLPOctets, and teTunnelLPPackets.  If no such
                    discontinuities have occurred since the last
                    re-initialization of the local management subsystem
                    then this object contains a zero value.
                   "
       ::= { teTunnelEntry 11 }

   teTunnelOctets   OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of octets that have been forwarded over
                    the Tunnel.

                    Discontinuities in the value of this counter can
                    occur at re-initialization of the management system,
                    and at other times, as indicated by the value of
                    teTunnelDiscontinuityTimer.
                   "
       ::= { teTunnelEntry 12 }

   teTunnelPackets  OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of packets that have been forwarded over
                    the Tunnel.

                    Discontinuities in the value of this counter can
                    occur at re-initialization of the management system
                    and at other times, as indicated by the value of
                    teTunnelDiscontinuityTimer.
                   "
       ::= { teTunnelEntry 13 }

   teTunnelLPOctets OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of octets that have been forwarded over
                    the Tunnel.

                    Discontinuities in the value of this counter can
                    occur at re-initialization of the management system
                    and at other times, as indicated by the value of
                    teTunnelDiscontinuityTimer.
                   "
       ::= { teTunnelEntry 14 }

   teTunnelLPPackets OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of packets that have been forwarded over
                    the Tunnel.
                    Discontinuities in the value of this counter can
                    occur at re-initialization of the management system
                    and at other times, as indicated by the value of
                    teTunnelDiscontinuityTimer.
                   "
       ::= { teTunnelEntry 15 }

   teTunnelAge      OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The age (i.e., time from creation of this conceptual
                    row till now) of this Tunnel in hundredths of a
                    second.  Note that because TimeTicks wrap in about
                    16 months, this value is best used in interval
                    measurements.
                   "
       ::= { teTunnelEntry 16 }

   teTunnelTimeUp   OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The total time in hundredths of a second that this
                    Tunnel has been operational.  Note that because
                    TimeTicks wrap in about 16 months, this value is
                    best used in interval measurements.

                    An example of usage of this object would be to
                    compute the percentage up time over a period of time
                    by obtaining values of teTunnelAge and
                    teTunnelTimeUp at two points in time and computing
                    the following ratio:
                    ((teTunnelTimeUp2 - teTunnelTimeUp1)/
                    (teTunnelAge2 - teTunnelAge1)) * 100 %.  In doing
                    so, the management station must account for
                    wrapping of the values of teTunnelAge and
                    teTunnelTimeUp between the two measurements.
                   "
       ::= { teTunnelEntry 17 }

   teTunnelPrimaryTimeUp OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The total time in hundredths of a second that this
                    Tunnel's primary path has been operational.  Note
                    that because TimeTicks wrap in about 16 months, this
                    value is best used in interval measurements.

                    An example of usage of this field would be to
                    compute what percentage of time that a TE Tunnel was
                    on the primary path over a period of time by
                    computing
                    ((teTunnelPrimaryTimeUp2 - teTunnelPrimaryTimeUp1)/
                    (teTunnelTimeUp2 - teTunnelTimeUp1))*100 %.  In
                    doing so, the management station must account for
                    wrapping of the values of teTunnelPrimaryTimeUp and
                    teTunnelTimeUp between the two measurements.
                   "
       ::= { teTunnelEntry 18 }

   teTunnelTransitions OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of operational state transitions
                    (up -> down and down -> up) this Tunnel has
                    undergone.
                   "
       ::= { teTunnelEntry 19 }

   teTunnelLastTransition OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The time in hundredths of a second since the last
                    operational state transition occurred on this
                    Tunnel.

                    Note that if the last transition was over 16
                    months ago, this value will be inaccurate.
                   "
       ::= { teTunnelEntry 20 }

   teTunnelPathChanges OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of path changes this Tunnel has had."
       ::= { teTunnelEntry 21 }

   teTunnelLastPathChange OBJECT-TYPE
       SYNTAX       TimeTicks
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The time in hundredths of a second since the last
                    path change occurred on this Tunnel.

                    Note that if the last transition was over 16
                    months ago, this value will be inaccurate.

                    Path changes may be caused by network events or by
                    reconfiguration that affects the path.
                   "
       ::= { teTunnelEntry 22 }

   teTunnelConfiguredPaths OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of paths configured for this Tunnel."
       ::= { teTunnelEntry 23 }

   teTunnelStandbyPaths OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of standby paths configured for this
                    Tunnel.
                   "
       ::= { teTunnelEntry 24 }

   teTunnelOperationalPaths OBJECT-TYPE
       SYNTAX       Gauge32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of operational paths for this Tunnel.
                    This includes the path currently active, as
                    well as operational standby paths.
                   "
       ::= { teTunnelEntry 25 }

   -- ****************************************************************
   --
   -- Tunnel Path Table
   --

   tePathTable      OBJECT-TYPE
       SYNTAX       SEQUENCE OF TePathEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Table of Configured Traffic Tunnels."
       ::= { teMIBObjects 3 }

   tePathEntry      OBJECT-TYPE
       SYNTAX       TePathEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Entry containing information about a particular
                    Traffic Tunnel.  Each Traffic Tunnel can have zero
                    or more Traffic Paths.

                    As a Traffic Path can only exist over an existing
                    Traffic Tunnel, all tePathEntries with
                    a value of n for teTunnelIndex MUST be removed by
                    the implementation when the corresponding
                    teTunnelEntry with a value of n for teTunnelIndex
                    is removed.
                   "
       INDEX       { teTunnelIndex, tePathIndex }
       ::= { tePathTable 1 }

   TePathEntry ::=
       SEQUENCE {
           tePathIndex                Unsigned32,
           tePathName                 SnmpAdminString,
        -- Conceptual row information
           tePathRowStatus            RowStatus,
           tePathStorageType          StorageType,
        -- Path properties
           tePathType                 INTEGER,
           tePathConfiguredRoute      Unsigned32,
           tePathBandwidth            MplsBitRate,
           tePathIncludeAny           Unsigned32,
           tePathIncludeAll           Unsigned32,
           tePathExclude              Unsigned32,
           tePathSetupPriority        Integer32,
           tePathHoldPriority         Integer32,
           tePathProperties           BITS,
        -- Path status
           tePathOperStatus           INTEGER,
           tePathAdminStatus          INTEGER,
           tePathComputedRoute        Unsigned32,
           tePathRecordedRoute        Unsigned32
       }

   tePathIndex      OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4294967295)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "An index that uniquely identifies a path within
                    a Tunnel.
                    The combination of <teTunnelIndex, tePathIndex> thus
                    uniquely identifies a path among all paths on this
                    router.
                   "
       ::= { tePathEntry 1 }

   tePathName       OBJECT-TYPE
       SYNTAX       SnmpAdminString (SIZE(0..32))
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The name of this path.

                    A pathName must be unique within the set of paths
                    over a single tunnel.  If a SET request is received
                    with a duplicate name, then the implementation MUST
                    return an inconsistentValue error.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { tePathEntry 2 }

   tePathRowStatus  OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The status of this conceptual row.

                    When the value of this object is 'active', then
                    the value of tePathName cannot be changed.  All
                    other writable objects may be changed; however,
                    these changes may affect traffic going over the TE
                    tunnel or require the path to be computed and/or
                    re-signaled.
                   "
       ::= { tePathEntry 3 }

   tePathStorageType OBJECT-TYPE
       SYNTAX       StorageType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The storage type for this conceptual row.

                    Conceptual rows having the value 'permanent' need
                    not allow write-access to any columnar objects
                    in the row.
                   "
       ::= { tePathEntry 4 }

   tePathType OBJECT-TYPE
       SYNTAX       INTEGER {
                        other(1),
                        primary(2),
                        standby(3),
                        secondary(4)
                    }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The type for this PathEntry; i.e., whether this path
                    is a primary path, a standby path, or a secondary
                    path.
                   "
       ::= { tePathEntry 5 }

   tePathConfiguredRoute OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The route that this TE path is configured to follow;
                    i.e., an ordered list of hops.  The value of this
                    object gives the primary index into the Hop Table.
                    The secondary index is the hop count in the path, so
                    to get the route, one could get the first hop with
                    index <tePathConfiguredRoute, 1> in the Hop Table
                    and do a getnext to get subsequent hops.
                   "
       ::= { tePathEntry 6 }

   tePathBandwidth  OBJECT-TYPE
       SYNTAX       MplsBitRate
       UNITS       "Kilobits per second"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The configured bandwidth for this Tunnel,
                    in units of thousands of bits per second (Kbps).
                   "
       DEFVAL      { 0 }
       ::= { tePathEntry 7 }

   tePathIncludeAny OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "This is a configured set of administrative groups
                    specified as a bit vector (i.e., bit n is 1 if group
                    n is in the set, where n = 0 is the LSB).  For each
                    link that this path goes through, the link must have
                    at least one of the groups specified in IncludeAny
                    to be acceptable.  If IncludeAny is zero, all links
                    are acceptable.
                   "
       DEFVAL      { 0 }
       ::= { tePathEntry 8 }

   tePathIncludeAll OBJECT-TYPE

       SYNTAX       Unsigned32
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "This is a configured set of administrative groups
                    specified as a bit vector (i.e., bit n is 1 if group
                    n is in the set, where n = 0 is the LSB).  For each
                    link that this path goes through, the link must have
                    all of the groups specified in IncludeAll to be
                    acceptable.  If IncludeAll is zero, all links are
                    acceptable.
                   "
       DEFVAL      { 0 }
       ::= { tePathEntry 9 }

   tePathExclude    OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "This is a configured set of administrative groups
                    specified as a bit vector (i.e., bit n is 1 if group
                    n is in the set, where n = 0 is the LSB).  For each
                    link that this path goes through, the link MUST have
                    groups associated with it, and the intersection of
                    the link's groups and the 'exclude' set MUST be
                    null.
                   "
       DEFVAL      { 0 }
       ::= { tePathEntry 10 }

   tePathSetupPriority OBJECT-TYPE
       SYNTAX       Integer32 (0..7)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The setup priority configured for this path, with 0
                    as the highest priority and 7 as the lowest.
                   "
       DEFVAL      { 7 }
       ::= { tePathEntry 11 }

   tePathHoldPriority OBJECT-TYPE
       SYNTAX       Integer32 (0..7)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The hold priority configured for this path, with 0
                    as the highest priority and 7 as the lowest.
                   "
       DEFVAL      { 0 }
       ::= { tePathEntry 12 }

   tePathProperties OBJECT-TYPE
       SYNTAX       BITS {
                        recordRoute(0),
                        cspf(1),
                        makeBeforeBreak(2),
                        mergeable(3),
                        fastReroute(4),
                        protected(5)
                    }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The set of configured properties for this path,
                    expressed as a bit map.  For example, if the path
                    supports 'make before break', then bit 2 is set.
                   "
       ::= { tePathEntry 13 }

   tePathOperStatus OBJECT-TYPE
       SYNTAX       INTEGER {
                        unknown(0),
                        down(1),
                        testing(2),
                        dormant(3),
                        ready(4),
                        operational(5)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The operational status of the path:
                    unknown:
                    down:        Signaling failed.
                    testing:     Administratively set aside for testing.
                    dormant:     Not signaled (for a backup tunnel).
                    ready:       Signaled but not yet carrying traffic.
                    operational: Signaled and carrying traffic.
                   "
       ::= { tePathEntry 14 }

   tePathAdminStatus OBJECT-TYPE
       SYNTAX       INTEGER {
                        normal(1),
                        testing(2)
                    }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The operational status of the path:
                    normal:      Used normally for forwarding.
                    testing:     Administratively set aside for testing.
                   "
       ::= { tePathEntry 15 }

   tePathComputedRoute OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The route computed for this path, perhaps using
                    some form of Constraint-based Routing.  The
                    algorithm is implementation dependent.

                    This object returns the computed route as an ordered
                    list of hops.  The value of this object gives the
                    primary index into the Hop Table.  The secondary
                    index is the hop count in the path, so to get the
                    route, one could get the first hop with index
                    <tePathComputedRoute, 1> in the Hop Table and do a
                    getnext to get subsequent hops.

                    A value of zero (0) means there is no computedRoute.
                   "
       ::= { tePathEntry 16 }

   tePathRecordedRoute OBJECT-TYPE
       SYNTAX       Unsigned32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The route actually used for this path, as recorded
                    by the signaling protocol.  This is again an ordered
                    list of hops; each hop is expected to be strict.

                    The value of this object gives the primary index
                    into the Hop Table.  The secondary index is the hop
                    count in the path, so to get the route, one can get
                    the first hop with index <tePathRecordedRoute, 1>
                    in the Hop Table and do a getnext to get subsequent
                    hops.

                    A value of zero (0) means there is no recordedRoute.
                   "
       ::= { tePathEntry 17 }

   -- ****************************************************************
   --
   -- Tunnel Path Hop Table
   --

   tePathHopTable   OBJECT-TYPE
       SYNTAX       SEQUENCE OF TePathHopEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Table of Tunnel Path Hops."
       ::= { teMIBObjects 4 }

   tePathHopEntry   OBJECT-TYPE
       SYNTAX       TePathHopEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "Entry containing information about a particular
                    hop.
                   "
       INDEX       { teHopListIndex, tePathHopIndex }
       ::= { tePathHopTable 1 }

   TePathHopEntry ::=
       SEQUENCE {
           teHopListIndex              Unsigned32,
           tePathHopIndex              Unsigned32,
        -- Conceptual row information
           tePathHopRowStatus          RowStatus,
           tePathHopStorageType        StorageType,
           tePathHopAddrType           TeHopAddressType,
           tePathHopAddress            TeHopAddress,
           tePathHopType               INTEGER
       }

   teHopListIndex   OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4294967295)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "An index that identifies a list of hops.  This is
                    the primary index to access hops.
                   "
       ::= { tePathHopEntry 1 }

   tePathHopIndex   OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4294967295)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION "An index that identifies a particular hop among the
                    list of hops for a path.  An index of i identifies
                    the ith hop.  This is the secondary index for a hop
                    entry.
                   "
       ::= { tePathHopEntry 2 }

   tePathHopRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The status of this conceptual row.

                    Any field in this table can be changed, even if the
                    value of this object is 'active'.  However, such a
                    change may cause traffic to be rerouted or even
                    disrupted.
                   "
       ::= { tePathHopEntry 3 }

   tePathHopStorageType OBJECT-TYPE
       SYNTAX       StorageType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The storage type for this conceptual row.

                    Conceptual rows having the value 'permanent' need
                    not allow write-access to any columnar objects
                    in the row.
                   "
       ::= { tePathHopEntry 4 }

   tePathHopAddrType OBJECT-TYPE
       SYNTAX       TeHopAddressType
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The type of Traffic Engineered Tunnel hop Address
                    of this hop.

                    The value of this object cannot be changed
                    if the value of the corresponding tePathRowStatus
                    object is 'active'.
                   "
       ::= { tePathHopEntry 5 }

   tePathHopAddress OBJECT-TYPE
       SYNTAX       TeHopAddress
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION "The Traffic Engineered Tunnel hop Address of this
                    hop.

                    The type of this address is determined by the value
                    of the corresponding tePathHopAddressType.

                    The value of this object cannot be changed
                    if the value of the corresponding teTunnelRowStatus
                    object is 'active'.
                   "
       ::= { tePathHopEntry 6 }

   tePathHopType    OBJECT-TYPE
       SYNTAX       INTEGER {
                        unknown(0),
                        loose(1),
                        strict(2)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The type of hop:
                    unknown:
                    loose:    This hop is a LOOSE hop.
                    strict:   This hop is a STRICT hop.
                   "
       ::= { tePathHopEntry 7 }

   -- ****************************************************************
   --
   -- TE Notifications
   --

   teTunnelUp       NOTIFICATION-TYPE
       OBJECTS      { teTunnelName,
                      tePathName }  -- TunnelPath
       STATUS       current
       DESCRIPTION "A teTunnelUp notification is generated when the
                    Tunnel indexed by teTunnelName transitions to the
                    'up' state.

                    A tunnel is up when at least one of its paths is up.
                    The tePathName is the name of the path whose
                    transition to up made the tunnel go up.
                    This notification MUST be limited to at most one
                    every minute, in case the tunnel flaps up and down.
                   "
       ::= { teMIBNotifications 1 }

   teTunnelDown     NOTIFICATION-TYPE
       OBJECTS      { teTunnelName,
                      tePathName }  -- TunnelPath
       STATUS       current
       DESCRIPTION "A teTunnelDown notification is generated when the
                    Tunnel indexed by teTunnelName transitions to the
                    'down' state.

                    A tunnel is up when at least one of its paths is up.
                    The tePathName is the name of the path whose
                    transition to down made the tunnel go down.

                    This notification MUST be limited to at most one
                    every minute, in case the tunnel flaps up and down.
                   "
       ::= { teMIBNotifications 2 }

   teTunnelChanged  NOTIFICATION-TYPE
       OBJECTS      { teTunnelName,
                      tePathName }  -- toTunnelPath
       STATUS       current
       DESCRIPTION "A teTunnelChanged notification is generated when an
                    active path on the Tunnel indexed by teTunnelName
                    changes or a new path becomes active.  The value
                    of tePathName is the new active path.

                    This notification MUST be limited to at most one
                    every minute, in case the tunnel changes quickly.
                   "
       ::= { teMIBNotifications 3 }

   teTunnelRerouted NOTIFICATION-TYPE
       OBJECTS      { teTunnelName,
                      tePathName }  -- toTunnelPath
       STATUS       current
       DESCRIPTION "A teTunnelRerouted notification is generated when
                    an active path for the Tunnel indexed by
                    teTunnelName stays the same, but its route changes.

                    This notification MUST be limited to at most one
                    every minute, in case the tunnel reroutes quickly.
                   "
       ::= { teMIBNotifications 4 }

   -- End of TE-MIB objects

   -- ****************************************************************
   --
   -- TE Compliance Statements
   --

   teGroups
       OBJECT IDENTIFIER ::= { teMIBConformance 1 }

   teModuleCompliance
       OBJECT IDENTIFIER ::= { teMIBConformance 2 }

   -- ****************************************************************
   --
   -- TE object groups
   --

   teTrafficEngineeringGroup OBJECT-GROUP
       OBJECTS {
           teTunnelName,
           teTunnelNextPathIndex,
           teTunnelRowStatus,
           teTunnelStorageType,
           teTunnelSourceAddressType,
           teTunnelSourceAddress,
           teTunnelDestinationAddressType,
           teTunnelDestinationAddress,
           teTunnelState,
           teTunnelDiscontinuityTimer,
           teTunnelOctets,
           teTunnelPackets,
           teTunnelLPOctets,
           teTunnelLPPackets,
           teTunnelAge,
           teTunnelTimeUp,
           teTunnelPrimaryTimeUp,
           teTunnelTransitions,
           teTunnelLastTransition,
           teTunnelPathChanges,
           teTunnelLastPathChange,
           teTunnelConfiguredPaths,
           teTunnelStandbyPaths,
           teTunnelOperationalPaths,
           tePathBandwidth,
           tePathIncludeAny,
           tePathIncludeAll,
           tePathExclude,
           tePathSetupPriority,
           tePathHoldPriority,
           tePathProperties,
           tePathOperStatus,
           tePathAdminStatus,
           tePathComputedRoute,
           tePathRecordedRoute,
           teDistProtocol,
           teSignalingProto,
           teNotificationEnable,
           teNextTunnelIndex,
           teNextPathHopIndex,
           teAdminGroupName,
           teAdminGroupRowStatus,
           teConfiguredTunnels,
           teActiveTunnels,
           tePrimaryTunnels,
           tePathName,
           tePathType,
           tePathRowStatus,
           tePathStorageType,
           tePathConfiguredRoute,
           tePathHopRowStatus,
           tePathHopStorageType,
           tePathHopAddrType,
           tePathHopAddress,
           tePathHopType
       }
       STATUS       current
       DESCRIPTION "Objects for Traffic Engineering in this MIB module."
       ::= { teGroups 1 }

   teNotificationGroup NOTIFICATION-GROUP
      NOTIFICATIONS {
          teTunnelUp,
          teTunnelDown,
          teTunnelChanged,
          teTunnelRerouted
      }
      STATUS       current
      DESCRIPTION "Notifications specified in this MIB module."
      ::= { teGroups 2 }

   -- ****************************************************************
   --
   -- TE compliance statements
   --
   --    There are four compliance statements: read-only and full
   --    compliance for regular TE devices, and read-only and full
   --    compliance for path computation servers.
   --

   teModuleReadOnlyCompliance MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION "When this MIB module is implemented without support
                    for read-create (i.e., in read-only mode), then such
                    an implementation can claim read-only compliance.
                    Such a device can be monitored but cannot be
                    configured with this MIB module.
                   "

       MODULE       -- enclosing module, i.e., TE-MIB

           MANDATORY-GROUPS {
               teTrafficEngineeringGroup
           }

           GROUP        teNotificationGroup
           DESCRIPTION "Implementation of this group is optional."

           OBJECT       teNotificationEnable
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teAdminGroupName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teAdminGroupRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."
           OBJECT       teTunnelSourceAddressType
           SYNTAX       TeHopAddressType { ipv4(1), ipv6(2) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required.  An
                        implementation is only required to support
                        IPv4 and IPv6 host addresses."

           OBJECT       teTunnelSourceAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelDestinationAddressType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelDestinationAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathConfiguredRoute
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathBandwidth
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathIncludeAny
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."
           OBJECT       tePathIncludeAll
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathExclude
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathSetupPriority
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHoldPriority
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathProperties
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathAdminStatus
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopAddrType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

       ::= { teModuleCompliance 1 }

   teModuleFullCompliance MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION "When this MIB module is implemented with support for
                    read-create, then the implementation can claim
                    full compliance.  Such devices can be both
                    monitored and configured with this MIB module.
                   "

       MODULE       -- enclosing module, i.e., TE-MIB

           MANDATORY-GROUPS {
               teTrafficEngineeringGroup
           }

           GROUP        teNotificationGroup
           DESCRIPTION "Implementation of this group is optional."


           OBJECT       teAdminGroupRowStatus
           SYNTAX       RowStatus { active(1) }
           WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
           DESCRIPTION "Support for notInService, createAndWait and
                        notReady is not required.
                       "

           OBJECT       teTunnelRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "

           OBJECT       teTunnelSourceAddressType
           SYNTAX       TeHopAddressType { ipv4(1), ipv6(2) }
           DESCRIPTION "Write access is required.  An implementation is
                        only required to support IPv4 and IPv6 host
                        addresses.
                       "

           OBJECT       tePathRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "

           OBJECT       tePathHopRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "
       ::= { teModuleCompliance 2 }

   teModuleServerReadOnlyCompliance MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION "When this MIB module is implemented by a path
                    computation server without support for read-create
                    (i.e., in read-only mode), then the implementation
                    can claim read-only compliance.  Such
                    a device can be monitored but cannot be
                    configured with this MIB module.
                   "

       MODULE       -- enclosing module, i.e., TE-MIB

           MANDATORY-GROUPS {
               teTrafficEngineeringGroup
           }

           GROUP        teNotificationGroup
           DESCRIPTION "Implementation of this group is optional."

           OBJECT       teNotificationEnable
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teAdminGroupName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teAdminGroupRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."
           OBJECT       teTunnelStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelSourceAddressType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required.  A path
                        computation server SHOULD implement all types
                        of tunnel source address types.
                       "

           OBJECT       teTunnelSourceAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelDestinationAddressType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       teTunnelDestinationAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathName
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathConfiguredRoute
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathBandwidth
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."
           OBJECT       tePathIncludeAny
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathIncludeAll
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathExclude
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathSetupPriority
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHoldPriority
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathProperties
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathAdminStatus
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopStorageType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopAddrType
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

           OBJECT       tePathHopAddress
           MIN-ACCESS   read-only
           DESCRIPTION "Write access is not required."

       ::= { teModuleCompliance 3 }

   teModuleServerFullCompliance MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION "When this MIB module is implemented by a path
                    computation server with support for read-create,
                    then the implementation can claim full
                    compliance.
                   "

       MODULE       -- enclosing module, i.e., TE-MIB
           MANDATORY-GROUPS {
               teTrafficEngineeringGroup
           }

           GROUP        teNotificationGroup
           DESCRIPTION "Implementation of this group is optional."


           OBJECT       teAdminGroupRowStatus
           SYNTAX       RowStatus { active(1) }
           WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
           DESCRIPTION "Support for notInService, createAndWait, and
                        notReady is not required.
                       "

           OBJECT       teTunnelRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "

           OBJECT       teTunnelSourceAddressType
           DESCRIPTION "Write access is required.  An implementation
                        of a path computation server SHOULD support all
                        types of tunnel source address types.
                       "

           OBJECT       tePathRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "

           OBJECT       tePathHopRowStatus
           SYNTAX       RowStatus { active(1), notInService(2) }
           WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                    createAndGo(4), destroy(6)
                                  }
           DESCRIPTION "Support for createAndWait and notReady is not
                        required.
                       "
       ::= { teModuleCompliance 4 }

   END

-- 
--    Copyright (C) The Internet Society (2005).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY AND THE INTERNET
--    ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS OR IMPLIED,
--    INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE
--    INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the IETF's procedures with respect to rights in IETF Documents can
--    be found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at ietf-
--    ipr@ietf.org.
-- 

