

ADSL-LINE-EXT-MIB DEFINITIONS ::= BEGIN

   IMPORTS
      Counter32,
      Integer32,
      NOTIFICATION-TYPE,
      MODULE-IDENTITY,
      OBJECT-TYPE                       FROM SNMPv2-SMI
      MODULE-COMPLIANCE, OBJECT-GROUP,
      NOTIFICATION-GROUP                FROM SNMPv2-CONF
      TEXTUAL-CONVENTION                FROM SNMPv2-TC
      PerfCurrentCount,
      PerfIntervalCount                 FROM PerfHist-TC-MIB
      AdslPerfCurrDayCount,
      AdslPerfPrevDayCount              FROM ADSL-TC-MIB
      SnmpAdminString                   FROM SNMP-FRAMEWORK-MIB
      adslLineAlarmConfProfileEntry,
      adslLineConfProfileEntry,
      adslAturIntervalEntry,
      adslAturPerfDataEntry,
      adslAtucIntervalEntry,
      adslAtucPerfDataEntry,
      adslLineEntry,
      adslMIB                           FROM ADSL-LINE-MIB
      ;

   adslExtMIB MODULE-IDENTITY

   LAST-UPDATED "200212100000Z"  -- 10 Dec 2002

   ORGANIZATION "IETF ADSL MIB Working Group"

   CONTACT-INFO
         "
          Faye Ly
          Pedestal Networks
          6503 Dumbarton Circle,
          Fremont, CA 94555
          Tel: +1 510-578-0158
          Fax: +1 510-744-5152
          E-Mail: faye@pedestalnetworks.com

          Gregory Bathrick
          Nokia Networks
          2235 Mercury Way,
          Fax: +1 707-535-7300
          E-Mail: greg.bathrick@nokia.com

          General Discussion:adslmib@ietf.org
          To Subscribe: https://www1.ietf.org/mailman/listinfo/adslmib
          Archive: https://www1.ietf.org/mailman/listinfo/adslmib
          "
   DESCRIPTION
           "Copyright (C) The Internet Society (2002). This version of
           this MIB module is part of RFC 3440; see the RFC itself for
           full legal notices.

           This MIB Module is a supplement to the ADSL-LINE-MIB
           [RFC2662]."

   REVISION     "200212100000Z"  -- 10 dec 2002
   DESCRIPTION  "Initial Version, published as RFC 3440. This MIB
                 module supplements the ADSL-LINE-MIB [RFC2662]."
          ::= { adslMIB 3 }

       adslExtMibObjects  OBJECT IDENTIFIER ::= { adslExtMIB 1 }

       AdslTransmissionModeType ::= TEXTUAL-CONVENTION
           STATUS       current
           DESCRIPTION
               "A set of ADSL line transmission modes, with one bit
                per mode.  The notes (F) and (L) denote Full-Rate
                and G.Lite respectively:
                  Bit 00 : Regional Std. (ANSI T1.413) (F)
                  Bit 01 : Regional Std. (ETSI DTS/TM06006) (F)
                  Bit 02 : G.992.1 POTS non-overlapped (F)
                  Bit 03 : G.992.1 POTS overlapped (F)
                  Bit 04 : G.992.1 ISDN non-overlapped (F)
                  Bit 05 : G.992.1 ISDN overlapped (F)
                  Bit 06 : G.992.1 TCM-ISDN non-overlapped (F)
                  Bit 07 : G.992.1 TCM-ISDN overlapped (F)
                  Bit 08 : G.992.2 POTS non-overlapped (L)
                  Bit 09 : G.992.2 POTS overlapped (L)
                  Bit 10 : G.992.2 with TCM-ISDN non-overlapped (L)
                  Bit 11 : G.992.2 with TCM-ISDN overlapped (L)
                  Bit 12 : G.992.1 TCM-ISDN symmetric (F)
               "
           SYNTAX      BITS {
               ansit1413(0),
               etsi(1),
               q9921PotsNonOverlapped(2),
               q9921PotsOverlapped(3),
               q9921IsdnNonOverlapped(4),
               q9921isdnOverlapped(5),
               q9921tcmIsdnNonOverlapped(6),
               q9921tcmIsdnOverlapped(7),
               q9922potsNonOverlapeed(8),
               q9922potsOverlapped(9),
               q9922tcmIsdnNonOverlapped(10),
               q9922tcmIsdnOverlapped(11),
               q9921tcmIsdnSymmetric(12)
           }

         adslLineExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslLineExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table is an extension of RFC 2662.  It
                  contains ADSL line configuration and
                  monitoring information. This includes the ADSL
                  line's capabilities and actual ADSL transmission
                  system."
         ::= { adslExtMibObjects 17 }

         adslLineExtEntry   OBJECT-TYPE
             SYNTAX          AdslLineExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "An entry extends the adslLineEntry defined in
                  [RFC2662].  Each entry corresponds to an ADSL
                  line."
             AUGMENTS { adslLineEntry }
         ::= { adslLineExtTable 1 }

         AdslLineExtEntry ::=
             SEQUENCE {
             adslLineTransAtucCap        AdslTransmissionModeType,
             adslLineTransAtucConfig     AdslTransmissionModeType,
             adslLineTransAtucActual     AdslTransmissionModeType,
             adslLineGlitePowerState     INTEGER,
             adslLineConfProfileDualLite SnmpAdminString
             }

         adslLineTransAtucCap OBJECT-TYPE
             SYNTAX      AdslTransmissionModeType
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The transmission modes, represented by a
                  bitmask that the ATU-C is capable of
                  supporting.  The modes available are limited
                  by the design of the equipment."
             REFERENCE "Section 7.3.2 ITU G.997.1"
         ::= { adslLineExtEntry 1 }

         adslLineTransAtucConfig OBJECT-TYPE
             SYNTAX      AdslTransmissionModeType
             MAX-ACCESS  read-write
             STATUS      current

             DESCRIPTION
                 "The transmission modes, represented by a bitmask,
                  currently enabled by the ATU-C.  The manager can
                  only set those modes that are supported by the
                  ATU-C.  An ATU-C's supported modes are provided by
                  AdslLineTransAtucCap."
             REFERENCE "Section 7.3.2 ITU G.997.1"
         ::= { adslLineExtEntry 2 }

         adslLineTransAtucActual OBJECT-TYPE
             SYNTAX      AdslTransmissionModeType
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The actual transmission mode of the ATU-C.
                  During ADSL line initialization, the ADSL
                  Transceiver Unit - Remote terminal end (ATU-R)
                  will determine the mode used for the link.
                  This value will be limited a single transmission
                  mode that is a subset of those modes enabled
                  by the ATU-C and denoted by
                  adslLineTransAtucConfig. After an initialization
                  has occurred, its mode is saved as the 'Current'
                  mode and is persistence should the link go
                  down. This object returns 0 (i.e. BITS with no
                  mode bit set) if the mode is not known."
             REFERENCE "Section 7.3.2 ITU G.997.1 "
         ::= { adslLineExtEntry 3 }

         adslLineGlitePowerState OBJECT-TYPE
             SYNTAX      INTEGER {
                         none(1),
                         l0(2),          -- L0 Power on
                         l1(3),          -- L1 Power on but reduced
                         l3(4)           -- L3 Power off
                         }
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object specifies the power
                  state of this interface.  L0 is power on, L1 is
                  power on but reduced and L3 is power off.  Power
                  state cannot be configured by an operator but it
                  can be viewed via the ifOperStatus object for the
                  managed ADSL interface.  The value of the object
                  ifOperStatus is set to down(2) if the ADSL
                  interface is in power state L3 and is set to up(1)
                  if the ADSL line interface is in power state L0 or
                  L1. If the object adslLineTransAtucActual is set to
                  a G.992.2 (G.Lite)-type transmission mode, the
                  value of this object will be one of the valid power
                  states: L0(2), L1(3), or L3(4).  Otherwise, its
                  value will be none(1)."
         ::= { adslLineExtEntry 4 }

         adslLineConfProfileDualLite OBJECT-TYPE
             SYNTAX SnmpAdminString
             MAX-ACCESS  read-write
             STATUS current
             DESCRIPTION
                 "This object extends the definition an ADSL line and
                  associated channels (when applicable) for cases
                  when it is configured in dual mode, and operating
                  in a G.Lite-type mode as denoted by
                  adslLineTransAtucActual.  Dual mode exists when the
                  object, adslLineTransAtucConfig, is configured with
                  one or more full-rate modes and one or more G.Lite
                  modes simultaneously.

                  When 'dynamic' profiles are implemented, the value
                  of object is equal to the index of the applicable
                  row in the ADSL Line Configuration Profile Table,
                  AdslLineConfProfileTable defined in ADSL-MIB
                  [RFC2662].

                  In the case when dual-mode has not been enabled,
                  the value of the object will be equal to the value
                  of the object adslLineConfProfile [RFC2662].

                  When `static' profiles are implemented, in much
                  like the case of the object,
                  adslLineConfProfileName [RFC2662], this object's
                  value will need to algorithmically represent the
                  characteristics of the line.  In this case, the
                  value of the line's ifIndex plus a value indicating
                  the line mode type (e.g., G.Lite, Full-rate) will
                  be used. Therefore, the profile's name is a string
                  concatenating the ifIndex and one of the follow
                  values: Full or Lite. This string will be
                  fixed-length (i.e., 14) with leading zero(s).  For
                  example, the profile name for ifIndex that equals
                  '15' and is a full rate line, it will be
                  '0000000015Full'."
             REFERENCE "Section 5.4 Profiles, RFC 2662"
         ::= { adslLineExtEntry 5 }

         adslAtucPerfDataExtTable   OBJECT-TYPE

             SYNTAX          SEQUENCE OF AdslAtucPerfDataExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table extends adslAtucPerfDataTable [RFC2662]
                  with additional ADSL physical line counter
                  information such as unavailable seconds-line and
                  severely errored seconds-line."
         ::= { adslExtMibObjects 18 }

         adslAtucPerfDataExtEntry   OBJECT-TYPE
             SYNTAX          AdslAtucPerfDataExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "An entry extends the adslAtucPerfDataEntry defined
                  in [RFC2662].  Each entry corresponds to an ADSL
                  line."
         AUGMENTS { adslAtucPerfDataEntry }
         ::= { adslAtucPerfDataExtTable 1 }

         AdslAtucPerfDataExtEntry ::=
             SEQUENCE {
             adslAtucPerfStatFastR            Counter32,
             adslAtucPerfStatFailedFastR      Counter32,
             adslAtucPerfStatSesL             Counter32,
             adslAtucPerfStatUasL             Counter32,
             adslAtucPerfCurr15MinFastR       PerfCurrentCount,
             adslAtucPerfCurr15MinFailedFastR PerfCurrentCount,
             adslAtucPerfCurr15MinSesL        PerfCurrentCount,
             adslAtucPerfCurr15MinUasL        PerfCurrentCount,
             adslAtucPerfCurr1DayFastR        AdslPerfCurrDayCount,
             adslAtucPerfCurr1DayFailedFastR  AdslPerfCurrDayCount,
             adslAtucPerfCurr1DaySesL         AdslPerfCurrDayCount,
             adslAtucPerfCurr1DayUasL         AdslPerfCurrDayCount,
             adslAtucPerfPrev1DayFastR        AdslPerfPrevDayCount,
             adslAtucPerfPrev1DayFailedFastR  AdslPerfPrevDayCount,
             adslAtucPerfPrev1DaySesL         AdslPerfPrevDayCount,
             adslAtucPerfPrev1DayUasL         AdslPerfPrevDayCount
         }

         adslAtucPerfStatFastR OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "line retrains"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  the number of fast line bs since last
                  agent reset."
             REFERENCE "ITU G.997.1 Section 7.4.15.1 "
         ::= { adslAtucPerfDataExtEntry 1 }

         adslAtucPerfStatFailedFastR OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "line retrains"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  the number of failed fast line retrains since
                  last agent reset."
             REFERENCE "ITU G.997.1 Section 7.4.15.2 "
         ::= { adslAtucPerfDataExtEntry 2 }

         adslAtucPerfStatSesL OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  the number of severely errored seconds-line since
                  last agent reset."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.7 "
         ::= { adslAtucPerfDataExtEntry 3 }

         adslAtucPerfStatUasL OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  the number of unavailable seconds-line since
                  last agent reset."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.9 "
         ::= { adslAtucPerfDataExtEntry 4 }

         adslAtucPerfCurr15MinFastR OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAtucPerfCurr15MinFastR reports the current
                  number of seconds during which there have been
                  fast retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.1 "
         ::= { adslAtucPerfDataExtEntry 5 }

         adslAtucPerfCurr15MinFailedFastR   OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAtucPerfCurr15MinFailedFastR reports the
                  current number of seconds during which there
                  have been failed fast retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.2 "
         ::= { adslAtucPerfDataExtEntry 6 }

         adslAtucPerfCurr15MinSesL OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAtucPerfCurr15MinSesL reports the current
                  number of seconds during which there have been
                  severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.7 "
         ::= { adslAtucPerfDataExtEntry 7 }

         adslAtucPerfCurr15MinUasL   OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAtucPerfCurr15MinUasL reports the current
                  number of seconds during which there have been
                  unavailable seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.9 "
         ::= { adslAtucPerfDataExtEntry 8 }

         adslAtucPerfCurr1DayFastR    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAtucPerfCurr1DayTimeElapsed [RFC2662],
                  adslAtucPerfCurr1DayFastR reports the number
                  of seconds during which there have been
                  fast retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.1 "
         ::= { adslAtucPerfDataExtEntry 9 }

         adslAtucPerfCurr1DayFailedFastR    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAtucPerfCurr1DayTimeElapsed [RFC2662],
                  adslAtucPerfCurr1DayFailedFastR reports the
                  number of seconds during which there have been
                  failed fast retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.2 "
         ::= { adslAtucPerfDataExtEntry 10 }

         adslAtucPerfCurr1DaySesL    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAtucPerfCurr1DayTimeElapsed [RFC2662],
                  adslAtucPerfCurr1DaySesL reports the
                  number of seconds during which there have been
                  severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.7 "
         ::= { adslAtucPerfDataExtEntry 11 }

         adslAtucPerfCurr1DayUasL    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAtucPerfCurr1DayTimeElapsed [RFC2662],
                  adslAtucPerfCurr1DayUasL reports the
                  number of seconds during which there have been
                  unavailable seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.9 "
         ::= { adslAtucPerfDataExtEntry 12 }

         adslAtucPerfPrev1DayFastR     OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day, adslAtucPerfPrev1DayFastR
                  reports the number of seconds during which there
                  were fast retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.1 "
         ::= { adslAtucPerfDataExtEntry 13 }

         adslAtucPerfPrev1DayFailedFastR OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day,
                  adslAtucPerfPrev1DayFailedFastR reports the number
                  of seconds during which there were failed fast
                  retrains."
             REFERENCE "ITU G.997.1 Section 7.4.15.2 "
         ::= { adslAtucPerfDataExtEntry 14 }

         adslAtucPerfPrev1DaySesL     OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day, adslAtucPerfPrev1DaySesL
                  reports the number of seconds during which there
                  were severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.7 "
         ::= { adslAtucPerfDataExtEntry 15 }

         adslAtucPerfPrev1DayUasL OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day, adslAtucPerfPrev1DayUasL
                  reports the number of seconds during which there
                  were unavailable seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.9 "
         ::= { adslAtucPerfDataExtEntry 16 }

         adslAtucIntervalExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslAtucIntervalExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table provides one row for each ATU-C
                  performance data collection interval for
                  ADSL physical interfaces whose
                  IfEntries' ifType is equal to adsl(94)."
         ::= { adslExtMibObjects 19 }

         adslAtucIntervalExtEntry   OBJECT-TYPE
             SYNTAX          AdslAtucIntervalExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION     "An entry in the
                              adslAtucIntervalExtTable."
             AUGMENTS        { adslAtucIntervalEntry }
         ::= { adslAtucIntervalExtTable 1 }

         AdslAtucIntervalExtEntry ::=
             SEQUENCE {
             adslAtucIntervalFastR            PerfIntervalCount,
             adslAtucIntervalFailedFastR      PerfIntervalCount,
             adslAtucIntervalSesL             PerfIntervalCount,
             adslAtucIntervalUasL             PerfIntervalCount
             }

         adslAtucIntervalFastR OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current interval, adslAtucIntervalFastR
                  reports the current number of seconds during which
                  there have been fast retrains."
         ::= { adslAtucIntervalExtEntry 1 }

         adslAtucIntervalFailedFastR OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the each interval, adslAtucIntervalFailedFastR
                  reports the number of seconds during which
                  there have been failed fast retrains."
         ::= { adslAtucIntervalExtEntry 2 }

         adslAtucIntervalSesL OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the each interval, adslAtucIntervalSesL
                  reports the number of seconds during which
                  there have been severely errored seconds-line."
         ::= { adslAtucIntervalExtEntry 3 }

         adslAtucIntervalUasL OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the each interval, adslAtucIntervalUasL
                  reports the number of seconds during which
                  there have been unavailable seconds-line."
         ::= { adslAtucIntervalExtEntry 4 }

         adslAturPerfDataExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslAturPerfDataExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table contains ADSL physical line counters
                  not defined in the adslAturPerfDataTable
                  from the ADSL-LINE-MIB [RFC2662]."
         ::= { adslExtMibObjects 20 }

         adslAturPerfDataExtEntry   OBJECT-TYPE
             SYNTAX          AdslAturPerfDataExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "An entry extends the adslAturPerfDataEntry defined
                  in [RFC2662].  Each entry corresponds to an ADSL
                  line."
             AUGMENTS { adslAturPerfDataEntry }
         ::= { adslAturPerfDataExtTable 1 }

         AdslAturPerfDataExtEntry ::=
             SEQUENCE {
             adslAturPerfStatSesL             Counter32,
             adslAturPerfStatUasL             Counter32,
             adslAturPerfCurr15MinSesL        PerfCurrentCount,
             adslAturPerfCurr15MinUasL        PerfCurrentCount,
             adslAturPerfCurr1DaySesL         AdslPerfCurrDayCount,
             adslAturPerfCurr1DayUasL         AdslPerfCurrDayCount,
             adslAturPerfPrev1DaySesL         AdslPerfPrevDayCount,
             adslAturPerfPrev1DayUasL         AdslPerfPrevDayCount
         }

         adslAturPerfStatSesL OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  severely errored second-line since the last agent
                  reset."
             REFERENCE "ITU G.997.1 Section 7.2.1.1.7 "
         ::= { adslAturPerfDataExtEntry 1 }

         adslAturPerfStatUasL OBJECT-TYPE
             SYNTAX      Counter32
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "The value of this object reports the count of
                  unavailable seconds-line since the last agent
                  reset."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.9 "
         ::= { adslAturPerfDataExtEntry 2 }

         adslAturPerfCurr15MinSesL OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAturPerfCurr15MinSesL reports the current
                  number of seconds during which there have been
                  severely errored seconds-line."

             REFERENCE "ITU G.997.1 Section 7.2.1.2.7 "
         ::= { adslAturPerfDataExtEntry 3 }

         adslAturPerfCurr15MinUasL   OBJECT-TYPE
             SYNTAX      PerfCurrentCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current 15-minute interval,
                  adslAturPerfCurr15MinUasL reports the current
                  number of seconds during which there have been
                  available seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.9 "
         ::= { adslAturPerfDataExtEntry 4 }

         adslAturPerfCurr1DaySesL    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAturPerfCurr1DayTimeElapsed [RFC2662],
                  adslAturPerfCurr1DaySesL reports the
                  number of seconds during which there have been
                  severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.7 "
         ::= { adslAturPerfDataExtEntry 5 }

         adslAturPerfCurr1DayUasL    OBJECT-TYPE
             SYNTAX      AdslPerfCurrDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the current day as measured by
                  adslAturPerfCurr1DayTimeElapsed [RFC2662],
                  adslAturPerfCurr1DayUasL reports the
                  number of seconds during which there have been
                  unavailable seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.9 "
         ::= { adslAturPerfDataExtEntry 6 }

         adslAturPerfPrev1DaySesL     OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day, adslAturPerfPrev1DaySesL
                  reports the number of seconds during which there
                  were severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.7 "
         ::= { adslAturPerfDataExtEntry 7 }

         adslAturPerfPrev1DayUasL OBJECT-TYPE
             SYNTAX      AdslPerfPrevDayCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the previous day, adslAturPerfPrev1DayUasL
                  reports the number of seconds during which there
                  were severely errored seconds-line."
             REFERENCE "ITU G.997.1 Section 7.2.1.2.9 "
         ::= { adslAturPerfDataExtEntry 8 }

         adslAturIntervalExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslAturIntervalExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table provides one row for each ATU-R
                  performance data collection interval for
                  ADSL physical interfaces whose
                  IfEntries' ifType is equal to adsl(94)."
         ::= { adslExtMibObjects 21 }

         adslAturIntervalExtEntry   OBJECT-TYPE
             SYNTAX          AdslAturIntervalExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION     "An entry in the
                              adslAturIntervalExtTable."
             AUGMENTS        { adslAturIntervalEntry }
         ::= { adslAturIntervalExtTable 1 }

         AdslAturIntervalExtEntry ::=
             SEQUENCE {
             adslAturIntervalSesL             PerfIntervalCount,
             adslAturIntervalUasL             PerfIntervalCount
             }

         adslAturIntervalSesL OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the each interval, adslAturIntervalSesL
                  reports the number of seconds during which
                  there have been severely errored seconds-line."
         ::= { adslAturIntervalExtEntry 1 }

         adslAturIntervalUasL OBJECT-TYPE
             SYNTAX      PerfIntervalCount
             UNITS       "seconds"
             MAX-ACCESS  read-only
             STATUS      current
             DESCRIPTION
                 "For the each interval, adslAturIntervalUasL
                  reports the number of seconds during which
                  there have been unavailable seconds-line."
         ::= { adslAturIntervalExtEntry 2 }

         adslConfProfileExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslConfProfileExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "The adslConfProfileExtTable extends the ADSL line
                  profile configuration information in the
                  adslLineConfProfileTable from the ADSL-LINE-MIB
                  [RFC2662] by adding the ability to configure the
                  ADSL physical line mode."
         ::= { adslExtMibObjects 22 }

         adslConfProfileExtEntry   OBJECT-TYPE
             SYNTAX          AdslConfProfileExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "An entry extends the adslLineConfProfileEntry
                  defined in [RFC2662].  Each entry corresponds to an
                  ADSL line profile."
             AUGMENTS { adslLineConfProfileEntry }
         ::= { adslConfProfileExtTable 1 }

         AdslConfProfileExtEntry ::=
             SEQUENCE {
                 adslConfProfileLineType  INTEGER
             }

         adslConfProfileLineType OBJECT-TYPE
             SYNTAX      INTEGER {
                 noChannel (1),        -- no channels exist
                 fastOnly (2),         -- only fast channel exists
                 interleavedOnly (3),  -- only interleaved channel
                                       -- exist
                 fastOrInterleaved (4),-- either fast or interleaved
                                       -- channels can exist, but
                                       -- only one at any time
                 fastAndInterleaved (5)-- both the fast channel and
                                       -- the interleaved channel
                                       -- exist
                 }
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "This object is used to configure the ADSL physical
                  line mode.  It has following valid values:

                  noChannel(1), when no channels exist.
                  fastOnly(2), when only fast channel exists.
                  interleavedOnly(3), when only interleaved channel
                      exist.
                  fastOrInterleaved(4), when either fast or
                      interleaved channels can exist, but only one
                      at any time.
                  fastAndInterleaved(5), when both the fast channel
                      and the interleaved channel exist.

                  In the case when no value has been set, the default
                  Value is noChannel(1).
                  "
             DEFVAL { fastOnly }
         ::= { adslConfProfileExtEntry 1 }

         adslAlarmConfProfileExtTable   OBJECT-TYPE
             SYNTAX          SEQUENCE OF AdslAlarmConfProfileExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "This table extends the
                  adslLineAlarmConfProfileTable and provides
                  threshold parameters for all the counters defined
                  in this MIB module."
         ::= { adslExtMibObjects 23 }

         adslAlarmConfProfileExtEntry   OBJECT-TYPE
             SYNTAX          AdslAlarmConfProfileExtEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION
                 "An entry extends the adslLineAlarmConfProfileTable
                  defined in [RFC2662].  Each entry corresponds to
                  an ADSL alarm profile."
             AUGMENTS { adslLineAlarmConfProfileEntry }
         ::= { adslAlarmConfProfileExtTable 1 }

         AdslAlarmConfProfileExtEntry ::=
             SEQUENCE {
             adslAtucThreshold15MinFailedFastR     Integer32,
             adslAtucThreshold15MinSesL            Integer32,
             adslAtucThreshold15MinUasL            Integer32,
             adslAturThreshold15MinSesL            Integer32,
             adslAturThreshold15MinUasL            Integer32
         }

         adslAtucThreshold15MinFailedFastR   OBJECT-TYPE
             SYNTAX      Integer32(0..900)
             UNITS       "seconds"
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "The first time the value of the corresponding
                  instance of adslAtucPerfCurr15MinFailedFastR
                  reaches or exceeds this value within a given
                  15-minute performance data collection period,
                  an adslAtucFailedFastRThreshTrap  notification
                  will be generated. The value '0' will disable
                  the notification. The default value of this
                  object is '0'."
             DEFVAL { 0 }
         ::= { adslAlarmConfProfileExtEntry 1 }

         adslAtucThreshold15MinSesL OBJECT-TYPE
             SYNTAX      Integer32(0..900)
             UNITS       "seconds"
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "The first time the value of the corresponding
                  instance of adslAtucPerf15MinSesL reaches or
                  exceeds this value within a given 15-minute
                  performance data collection period, an
                  adslAtucSesLThreshTrap notification will be
                  generated. The value '0' will disable the
                  notification.  The default value of this
                  object is '0'."
             DEFVAL { 0 }

         ::= { adslAlarmConfProfileExtEntry 2 }

         adslAtucThreshold15MinUasL OBJECT-TYPE
             SYNTAX      Integer32(0..900)
             UNITS       "seconds"
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "The first time the value of the corresponding
                  instance of adslAtucPerf15MinUasL reaches or
                  exceeds this value within a given 15-minute
                  performance data collection period, an
                  adslAtucUasLThreshTrap notification will be
                  generated. The value '0' will disable the
                  notification.  The default value of this
                  object is '0'."
             DEFVAL { 0 }
         ::= { adslAlarmConfProfileExtEntry 3 }

         adslAturThreshold15MinSesL OBJECT-TYPE
             SYNTAX      Integer32(0..900)
             UNITS       "seconds"
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "The first time the value of the corresponding
                  instance of adslAturPerf15MinSesL reaches or
                  exceeds this value within a given 15-minute
                  performance data collection period, an
                  adslAturSesLThreshTrap notification will be
                  generated. The value '0' will disable the
                  notification.  The default value of this
                  object is '0'."
             DEFVAL { 0 }
         ::= { adslAlarmConfProfileExtEntry 4 }

         adslAturThreshold15MinUasL OBJECT-TYPE
             SYNTAX      Integer32(0..900)
             UNITS       "seconds"
             MAX-ACCESS  read-create
             STATUS      current
             DESCRIPTION
                 "The first time the value of the corresponding
                  instance of adslAturPerf15MinUasL reaches or
                  exceeds this value within a given 15-minute
                  performance data collection period, an
                  adslAturUasLThreshTrap notification will be
                  generated. The value '0' will disable the
                  notification.  The default value of this
                  object is '0'."
             DEFVAL { 0 }

         ::= { adslAlarmConfProfileExtEntry 5 }

  --   definitions

   adslExtTraps OBJECT IDENTIFIER ::= { adslExtMibObjects 24 }

   adslExtAtucTraps OBJECT IDENTIFIER ::= { adslExtTraps 1 }

   adslExtAtucTrapsPrefix OBJECT IDENTIFIER ::= { adslExtAtucTraps 0 }

         adslAtucFailedFastRThreshTrap      NOTIFICATION-TYPE
             OBJECTS { adslAtucPerfCurr15MinFailedFastR }
             STATUS  current
             DESCRIPTION
                 "Failed Fast Retrains 15-minute threshold reached."
         ::= { adslExtAtucTrapsPrefix 1 }

         adslAtucSesLThreshTrap      NOTIFICATION-TYPE
             OBJECTS { adslAtucPerfCurr15MinSesL }
             STATUS  current
             DESCRIPTION
                 "Severely errored seconds-line 15-minute threshold
                  reached."
         ::= { adslExtAtucTrapsPrefix 2 }

         adslAtucUasLThreshTrap      NOTIFICATION-TYPE
             OBJECTS { adslAtucPerfCurr15MinUasL }
             STATUS  current
             DESCRIPTION
                 "Unavailable seconds-line 15-minute threshold
                  reached."
         ::= { adslExtAtucTrapsPrefix 3 }


   adslExtAturTraps OBJECT IDENTIFIER ::= { adslExtTraps 2 }

   adslExtAturTrapsPrefix OBJECT IDENTIFIER ::= { adslExtAturTraps 0 }

         adslAturSesLThreshTrap      NOTIFICATION-TYPE
             OBJECTS { adslAturPerfCurr15MinSesL }
             STATUS  current
             DESCRIPTION
                 "Severely errored seconds-line 15-minute threshold
                  reached."
         ::= { adslExtAturTrapsPrefix 1 }

         adslAturUasLThreshTrap      NOTIFICATION-TYPE
             OBJECTS { adslAturPerfCurr15MinUasL }
             STATUS  current
             DESCRIPTION
                 "Unavailable seconds-line 15-minute threshold
                  reached."
         ::= { adslExtAturTrapsPrefix 2 }


   -- conformance information

   adslExtConformance OBJECT IDENTIFIER ::= { adslExtMIB 2 }

   adslExtGroups OBJECT IDENTIFIER ::= { adslExtConformance 1 }
   adslExtCompliances OBJECT IDENTIFIER ::= { adslExtConformance 2 }

         -- ATU-C agent compliance statements

         adslExtLineMibAtucCompliance MODULE-COMPLIANCE
             STATUS  current
             DESCRIPTION
                 "The compliance statement for SNMP entities which
                  represent ADSL ATU-C interfaces."

             MODULE  -- this module
             MANDATORY-GROUPS
                {
                adslExtLineGroup,
                adslExtLineConfProfileControlGroup,
                adslExtLineAlarmConfProfileGroup
                }

             GROUP       adslExtAtucPhysPerfCounterGroup
             DESCRIPTION
                 "This group is optional.  Implementations which
                  require continuous ATU-C physical event counters
                  should implement this group."

             GROUP       adslExtAturPhysPerfCounterGroup
             DESCRIPTION
                 "This group is optional.  Implementations which
                  require continuous ATU-R physical event counters
                  should implement this group."
             GROUP   adslExtNotificationsGroup
             DESCRIPTION
           "This group is optional.  Implementations which
                  support TCA (Threshold Crossing Alert) should
                  implement this group."

             OBJECT      adslAtucThreshold15MinFailedFastR
             MIN-ACCESS  read-write
             DESCRIPTION
                 "Read-write access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."

             OBJECT      adslAtucThreshold15MinSesL
             MIN-ACCESS  read-write
             DESCRIPTION
                 "Read-write access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."

             OBJECT      adslAtucThreshold15MinUasL
             MIN-ACCESS  read-write
             DESCRIPTION
                 "Read-write access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."

             OBJECT      adslAturThreshold15MinSesL
             MIN-ACCESS  read-write
             DESCRIPTION
                 "Read-write access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."

             OBJECT      adslAturThreshold15MinUasL
             MIN-ACCESS  read-write
             DESCRIPTION
                 "Read-write access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."

             OBJECT      adslLineConfProfileDualLite
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Read-only access is applicable only when
                  static profiles as defined in ADSL Line MIB
                  [RFC2662] are implemented."
         ::= { adslExtCompliances 1 }

         -- units of conformance
         adslExtLineGroup    OBJECT-GROUP
             OBJECTS {
                 adslLineConfProfileDualLite,
                 adslLineTransAtucCap,
                 adslLineTransAtucConfig,
                 adslLineTransAtucActual,
                 adslLineGlitePowerState
                }
             STATUS     current
             DESCRIPTION
                 "A collection of objects providing extended
                 configuration information about an ADSL Line."
         ::= { adslExtGroups 1 }

         adslExtAtucPhysPerfCounterGroup OBJECT-GROUP
             OBJECTS {
                 adslAtucPerfStatFastR,
                 adslAtucPerfStatFailedFastR,
                 adslAtucPerfCurr15MinFastR,
                 adslAtucPerfCurr15MinFailedFastR,
                 adslAtucPerfCurr1DayFastR,
                 adslAtucPerfCurr1DayFailedFastR,
                 adslAtucPerfPrev1DayFastR,
                 adslAtucPerfPrev1DayFailedFastR,
                 adslAtucPerfStatSesL,
                 adslAtucPerfStatUasL,
                 adslAtucPerfCurr15MinSesL,
                 adslAtucPerfCurr15MinUasL,
                 adslAtucPerfCurr1DaySesL,
                 adslAtucPerfCurr1DayUasL,
                 adslAtucPerfPrev1DaySesL,
                 adslAtucPerfPrev1DayUasL,
                 adslAtucIntervalFastR,
                 adslAtucIntervalFailedFastR,
                 adslAtucIntervalSesL,
                 adslAtucIntervalUasL
                }
             STATUS     current
             DESCRIPTION
                 "A collection of objects providing raw performance
                 counts on an ADSL Line (ATU-C end)."
         ::= { adslExtGroups 2 }

         adslExtAturPhysPerfCounterGroup OBJECT-GROUP
             OBJECTS {
                 adslAturPerfStatSesL,
                 adslAturPerfStatUasL,
                 adslAturPerfCurr15MinSesL,
                 adslAturPerfCurr15MinUasL,
                 adslAturPerfCurr1DaySesL,
                 adslAturPerfCurr1DayUasL,
                 adslAturPerfPrev1DaySesL,
                 adslAturPerfPrev1DayUasL,
                 adslAturIntervalSesL, adslAturIntervalUasL
                }
             STATUS     current
             DESCRIPTION
                 "A collection of objects providing raw performance
                 counts on an ADSL Line (ATU-C end)."
         ::= { adslExtGroups 3 }

         adslExtLineConfProfileControlGroup OBJECT-GROUP
             OBJECTS {
                 adslConfProfileLineType
                }
             STATUS     current
             DESCRIPTION
                 "A collection of objects providing profile
                 control for the ADSL system."
         ::= { adslExtGroups 4 }

         adslExtLineAlarmConfProfileGroup OBJECT-GROUP
             OBJECTS {
                    adslAtucThreshold15MinFailedFastR,
                    adslAtucThreshold15MinSesL,
                    adslAtucThreshold15MinUasL,
                    adslAturThreshold15MinSesL,
                    adslAturThreshold15MinUasL
                }
             STATUS     current
             DESCRIPTION
                 "A collection of objects providing alarm profile
                 control for the ADSL system."
         ::= { adslExtGroups 5 }

         adslExtNotificationsGroup NOTIFICATION-GROUP
             NOTIFICATIONS {
                 adslAtucFailedFastRThreshTrap,
                 adslAtucSesLThreshTrap,
                 adslAtucUasLThreshTrap,
                 adslAturSesLThreshTrap,
                 adslAturUasLThreshTrap
             }
             STATUS        current
             DESCRIPTION
                 "The collection of ADSL extension notifications."
            ::= { adslExtGroups 6 }

END
