-- extracted from rfc4802.txt
-- at Thu Mar  1 06:08:22 2007

   IANA-GMPLS-TC-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, mib-2              FROM SNMPv2-SMI  -- RFC 2578
       TEXTUAL-CONVENTION                  FROM SNMPv2-TC;  -- RFC 2579

   ianaGmpls MODULE-IDENTITY
       LAST-UPDATED
                  "200702270000Z" -- 27 February 2007 00:00:00 GMT
       ORGANIZATION
                  "IANA"
       CONTACT-INFO
                  "Internet Assigned Numbers Authority
                   Postal: 4676 Admiralty Way, Suite 330
                           Marina del Rey, CA 90292
                   Tel:    +1 310 823 9358
                   E-Mail: iana@iana.org"
       DESCRIPTION
         "Copyright (C) The IETF Trust (2007).  The initial version
          of this MIB module was published in RFC 4802.  For full legal
          notices see the RFC itself.  Supplementary information
          may be available on:
          http://www.ietf.org/copyrights/ianamib.html"

          REVISION
           "200702270000Z" -- 27 February 2007 00:00:00 GMT
         DESCRIPTION
           "Initial version issued as part of RFC 4802."
       ::= { mib-2 152 }

   IANAGmplsLSPEncodingTypeTC ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
            "This type is used to represent and control
             the LSP encoding type of an LSP signaled by a GMPLS
             signaling protocol.

             This textual convention is strongly tied to the LSP
             Encoding Types sub-registry of the GMPLS Signaling
             Parameters registry managed by IANA.  Values should be
             assigned by IANA in step with the LSP Encoding Types
             sub-registry and using the same registry management rules.
             However, the actual values used in this textual convention
             are solely within the purview of IANA and do not
             necessarily match the values in the LSP Encoding Types
             sub-registry.

             The definition of this textual convention with the
             addition of newly assigned values is published
             periodically by the IANA, in either the Assigned
             Numbers RFC, or some derivative of it specific to
             Internet Network Management number assignments.  (The
             latest arrangements can be obtained by contacting the
             IANA.)

             Requests for new values should be made to IANA via
             email (iana@iana.org)."
       REFERENCE
            "1. Generalized Multi-Protocol Label Switching (GMPLS)
                Signaling Functional Description, RFC 3471, section
                3.1.1.
             2. Generalized MPLS Signalling Extensions for G.709 Optical
                Transport Networks Control, RFC 4328, section 3.1.1."
       SYNTAX  INTEGER {
                  tunnelLspNotGmpls(0),        -- GMPLS is not in use
                  tunnelLspPacket(1),          -- Packet
                  tunnelLspEthernet(2),        -- Ethernet
                  tunnelLspAnsiEtsiPdh(3),     -- PDH
                  -- the value 4 is deprecated
                  tunnelLspSdhSonet(5),        -- SDH or SONET
                  -- the value 6 is deprecated
                  tunnelLspDigitalWrapper(7),  -- Digital Wrapper
                  tunnelLspLambda(8),          -- Lambda
                  tunnelLspFiber(9),           -- Fiber
                  -- the value 10 is deprecated
                  tunnelLspFiberChannel(11),   -- Fiber Channel
                  tunnelDigitalPath(12),       -- Digital Path
                  tunnelOpticalChannel(13)     -- Optical Channel
                }

   IANAGmplsSwitchingTypeTC ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
            "This type is used to represent and
             control the LSP switching type of an LSP signaled by a
             GMPLS signaling protocol.

             This textual convention is strongly tied to the Switching
             Types sub-registry of the GMPLS Signaling Parameters
             registry managed by IANA.  Values should be assigned by
             IANA in step with the Switching Types sub-registry and
             using the same registry management rules.  However, the
             actual values used in this textual convention are solely
             within the purview of IANA and do not necessarily match
             the values in the Switching Types sub-registry.

             The definition of this textual convention with the
             addition of newly assigned values is published
             periodically by the IANA, in either the Assigned
             Numbers RFC, or some derivative of it specific to
             Internet Network Management number assignments.  (The
             latest arrangements can be obtained by contacting the
             IANA.)

             Requests for new values should be made to IANA via
             email (iana@iana.org)."
       REFERENCE
            "1. Routing Extensions in Support of Generalized
                Multi-Protocol Label Switching, RFC 4202, section 2.4.
             2. Generalized Multi-Protocol Label Switching (GMPLS)
                Signaling Functional Description, RFC 3471, section
                3.1.1."
       SYNTAX  INTEGER {
                  unknown(0),   -- none of the following, or not known
                  psc1(1),      -- Packet-Switch-Capable 1
                  psc2(2),      -- Packet-Switch-Capable 2
                  psc3(3),      -- Packet-Switch-Capable 3
                  psc4(4),      -- Packet-Switch-Capable 4
                  l2sc(51),     -- Layer-2-Switch-Capable
                  tdm(100),     -- Time-Division-Multiplex
                  lsc(150),     -- Lambda-Switch-Capable
                  fsc(200)      -- Fiber-Switch-Capable
                }

   IANAGmplsGeneralizedPidTC ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
            "This data type is used to represent and control the LSP
             Generalized Protocol Identifier (G-PID) of an LSP
             signaled by a GMPLS signaling protocol.

             This textual convention is strongly tied to the Generalized
             PIDs (G-PID) sub-registry of the GMPLS Signaling Parameters
             registry managed by IANA.  Values should be assigned by
             IANA in step with the Generalized PIDs (G-PID) sub-registry
             and using the same registry management rules.  However, the
             actual values used in this textual convention are solely
             within the purview of IANA and do not necessarily match the
             values in the Generalized PIDs (G-PID) sub-registry.

             The definition of this textual convention with the
             addition of newly assigned values is published
             periodically by the IANA, in either the Assigned
             Numbers RFC, or some derivative of it specific to
             Internet Network Management number assignments.  (The
             latest arrangements can be obtained by contacting the
             IANA.)

             Requests for new values should be made to IANA via
             email (iana@iana.org)."
        REFERENCE
            "1. Generalized Multi-Protocol Label Switching (GMPLS)
                Signaling Functional Description, RFC 3471, section
                3.1.1.
             2. Generalized MPLS Signalling Extensions for G.709 Optical
                Transport Networks Control, RFC 4328, section 3.1.3."
        SYNTAX  INTEGER {
                  unknown(0),      -- unknown or none of the following
                  -- the values 1, 2, 3 and 4 are reserved in RFC 3471
                  asynchE4(5),
                  asynchDS3T3(6),
                  asynchE3(7),
                  bitsynchE3(8),
                  bytesynchE3(9),
                  asynchDS2T2(10),
                  bitsynchDS2T2(11),
                  reservedByRFC3471first(12),
                  asynchE1(13),
                  bytesynchE1(14),
                  bytesynch31ByDS0(15),
                  asynchDS1T1(16),
                  bitsynchDS1T1(17),
                  bytesynchDS1T1(18),
                  vc1vc12(19),
                  reservedByRFC3471second(20),
                  reservedByRFC3471third(21),
                  ds1SFAsynch(22),
                  ds1ESFAsynch(23),
                  ds3M23Asynch(24),
                  ds3CBitParityAsynch(25),
                  vtLovc(26),
                  stsSpeHovc(27),
                  posNoScramble16BitCrc(28),
                  posNoScramble32BitCrc(29),
                  posScramble16BitCrc(30),
                  posScramble32BitCrc(31),
                  atm(32),
                  ethernet(33),
                  sdhSonet(34),
                  digitalwrapper(36),
                  lambda(37),
                  ansiEtsiPdh(38),
                  lapsSdh(40),
                  fddi(41),
                  dqdb(42),
                  fiberChannel3(43),
                  hdlc(44),
                  ethernetV2DixOnly(45),
                  ethernet802dot3Only(46),
                  g709ODUj(47),
                  g709OTUk(48),
                  g709CBRorCBRa(49),
                  g709CBRb(50),
                  g709BSOT(51),
                  g709BSNT(52),
                  gfpIPorPPP(53),
                  gfpEthernetMAC(54),
                  gfpEthernetPHY(55),
                  g709ESCON(56),
                  g709FICON(57),
                  g709FiberChannel(58)
                }

   IANAGmplsAdminStatusInformationTC ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
            "This data type determines the setting of the
             Admin Status flags in the Admin Status object or TLV, as
             described in RFC 3471.  Setting this object to a non-zero
             value will result in the inclusion of the Admin Status
             object or TLV on signaling messages.

             This textual convention is strongly tied to the
             Administrative Status Information Flags sub-registry of
             the GMPLS Signaling Parameters registry managed by IANA.
             Values should be assigned by IANA in step with the
             Administrative Status Flags sub-registry and using the
             same registry management rules.  However, the actual
             values used in this textual convention are solely
             within the purview of IANA and do not necessarily match
             the values in the Administrative Status Information
             Flags sub-registry.

             The definition of this textual convention with the
             addition of newly assigned values is published
             periodically by the IANA, in either the Assigned
             Numbers RFC, or some derivative of it specific to
             Internet Network Management number assignments.  (The
             latest arrangements can be obtained by contacting the
             IANA.)

             Requests for new values should be made to IANA via
             email (iana@iana.org)."
        REFERENCE
            "1. Generalized Multi-Protocol Label Switching (GMPLS)
                Signaling Functional Description, RFC 3471, section 8.
             2. Generalized MPLS Signaling - RSVP-TE Extensions,
                RFC 3473, section 7.
             3. GMPLS - Communication of Alarm Information,
                RFC 4783, section 3.2.1."
        SYNTAX BITS {
                  reflect(0), -- Reflect bit (RFC 3471)
                  reserved1(1), -- reserved
                  reserved2(2), -- reserved
                  reserved3(3), -- reserved
                  reserved4(4), -- reserved
                  reserved5(5), -- reserved
                  reserved6(6), -- reserved
                  reserved7(7), -- reserved
                  reserved8(8), -- reserved
                  reserved9(9), -- reserved
                  reserved10(10), -- reserved
                  reserved11(11), -- reserved
                  reserved12(12), -- reserved
                  reserved13(13), -- reserved
                  reserved14(14), -- reserved
                  reserved15(15), -- reserved
                  reserved16(16), -- reserved
                  reserved17(17), -- reserved
                  reserved18(18), -- reserved
                  reserved19(19), -- reserved
                  reserved20(20), -- reserved
                  reserved21(21), -- reserved
                  reserved22(22), -- reserved
                  reserved23(23), -- reserved
                  reserved24(24), -- reserved
                  reserved25(25), -- reserved
                  reserved26(26), -- reserved
                  reserved27(27), -- Inhibit Alarm bit (RFC 4783)
                  reserved28(28), -- reserved
                  testing(29), -- Testing bit (RFC 3473)
                  administrativelyDown(30), -- Admin down (RFC 3473)
                  deleteInProgress(31) -- Delete bit (RFC 3473)
                }
   END

-- 
--    Copyright (C) The IETF Trust (2007).
-- 
--    This document is subject to the rights, licenses and restrictions
--    contained in BCP 78, and except as set forth therein, the authors
--    retain all their rights.
-- 
--    This document and the information contained herein are provided on an
--    "AS IS" basis and THE CONTRIBUTOR, THE ORGANIZATION HE/SHE REPRESENTS
--    OR IS SPONSORED BY (IF ANY), THE INTERNET SOCIETY, THE IETF TRUST AND
--    THE INTERNET ENGINEERING TASK FORCE DISCLAIM ALL WARRANTIES, EXPRESS
--    OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF
--    THE INFORMATION HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED
--    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 
-- Intellectual Property
-- 
--    The IETF takes no position regarding the validity or scope of any
--    Intellectual Property Rights or other rights that might be claimed to
--    pertain to the implementation or use of the technology described in
--    this document or the extent to which any license under such rights
--    might or might not be available; nor does it represent that it has
--    made any independent effort to identify any such rights.  Information
--    on the procedures with respect to rights in RFC documents can be
--    found in BCP 78 and BCP 79.
-- 
--    Copies of IPR disclosures made to the IETF Secretariat and any
--    assurances of licenses to be made available, or the result of an
--    attempt made to obtain a general license or permission for the use of
--    such proprietary rights by implementers or users of this
--    specification can be obtained from the IETF on-line IPR repository at
--    http://www.ietf.org/ipr.
-- 
--    The IETF invites any interested party to bring to its attention any
--    copyrights, patents or patent applications, or other proprietary
--    rights that may cover technology that may be required to implement
--    this standard.  Please address the information to the IETF at
--    ietf-ipr@ietf.org.
-- 

