-- extracted from rfc3595.txt
-- at Fri Sep 12 06:15:26 2003

   IPV6-FLOW-LABEL-MIB DEFINITIONS ::= BEGIN

   IMPORTS

       MODULE-IDENTITY, mib-2, Integer32           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION                          FROM SNMPv2-TC;

   ipv6FlowLabelMIB   MODULE-IDENTITY

       LAST-UPDATED  "200308280000Z"  -- 28 August 2003
       ORGANIZATION  "IETF Operations and Management Area"
       CONTACT-INFO  "Bert Wijnen (Editor)
                      Lucent Technologies
                      Schagen 33
                      3461 GL Linschoten
                      Netherlands
                      Phone: +31 348-407-775
                      EMail: bwijnen@lucent.com

                      Send comments to <mibs@ops.ietf.org>.
                     "
       DESCRIPTION   "This MIB module provides commonly used textual
                      conventions for IPv6 Flow Labels.

                      Copyright (C) The Internet Society (2003).  This
                      version of this MIB module is part of RFC 3595,
                      see the RFC itself for full legal notices.
                     "
       -- Revision History

       REVISION      "200308280000Z"  -- 28 August 2003
       DESCRIPTION   "Initial version, published as RFC 3595."

       ::= { mib-2 103 }

   IPv6FlowLabel      ::= TEXTUAL-CONVENTION
       DISPLAY-HINT  "d"
       STATUS         current
       DESCRIPTION   "The flow identifier or Flow Label in an IPv6
                      packet header that may be used to discriminate
                      traffic flows.
                     "
       REFERENCE     "Internet Protocol, Version 6 (IPv6) specification,
                      section 6.  RFC 2460.
                     "
       SYNTAX         Integer32 (0..1048575)

   IPv6FlowLabelOrAny ::= TEXTUAL-CONVENTION
       DISPLAY-HINT  "d"
       STATUS         current
       DESCRIPTION   "The flow identifier or Flow Label in an IPv6
                      packet header that may be used to discriminate
                      traffic flows.  The value of -1 is used to
                      indicate a wildcard, i.e. any value.
                     "
       SYNTAX         Integer32 (-1 | 0..1048575)

   END

-- 
--    Copyright (C) The Internet Society (2003).  All Rights Reserved.
-- 
--    This document and translations of it may be copied and furnished to
--    others, and derivative works that comment on or otherwise explain it
--    or assist in its implementation may be prepared, copied, published
--    and distributed, in whole or in part, without restriction of any
--    kind, provided that the above copyright notice and this paragraph are
--    included on all such copies and derivative works.  However, this
--    document itself may not be modified in any way, such as by removing
--    the copyright notice or references to the Internet Society or other
--    Internet organizations, except as needed for the purpose of
--    developing Internet standards in which case the procedures for
--    copyrights defined in the Internet Standards process must be
--    followed, or as required to translate it into languages other than
--    English.
-- 
--    The limited permissions granted above are perpetual and will not be
--    revoked by the Internet Society or its successors or assignees.
-- 
--    This document and the information contained herein is provided on an
--    "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING
--    TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING
--    BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION
--    HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF
--    MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 

