-- extracted from rfc2621.txt
-- at Mon Nov 15 17:12:04 1999

RADIUS-ACC-SERVER-MIB DEFINITIONS ::= BEGIN

IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
       Counter32, Integer32,
       IpAddress, TimeTicks, mib-2      FROM SNMPv2-SMI
       SnmpAdminString                  FROM SNMP-FRAMEWORK-MIB
       MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF;

radiusAccServMIB MODULE-IDENTITY
       LAST-UPDATED "9906110000Z" -- 11 Jun 1999
       ORGANIZATION "IETF RADIUS Working Group."
       CONTACT-INFO
          " Bernard Aboba
            Microsoft
            One Microsoft Way
            Redmond, WA  98052
            US

            Phone: +1 425 936 6605
            EMail: bernarda@microsoft.com"
       DESCRIPTION
           "The MIB module for entities implementing the server
            side of the Remote Access Dialin User Service (RADIUS)
            accounting protocol."
       REVISION "9906110000Z"    -- 11 Jun 1999
       DESCRIPTION "Initial version as published in RFC 2621"
       ::= { radiusAccounting 1 }

radiusMIB OBJECT-IDENTITY
       STATUS  current
       DESCRIPTION
           "The OID assigned to RADIUS MIB work by the IANA."
        ::= { mib-2 67 }

radiusAccounting  OBJECT IDENTIFIER ::= {radiusMIB 2}

radiusAccServMIBObjects     OBJECT IDENTIFIER ::=
                                                { radiusAccServMIB 1 }

radiusAccServ      OBJECT IDENTIFIER ::= { radiusAccServMIBObjects 1 }

radiusAccServIdent OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "The implementation identification string for the
              RADIUS accounting server software in use on the
              system, for example; `FNS-2.1'"
       ::= {radiusAccServ 1}

radiusAccServUpTime OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "If the server has a persistent state (e.g., a process),
              this value will be the time elapsed (in hundredths of a
              second) since the server process was started.
              For software without persistent state, this value will
              be zero."
       ::= {radiusAccServ 2}

radiusAccServResetTime OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "If the server has a persistent state (e.g., a process)
              and supports a `reset' operation (e.g., can be told to
              re-read configuration files), this value will be the
              time elapsed (in hundredths of a second) since the
              server was `reset.'  For software that does not
              have persistence or does not support a `reset' operation,
              this value will be zero."
       ::= {radiusAccServ 3}

radiusAccServConfigReset OBJECT-TYPE
       SYNTAX INTEGER { other(1),
                        reset(2),
                        initializing(3),
                        running(4)}
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
              "Status/action object to reinitialize any persistent
               server state.  When set to reset(2), any persistent
               server state (such as a process) is reinitialized as if
               the server had just been started.  This value will
               never be returned by a read operation.  When read, one
               of the following values will be returned:
                   other(1) - server in some unknown state;
                   initializing(3) - server (re)initializing;
                   running(4) - server currently running."
       ::= {radiusAccServ 4}

-- New Stats proposed by Dale E. Reed Jr (daler@iea.com)

radiusAccServTotalRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of packets received on the
              accounting port."
       ::= { radiusAccServ 5 }

radiusAccServTotalInvalidRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Request packets
              received from unknown addresses."
       ::= { radiusAccServ 6 }

radiusAccServTotalDupRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of duplicate RADIUS Accounting-Request
              packets received."
       ::= { radiusAccServ 7 }

radiusAccServTotalResponses OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Response packets sent."
       ::= { radiusAccServ 8 }

radiusAccServTotalMalformedRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of malformed RADIUS Accounting-Request
              packets received. Bad authenticators or unknown
              types are not included as malformed Access-Requests."
       ::= { radiusAccServ 9 }

radiusAccServTotalBadAuthenticators OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS Accounting-Request packets
             which contained invalid Signature attributes."
      ::= { radiusAccServ 10 }

radiusAccServTotalPacketsDropped OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of incoming packets silently discarded
             for a reason other than malformed, bad authenticators,
             or unknown types."
      ::= { radiusAccServ 11 }

radiusAccServTotalNoRecords OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Request packets
              which were received and responded to but not
              recorded."
       ::= { radiusAccServ 12 }

radiusAccServTotalUnknownTypes OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS packets of unknowntype which
             were received."
      ::= { radiusAccServ 13 }

-- End of new

radiusAccClientTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF RadiusAccClientEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "The (conceptual) table listing the RADIUS accounting
              clients with which the server shares a secret."
       ::= { radiusAccServ 14 }

radiusAccClientEntry OBJECT-TYPE
       SYNTAX     RadiusAccClientEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "An entry (conceptual row) representing a RADIUS
              accounting client with which the server shares a secret."
       INDEX      { radiusAccClientIndex }
       ::= { radiusAccClientTable 1 }

RadiusAccClientEntry ::= SEQUENCE {
       radiusAccClientIndex                           Integer32,
       radiusAccClientAddress                         IpAddress,
       radiusAccClientID                        SnmpAdminString,
       radiusAccServPacketsDropped                    Counter32,
       radiusAccServRequests                          Counter32,
       radiusAccServDupRequests                       Counter32,
       radiusAccServResponses                         Counter32,
       radiusAccServBadAuthenticators                 Counter32,
       radiusAccServMalformedRequests                 Counter32,
       radiusAccServNoRecords                         Counter32,
       radiusAccServUnknownTypes                      Counter32
}

radiusAccClientIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "A number uniquely identifying each RADIUS accounting
              client with which this server communicates."
       ::= { radiusAccClientEntry 1 }

radiusAccClientAddress OBJECT-TYPE
       SYNTAX     IpAddress
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The NAS-IP-Address of the RADIUS accounting client
              referred to in this table entry."
       ::= { radiusAccClientEntry 2 }

radiusAccClientID OBJECT-TYPE
       SYNTAX     SnmpAdminString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The NAS-Identifier of the RADIUS accounting client
              referred to in this table entry. This is not necessarily
              the same as sysName in MIB II."
       ::= { radiusAccClientEntry 3 }

-- Server Counters
--
-- Requests - DupRequests - BadAuthenticators - MalformedRequests -
-- UnknownTypes -  PacketsDropped - Responses = Pending
--
-- Requests - DupRequests - BadAuthenticators - MalformedRequests -
-- UnknownTypes - PacketsDropped - NoRecords = entries logged

radiusAccServPacketsDropped OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
           "The number of incoming packets received
            from this client and silently discarded
            for a reason other than malformed, bad
            authenticators, or unknown types."
     ::= { radiusAccClientEntry  4 }

radiusAccServRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of packets received from this
              client on the accounting port."
       ::= { radiusAccClientEntry  5 }

radiusAccServDupRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of duplicate RADIUS Accounting-Request
              packets received from this client."
       ::= { radiusAccClientEntry 6 }

radiusAccServResponses OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Response packets
              sent to this client."
       ::= { radiusAccClientEntry  7 }

radiusAccServBadAuthenticators OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Request packets
              which contained invalid  authenticators received
              from this client."
       ::= { radiusAccClientEntry  8 }

radiusAccServMalformedRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of malformed RADIUS Accounting-Request
              packets which were received from this client.
              Bad authenticators and unknown types
              are not included as malformed Accounting-Requests."
       ::= { radiusAccClientEntry  9 }

radiusAccServNoRecords OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Accounting-Request packets
              which were received and responded to but not
              recorded."
       ::= { radiusAccClientEntry  10 }

radiusAccServUnknownTypes OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS packets of unknown type which
              were received from this client."
       ::= { radiusAccClientEntry  11 }


-- conformance information

radiusAccServMIBConformance
              OBJECT IDENTIFIER ::= { radiusAccServMIB 2 }
radiusAccServMIBCompliances
              OBJECT IDENTIFIER ::= { radiusAccServMIBConformance 1 }
radiusAccServMIBGroups
              OBJECT IDENTIFIER ::= { radiusAccServMIBConformance 2 }

-- compliance statements

radiusAccServMIBCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
             "The compliance statement for accounting servers
              implementing the RADIUS Accounting Server MIB."
       MODULE  -- this module
       MANDATORY-GROUPS { radiusAccServMIBGroup }

       OBJECT        radiusAccServConfigReset
       WRITE-SYNTAX  INTEGER { reset(2) }
       DESCRIPTION  "The only SETable value is 'reset' (2)."

       ::= { radiusAccServMIBCompliances 1 }


-- units of conformance

radiusAccServMIBGroup OBJECT-GROUP
      OBJECTS {radiusAccServIdent,
               radiusAccServUpTime,
               radiusAccServResetTime,
               radiusAccServConfigReset,
               radiusAccServTotalRequests,
               radiusAccServTotalInvalidRequests,
               radiusAccServTotalDupRequests,
               radiusAccServTotalResponses,
               radiusAccServTotalMalformedRequests,
               radiusAccServTotalBadAuthenticators,
               radiusAccServTotalPacketsDropped,
               radiusAccServTotalNoRecords,
               radiusAccServTotalUnknownTypes,
               radiusAccClientAddress,
               radiusAccClientID,
               radiusAccServPacketsDropped,
               radiusAccServRequests,
               radiusAccServDupRequests,
               radiusAccServResponses,
               radiusAccServBadAuthenticators,
               radiusAccServMalformedRequests,
               radiusAccServNoRecords,
               radiusAccServUnknownTypes
              }
      STATUS  current
      DESCRIPTION
            "The collection of objects providing management of
             a RADIUS Accounting Server."
      ::= { radiusAccServMIBGroups 1 }

END

-- 
--    Copyright (C) The Internet Society (1999).  All Rights Reserved.
-- 
--    This document and translations of it may be copied and furnished to
--    others, and derivative works that comment on or otherwise explain it
--    or assist in its implmentation may be prepared, copied, published and
--    distributed, in whole or in part, without restriction of any kind,
--    provided that the above copyright notice and this paragraph are
--    included on all such copies and derivative works.  However, this
--    document itself may not be modified in any way, such as by removing
--    the copyright notice or references to the Internet Society or other
--    Internet organizations, except as needed for the purpose of
--    developing Internet standards in which case the procedures for
--    copyrights defined in the Internet Standards process must be
--    followed, or as required to translate it into languages other than
--    English.
-- 
--    The limited permissions granted above are perpetual and will not be
--    revoked by the Internet Society or its successors or assigns.
-- 
--    This document and the information contained herein is provided on an
--    "AS IS" basis and THE INTERNET SOCIETY AND THE INTERNET ENGINEERING
--    TASK FORCE DISCLAIMS ALL WARRANTIES, EXPRESS OR IMPLIED, INCLUDING
--    BUT NOT LIMITED TO ANY WARRANTY THAT THE USE OF THE INFORMATION
--    HEREIN WILL NOT INFRINGE ANY RIGHTS OR ANY IMPLIED WARRANTIES OF
--    MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.
-- 

